# Connecting to the IxB Software Web User Interface

1. Attach the power source to the tool. The red and green LED indicators, together with the direction LED indicators are flashing, showing that the tool is starting up. Wait until the battery LED, and one of the direction LED indicators are lit. The tool is now ready to operate.

2. Remove the cover of the tool's USB port.

3. Connect the tool to the USB port of the PC. Open a web browser and type in the address of the IxB Software user interface: 169.254.1.1.

Battery LED do not light when PSU is connected.

## Product Essentials Tutorials

https://www.youtube.com/watch?v=ffQHjRwbIgw