# LED Indicators

The LED ring of the tool is equipped with the following indicators:

Position | LED indicator | Main indication
--- | --- | ---
1 | Red status LEDs | Tightening result, NOK
2 | Green status LEDs | Tightening result, OK
3 | Yellow status LEDs | Can be configured in the IxB Software to indicate different events
4 | Blue LED | Can be configured in the IxB Software to indicate different events
5 | Direction LEDs | Tightening direction
6 | - | -
7 | Alarm LED | Error has occurred in the tool
8 | Battery LEDs | Battery charge status
9 | Wireless connection LED | Connection established

To configure the LED indicators, refer to IxB Software User Guide.