# Tightening Program Selection Indication

The indicators in the LED ring can be configured to show the currently selected tightening program in a sequence (1−9). The function must be activated in the IxB Software web user interface.

1. To show the currently selected program in a sequence, turn the reverse ring to the left. The LED of the tightening program is displayed from left to right and top to bottom, as shown below. If the currently selected tightening program has a position in the sequence which is greater than nine, no LED indicator will be lit.

2. Turn the reverse ring to the right and push the tool trigger to run the tightening program. The result is displayed on the LED ring.

3. To show the selected program again, turn the reverse ring to the left.

The result for a loosening will be displayed as normal. If the reverse ring is turned to the right after a completed loosening then the selected tightening program will be shown on the LED ring.