# Fit the Piston to the Lower Load Cell Body

1. Fit the body seal assembly tool to the lower body; ensure the tool is completely pushed down, with no gaps between the tool and the outer chamber wall of the load cell body.

2. Apply a smear of light grease around the chamfer machined into the seal assembly tool.

3. Apply a smear of light grease around the chamfer machined into the piston nose.

4. Offer the piston into the seal assembly Tool; insert it into the housing at one side of the Tool. Make sure the seal assembly tool stays in contact with the load cell.

5. Using a soft mallet tap the opposite edge of the piston into the seal assembly tool.

6. Working around the Piston tap the Piston fully into the Load Cell Body.

7. Remove the seal assembly tool.