# Puller Bar Replacement

When ordering replacement puller bars from either bolting solutions direct or your local Atlas Copco distributor be aware that a puller bar replacement kit consists of both a puller bar and a top reaction nut pre-fitted with a locking screw. See also Puller Bar Assembly for detailed puller bar fitting instructions.

1. Unscrew the endcap (be aware of spring forces inside the cap).

2. Make a note of the number and configuration of the disc springs inside the endcap and remove the disc springs.

3. Remove the small setscrew that holds the reaction nut to the puller bar and unscrew the reaction nut.

4. Withdraw the puller bar from the load cell.

5. Ensure the four retaining screws between spacer and bridge are tightened fully prior to using the tensioner.