# Puller Bar Inspection Procedure

The puller bar in the centre of the aero WTB Tensioner is a highly stressed critical component and it is recommended that the condition of the component be inspected on a regular basis. Look out for:

- Thread damage, both female and male threads.

- Mechanical damage.

- Mechanical wear.

If any damage is noted do not re-use the component, contact Atlas Copco for replacement puller bars.