# Storage Instructions

- Spray the internal threads of the puller bar with a light coating of oil or a rust inhibitor.

- Spray a light coat of oil or rust inhibitor to all plated surfaces for extra corrosion resistance.

- Store the tensioner in an upright position.

- Store the tensioner with the ram retracted

- Store the tensioner in dry conditions.

- Keep the dust cap on the oil inlet nipple when the tensioner is not in use.