# Configuring I/O Signals

For information about configuring I/O signals in IxB, see IxB Software User Guide.

For information about configuring I/O signals in Power Focus 6000, see procedures below.

## Setting a Channel to an Input

1. In the configurations menu in Power Focus 6000, select I/O Expander > Edit. Two lists are displayed, one for Inputs and one for Outputs.

2. To set a channel to an input, select the required channel in the Inputs list. Choose signal typ in the appearing list.

3. Select the same channel in the Outputs list. Select None in the appearing dialog box. Close the appearing list of items without selecting anything.

## Setting a Channel to an Output

1. In the configurations menu in Power Focus 6000, select I/O Expander > Edit. Two lists are displayed, one for Inputs and one for Outputs.

2. To set a channel to an output, select the required channel in the Outputs list. Select None in the appearing dialog box. Select item typ in the appearing list.

3. Select the same channel in the Inputs list. Select None in the appearing list.

After setting the channels, always check that no channel is set to both an input and an output signal at the same time.