# Setting the Controller IP Address

1. In the I/O Hub Settings home menu, select the IP address of the required device in the IP address column. The I/O Hub Web Interface opens.

2. In the Controller section, enter the IP address in the Controller IP field.

3. Select Apply to save settings.

When Apply has been selected, Power Focus 6000 will indicate that the I/O Hub has been disconnected from the controller. The connection will be reestablished automatically.