# Updating the Software

1. Download the Software package to a USB drive.

   The software file must be placed at root level on the USB drive.

2. On the ILT Base Station, remove the lid protecting the USB port and connect the USB drive.

3. On the ILT Base Station Home screen, select System and then select USB.

4. Select Software update and choose the updates you require.

   If the ILT Base Station User Interface Software has been updated, the ILT Base Station will verify the update and then restart.

   To update an ILT Tool Tag, the Tool Tag must be connected to a virtual station.

5. Remove the USB drive and close the lid protecting the USB port.

## Verifying updated Software

- On the ILT Base Station Home screen, select System, then select About, to view the current Software versions.