# Setting Timeouts

The timeout is the delay time, from when a tool leaves, or enters, a defined area until the Disable Tool command is sent to the controller. A small timeout is recommended in order to avoid sending unnecessary Open Protocol commands when a tool is at the edge of an area.

1. From the Home screen, select Configuration, select a Virtual Station, and then select Controller settings.

2. Select Timeouts and then select T/O Dsbl. tool.

3. Enter the timeout, in milliseconds, and select OK to confirm.

It is recommended to use timeout values between 100 and 1000 milliseconds.