# Soft Start

During Soft start it is possible to set the speed, the maximum torque and the the rotation angle to help the screw to enter the thread, and to prevent the tool being jerked out of position when the tool trigger is pressed.

Parameter name | Description | Default value
--- | --- | ---
Soft start | Enables setting of the tool’s speed, angle and maximum torque to facilitate the screw entering the thread. Off: Soft start is turned off. On: Soft start is turned on. | On
Speed | Defines the speed during Soft start. | 35 rpm
Angle | Defines the angle to turn the spindle for the screw to enter the thread. | 90°
Torque max | Defines the upper torque limit during Soft start. If Torque max is exceeded, the tightening is aborted and an error message is given. The tightening will be considered NOK. | 1.25 Nm