# TLS Tag

The Tool Location System (TLS) tag, is a tool accessory. The TLS tag is installed on the tool and connected to the tool accessory bus. The TLS tag is part of the Ubisense positioning system and is handled independently from the controller. In addition to the positioning, the TLS tag can be used to provide information to the operator. Selected output signals can generate different LED light combinations.

Up to 10 different output signals can be mapped to a light priority.

TLS tag configuration parameters
Parameter | Description
--- | ---
Signal | Select a signal to trigger the LED light from a shortcut menu. For a signal of the type Event, select the duration of the signal.
Color | Select a color for the LED.
Priority | 10 priority levels are available for the sounds where one (1) is the highest priority level. Default priority level is five (5).

For two simultaneous signals, the signal with the highest priority wins. When two signals with the same priority triggers the LED, the first arriving signal wins.

An output signal can be of type Event or of type State.

A state signal is active as long as the state is active.

An event signal is active during a configurable time.