# Power Focus 6000 (3.6)

## Software

# Introduction

In this section, you can find the basic information about the product and also the formatting conventions used in the topics.

In this Section

- General Description
- Features
- Benefits
- Conventions
- General Data Protection Regulation (GDPR)
- Liabilities and Warnings
- About the User Guide
- Revision History
- Prerequisites
- System Overview
- License Introduction
- Licenses Overview
- License Sources
- Supported Tools

# General Description

The Power Focus 6000 from Atlas Copco takes productivity, ergonomics, quality and connectivity to entirely new levels. And all this while minimizing environmental impact. The Power Focus 6000 connects a wide range of Atlas Copco assembly tools, giving you a single assembly platform in your station. With Virtual Stations each tool gets its own virtual controller that is easily addressed from overlying systems. The perfect option for your smart connected assembly operation.

# Features

- Connects a wide range of tool types

- Virtual Stations – connect up to 6 tools to one controller

- Web HMI – easy remote connection

- Results, process information and programming on 7” touch screen

- Dedicated factory network port, fieldbus slot, DIO and Open Protocol

- IAM module that carries all controller software

- On demand functionality via the Functionality Management System

- Connectors protected behind lockable front door

# Benefits

- Increased flexibility in rebalancing assembly lines including integration of new tools

- Streamlined communication to overlying interfaces

- Easy installation with fewer cables, hardware components and network drops

- State of the art connectivity through both WiFi and Bluetooth

- Reduced inventory costs

# Conventions

To enhance user understanding, certain formatting conventions are used throughout this document. The formatting conventions used are listed below.

User Guide Conventions
Element | Notation | Description | Output
--- | --- | --- | ---
General emphasis | In the Program workspace. | To make certain text elements stand out, or to highlight. | Text in Bold
Graphical User Interface (GUI) items | Select the Function button. | Any reference to items found on screen in the GUI (for example, command buttons, icon names and field names). | Text in Bold
Graphical User Interface (GUI) Path > | Generally, on the top of the GUI. | Navigation aid which keeps track of the location in the GUI. | For example: Controller > Program > Edit
User input | Enter a Description for the program. | Any text input by the user. | Text in Bold
File names | Enter a File Name for the export. | Files either exported from, or imported into the system. | Text in Bold Italic
Variable and parameter names | Enter a Name for the export. | Variable and parameter names (not values). | Text in Italic
Variable and parameter values | Enter a VALUE for the export. | Variable and parameter values. | Text in BOLD CAPS
System output | Client.Domain.Models.ExportImportConfiguration | Any text output by the system. | Text in Monospace
External links |  | Links to external sites that have information connected to the document or subject content. These could include: Technical Product Data Dimensional Drawings Accessories Product Specific Information | Selectable text to external sites
Internal documentation links |  | Relevant Information - links to information which is directly related to the current topic and needs to be considered for certain configurations that are made. In this Section - links to all the topics within the section, which can be useful when understanding a feature, or configuration. If available, these links will be presented below the text. | Selectable text to internal content

# General Data Protection Regulation (GDPR)

This product offers the possibility to process personal identifiable information such as system user name, role and IP-address. The purpose of this processing capability could be to enhance quality control through traceability and proper access management.

If you decide to process personal data you need to be aware of and comply with relevant personal data protection rules, including, in the EU the GDPR as well as other applicable laws, directives and regulations. Atlas Copco can in no way be held liable for any use made by you of the product.

# Liabilities and Warnings

# Liability

Many events in the operating environment may affect the tightening process and shall require a validation of results. In compliance with applicable standards and/or regulations, we hereby require you to check the installed torque and rotational direction after any event that can influence the tightening result. Examples of such events include but are not limited to:

- initial installation of the tooling system

- change of part batch, bolt, screw batch, tool, software, configuration or environment

- change of air- or electrical connections

- change in line ergonomics, process, quality procedures or practices

- changing of operator

- any other change that influences the result of the tightening process

The check should:

- Ensure that the joint conditions have not changed due to events of influence.

- Be done after initial installation, maintenance or repair of the equipment.

- Occur at least once per shift or at another suitable frequency.

# Warnings

NOTICE

Changing parameters may lead to a decrease in tool performance and may also slow down the production.

WARNING

Risk of Property Damage or Severe Injury

Ensure that you read, understand and follow all instructions before operating the tool. Failure to follow all the instructions may result in electric shock, fire, property damage and/or severe bodily injury.

- Read all Safety Information delivered together with the different parts of the system.

- Read all Product Instructions for installation, operation and maintenance of the different parts of the system.

- Read all locally legislated safety regulations regarding the system and parts thereof.

- Save all Safety Information and instructions for future reference.

# About the User Guide

The User Guide describes how to set up and configure the POWER FOCUS 6000.

It is intended for anyone operating or servicing the POWER FOCUS 6000.

In the Search window on the top menu bar, search for Product Essentials Tutorials for checking the available video tutorials.

Each Product Essentials Tutorial will provide an overview of how to do a specific task with an Atlas Copco product. These tutorials are designed so that users can watch and follow along with their own equipment. The Product Essentials Tutorials are available online to ensure they are always available to users on-demand, and provide baseline knowledge needed to work with Atlas Copco products.

# Revision History

Release Number | Revision Date | Revision Description
--- | --- | ---
3.6 | 06/2021 | UPDATED content: Multistep Programs > Tightening Steps (Wait tightening step) Multistep Programs > Step Restrictions (RH - Rehit, RT - Rescinding Torque) Event Codes list Input Signals - Power Focus 6000 Input Signals - StepSync Output Signals - Power Focus 6000 Output Signals - StepSync Input/Output Signals - StepSync DELETED content: Four step tightening strategy
3.5 | 12/2020 | Added or updated paragraphs: Updated "Multistep Programs > Tightening Steps" paragraph Updated "Multistep Programs > Step Monitors" paragraph Updated "Multistep Programs > Step Restrictions" paragraph Updated "Multistep Programs > Result Reporters" paragraph Updated "Trigger Lost" paragraph Added "Configuring Result Presentation Settings" paragraph Added "Show Final Torque with PrT Compensation: ON / Show PrT Compensation Value on Live Result: ON" paragraph Added "Show Final Torque with PrT Compensation: OFF / Show PrT Compensation Value on Live Result: ON" paragraph Added "Show Final Torque with PrT Compensation: OFF / Show PrT Compensation Value on Live Result: OFF" paragraph Added "Show Final Torque with PrT Compensation: ON / Show PrT Compensation Value on Live Result: OFF" paragraph Updated "StepSync Signals > Input Signals" paragraph Updated "StepSync Signals > Output Signals" paragraph Updated "Configuring the ToolsTalk Connection" paragraph Updated "Configuring the ToolsNet Connection" paragraph Updated "Configuring the PIN" paragraph Updated "Clear Results" paragraph Added "Viewing Protocol Status" paragraph Updated "Stored Results" paragraph Added "Viewing Synchronized Traces" paragraph Updated "Event Codes" paragraph Added "SPC - Statistics Process Control" paragraph Added "Configuring SPC Parameters" paragraph Added "Configuring SPC Variables" paragraph Added "Calculating Statistics" paragraph Added "Viewing Statistics Results" paragraph Updated "Input Signals" paragraph Updated "Output Signals" paragraph Updated "Input/Output Signals" paragraph
3.4 |  | Added or updated paragraphs: Updated "Software" paragraph Updated "Export/Import" paragraph Added "Exporting "All Controller Information"" paragraph Added "Exporting "Settings and Configurations"" paragraph Added "Exporting "Logs from Connected Tools"" paragraph Added "Exporting "Results"" paragraph Added "Importing Controller Configurations and Settings" paragraph Added "Automated Backup" paragraph Added "Supported Tools" paragraph Updated " Tightening Steps" paragraph Updated "Tool Motor Tuning" paragraph Added "Open End Tuning" paragraph Updated "Settings for a Multistep Program" paragraph Added "Trace Setting" paragraph Added "Setting up the Firewall" paragraph Updated "General Virtual Station" paragraph Updated "Configuration of the Direction Switch" paragraph Updated "Event Codes" paragraph Updated "Stored Results" paragraph
3.3 |  | Added or updated paragraphs: Updated "TrueAngle Compensation" paragraph Updated "STwrench" paragraph Updated "Configuration of the PIN Settings" paragraph Added "Running the External Result Tightening Strategy with a Tool Connected" paragraph Added "Running the External Result Tightening Strategy without a Tool Connected" paragraph Updated "Tool Configuration" paragraph Updated "TAG Check" paragraph Updated "TAG Selection" paragraph Added "Input Signals" paragraph Added "Output Signals" paragraph Added "Input/Output Signals" paragraph Updated "Tightening Steps" paragraph Updated "Step Monitors" paragraph Updated "Step Restrictions" paragraph Added "Result Reporters" paragraph Updated "Settings for a Multistep Program" paragraph Added "Result View - Result Reporter" paragraph Updated "Emergency Stop" paragraph
3.1.X |  | Added or updated sections: Updated Fieldbus Configuration settings Updated General Virtual Station - Unlock tool on loosening Updated Event Codes
3.1 |  | Added or updated sections: Updated license management Copying pasting of tightening programs Updated signal Updated third party licenses
3.0 |  | Added or updated sections: License (FMS) chapter StepSync chapter Updated Multistep Apply and Undo button for Tightening and Source Tightening
2.8 |  | Added or updated sections: Calibration using STa6000 or STpad Configurable job counter Decrement on OK Scanner pass-through
2.7 |  | Added or updated sections: Updated multistep steps Source Batch (barcode scanning) Updated Event Codes for SRB and TBP tools
2.6 |  | Added or updated sections Multistep tightening strategy (Editor) WLAN and Bluetooth for wireless tools
2.5 |  | Added or updated sections: Multistep tightening strategy Selector confirm Saved positions General virtual station Wifi socket selector Multiple PINs External OK Service alarms for pulse tools Manual mode virtual station
2.4 |  | Added or updated sections: Settings: License manager Settings: PIN code Settings: Configure start screen Tightening: Disable tightening, Measure angle to, Trigger lost, Torque tuning factor Tool health and battery check Controller health and battery check Pulse strategies 3-step tightening Device: Accessory bus Device: Led ring Device: EHMI Device: Fieldbus diagnostics Export/Import
2.3 |  | Added or updated sections: System settings: network configuration System settings: preferences System settings: protocol configuration System settings: tightening Tightening: Time monitoring and Torque tuning factor ST Wrench Sources Accessory configuration: tool configuration, start condition, and socket selector configuration System administration: Export/Import Tool configuration; ST Wrench Appendix A: Front connections
2.1 |  | Added or updated sections: Settings: Fieldbus Controller menu - Tightening: Current monitoring and True angle compensation Four step tightening System administration: Exported csv file format Virtual station: I/O diagnostics and Fieldbus Appendix A: Emergency stop
2.0 |  | Added or updated sections: Settings: Tool alarms Tool configuration: Tool connection, Tool maintenance, Internal Wlan for wireless tools Tightening setup: Loosening step Tightening results: Live results, Stored results, Status for NOK results Virtual station Event codes in Power Focus 6000
1.6 |  | First official release of the configuration guide for Power Focus 6000.

# Prerequisites

Anyone interested in learning more about POWER FOCUS 6000 can benefit from reading this User Guide.

For a complete understanding of the technical aspects described in the User Guide, we recommend the following:

- Knowledge about tightening techniques

- Experience of working with the previous versions of Power Focus

# System Overview

# Software Structure

# Menu Overview

The controller has several menus available to configure tightening and hardware accessories, perform tool maintenance, administer software, and view reports.

In this Section

- Tightening Tab
- Batch Sequence Tab
- Sources Tab
- Tool Tab
- Virtual Station Tab
- Controller Tab
- Configurations Tab
- Reports Tab
- Settings Tab
- License Assignment Tab
- Help Tab

# Tightening Tab

The Tightening tab lists the Tightening programs stored on the controller that are available for an individual tightening.
Tightening configurations are described in the Tightening tab.

Relevant Information

- Working with the Tightening Tab

# Batch Sequence Tab

The Batch Sequence tab lists the batch sequences stored in the controller.

A Batch Sequence is one or more repetitive tightening programs in various combinations. Batch sequences are created and configured in the Batch sequence tab.

Relevant Information

- Working with the Batch Sequence Tab

# Sources Tab

The Sources tab lists the available options for controlling the selection of a tightening program (for example, a tightening program or a batch sequence, via digital input from different hardware). Scanner configurations are done in the Sources tab.

Relevant Information

- Working with the Sources Tab

# Tool Tab

The Tool tab provides information about the tools connected to the controller.
This menu is also for wireless tools connected to the controller.
Tool reference product, and when the tool was serviced and calibrated are some of the data available in the Tool tab.

Relevant Information

- Working with the Tool Tab

# Virtual Station Tab

The Virtual station tab configures the Virtual Stations.

The Virtual Station is a software abstraction of a controller system.
In the Virtual station tab the different resources, accessories, tools and tasks are assigned to a Virtual Station.

Relevant Information

- Working with the Virtual Station Tab

# Controller Tab

The Controller tab lists hardware and software components.

The software versions stored and used in the controller are listed and can be updated.
The license manager for additional features is handled. It is also possible to import or export settings to and from the controller.

Relevant Information

- Working with the Controller Tab

# Configurations Tab

A list of accessory configurations are given in the Configurations tab.

Accessories like tool accessories, I/O Expander, Internal I/O, Stacklight, Operator Panel, and Socket selectors can be configured.
Digital I/O signals are mapped to buttons, lamps, switches and connectors.

Relevant Information

- Working with the Configurations Tab

# Reports Tab

In the Reports tab the tightening results and events are listed.

Relevant Information

- Results

# Settings Tab

The Settings tab is used to set up the controller specific settings such as language, pin code, wireless network, fieldbus.

Relevant Information

- Working with the Settings Tab

# License Assignment Tab

The License Assignment tab is used to assign licenses and license features to Virtual Stations.

# Help Tab

The Help tab contains useful help sections about the controller.
It is possible to download PDF-files in several languages through a computer connected to the controller.

# Quick Start Guide

To create a better overview of the system, this instruction lightly goes through the different steps required to get started using the system.

This section does not cover every feature of the system, but instead focuses on the most basic features.

1. Decide on what kind of tool to use. The kind of tool being used affect the availability of tightening strategies.

2. The main purpose of the tool is to perform a tightening. This is done by defining a tightening program which contains all relevant parameters of a tightening, for example target angle and target torque.

3. One or several tightening programs can be added to a Batch Sequence which works as a series of tightening programs. A batch sequence can for example be a certain number of tightenings with a tightening program, or a sequence of different tightening programs.

4. Create a Virtual Station and assign a tool to it. The virtual station acts as an interface between the controller and the tool, allowing for several tools to be connected to a single physical controller. A virtual station is required even if only one tool is connected to the controller.

5. Assign a task to the Virtual Station. The task can be either a tightening program, a batch sequence, or a specified digital input (from for example a barcode scanner). The tool assigned to the station will now be able to perform the task.

# Hardware Structure

# Operating and Handling

The POWER FOCUS 6000 is set up and configured by using the controller front panel. It is also possible to access the controller interface through a web GUI by browsing to the controller’s IP address on a connected PC.

Relevant Information

- Accessing the Controller Through a Web GUI

In this Section

- Front Panel
- Web GUI

# Front Panel

The front panel contains a touch-screen display and special buttons.

1 | Display_A color display with touch screen showing configuration views and results.
2 | Special buttons_Special function buttons

In this Section

- Front Panel Buttons
- Touch Screen Buttons
- Navigation

# Front Panel Buttons

These buttons are available as clickable icons in the web GUI.

Button | Name | Description
--- | --- | ---
| Home | Go to the Home screen.
| Result | Go to the live result view.

# Touch Screen Buttons

Button | Name | Description
--- | --- | ---
| Add | Adds an additional item.
| Back | Return to previous view.
| Scroll up / Scroll down | Move in a list that is too long for the screen.
| Maximize / Minimize | Maximize or minimize a section with parameters.
| Back (in a list) | Back (and forward) between pages of a list.
| Close | Tap to close the window.
| Notice | Sign showing that a parameter is configured wrong.
| Home | Go to the Home screen. Only available in the web GUI.
| Go Result | Go to the live results screen. Only available in the web GUI.

# Navigation

- To navigate in the controller GUI either tap on a menu item or move a finger (drag) across the display to scroll through items.

- Options are selected by tapping the required option.

- To enter data into a text box, tap the text box and a keyboard appears on the display.

50305931

# Web GUI

The web GUI is very similar to the controller display. It enables configuration and programming of the controller through a web browser on a computer connected to the controller.

Users can program the controller from the controller and the web interface at the same time.

Relevant Information

- Configuration of the Network

# License Introduction

Licenses for controller features are managed through the Functionality Management System (FMS). This allows customers to tailor controller functions to their specific needs through a dynamic licensing scheme.

Licenses can be obtained for individual features or collections of features and can be deployed across multiple virtual stations. The licenses can be returned to the pool when they are no longer required. Licenses can be obtained through the Atlas Copco License Portal (ACLP). Licenses can be downloaded from the ACLP and managed/distributed through ToolsTalk, or can be stored on a FMS Portable (USB drive) to be inserted into the controller.

Note that the creation and management of a customer account in the ACLP is not covered in this documentation. Contact your local Atlas Copco representative for more information.

# Licenses Overview

Configuration of features governed by licenses can be done even in the absence of an installed license. E.g. configuration of tightening programs and configuration of Multistep programs. Assigning these features to a tool or virtual station is also possible. Running the feature without a valid license, however, will require the installation of the appropriate license.

License enforcement is performed at two stages: assignment and runtime (trigger pressed). If a feature for which no license is installed is assigned to a Virtual Station, a red exclamation mark will appear at the Virtual Station View in ToolsTalk 2. The controller GUI will also show a warning triangle at the tool or task section (depending on what is missing). If a feature for which no license is installed is started (i.e. trigger pressed), an event will be presented to the user informing the user of which license is missing. It will not be possible to proceed without a correct license installed.

Running an unlicensed feature will, in most cases, result in a locked tool.

Many features and functions in the controller require a license in order to be assigned and used by a virtual station. There are three types of licenses:

## Virtual Station Type

Fixed collection of features bundled together in a single package. The Virtual Station Type determines, among other things, what tools can be run, how many programs and sequences can be used, which tightening strategies are available, and the type of reporting that can be done. The features contained in each Virtual Station Type are features that often are used in conjunction with each other, or which have internal dependencies that require the presence of other features in the package. Virtual Station Types are assigned in their entirety to a virtual station. The virtual station can then make use of all features contained in the Virtual Station Type. In order to be able to perform tightenings, a Virtual Station has to be assigned a Virtual Station Type license. Depending on the license type, various tightening options will be enabled or blocked.

## Virtual Station Feature

Individual features which can complement Virtual Station Types. A lot of features can be purchased as a single license.

## Controller Feature

Features that are controller-wide. These are features such as Soft PLC and Step Sync, which are assigned to a controller and once assigned can be used by all virtual stations on that controller.

# License Sources

Licenses used on a controller can be pulled from several different sources. The number of simultaneous sources is limited to 10 (either 10 FMS Portable sources, or one License Server (TT2) in addition to 9 FMS Portable sources). If you would like to add licenses from a source when the source limit (10) has been reached, all licenses from one source need to be removed from the controller to make room for licenses from the other source.

## Source Overview

The Source Overview tab (License assignment > Source Overview) provides the user with an overview of the licenses installed on the controller, as well as where they were installed from. A maximum number of 10 different sources can be displayed here, and each will be designated with FMS P (for FMS Portable, or dongle), or License Server (TT2).

Clicking on any license source will present that source's detailed license source information. It lists the source name and type, as well as the number and type of licenses in each category (Virtual Station Type, Virtual Station Feature and Controller Feature).

# Supported Tools

Tools supported by a Virtual Station may vary depending on the Virtual Station type on the controller.

Supported Tools | BatchControl | JointControl | StationControl | CriticalControl | ProcessControl
--- | --- | --- | --- | --- | ---
BCP / BCV | X | - | - | - | -
TensorSB | - | X | X | - | -
TensorSL | - | - | X | X | X
TBP | - | - | X | X | X
TensorST | - | - | X | X | X
TensorSTR | - | - | X | X | X
SRB | - | - | X | X | X
TensorSTB | - | - | X | X | X
STWrench | - | - | X | X | X
TensorES | - | X | X | - | -
TensorSR | - | - | X | X | X
QST (Fixtured spindle) | - | - | X | X | X
TBPS | - | X | X | - | -
MWR-S (Mechatronic Wrench Signal) | - | - | - | - | -
MWR-T (Mechatronic Wrench Torque) | X | X | X | X | -
MWR-TA (Mechatronic Wrench Torque Angle) | - | - | X | X | X
External tool | X | X | X | X | X

# Installation and Upgrade

In this section, you can find information to help with the initial installation of the product, or upgrading from one version to another.

In this Section

- License Installation

# License Installation

# Installing Licenses on the Controller

Note that licenses sources are limited to 1 License Server (TT2) and 9 FMS Portables (dongles) simultaneously. Licenses are installed either through the server (ToolsTalk 2) or FMS Portable. If the license source limit is reached, all licenses from one source need to be removed from the controller in order to add licenses from another source.

Before installing licenses through the server (ToolsTalk 2), make sure that the controller time is synced with the server time.

## Installing from the Server

Distributing server-based licenses is done through ToolsTalk 2. Please refer to the ToolsTalk 2 User Guide for instructions on installing licenses.

In order to be able to install licenses using ToolsTalk 2, the correct license server needs to be configured:

1. Select the Settings menu, and select the Server connections tab.

2. In the Atlas Copco License Manager field, set the switch to On.

3. Insert the correct Server host IP address (usually the same as the IP address for ToolsTalk 2) and Server Port.

4. Select Apply.

## Installing from FMS Portable (USB)

The Functionality Management System (FMS) uses a special FMS Portable device to transfer functionality to and from a controller. The USB flash drive contains both a general purpose memory area and a trusted storage area that is only accessible by the License manager in a controller. The purchased feature items are downloaded from Atlas Copco to the general purpose area. The first time the FMS Portable is inserted into a controller with a License manager, the file is detected and decoded and the feature items are transferred to the trusted storage area that is only accessible from a License manager.

If you have a USB drive with the licenses installed, perform the following steps to install them on the controller.

1. Insert the USB into the USB port in the controller

   The USB License Management window will pop up in the GUI. The Pool column will show the total license count on the controller from all sources. The Available on FMS P column shows the licenses available on this dongle, while the From this FMS P column shows the number of licenses that have been moved to this controller from this particular FMS P.

2. Select the left-pointing arrow next to license you want to install on the controller.

   The number in the Available on FMS P column will decrease by 1 and the number in the From this FMS P column will increase by 1.

The user will be presented with events on the controller for both license transfer start and end.

## License sync

Existing licenses are checked against the license server every two hours. If no response from the license server is obtained within a 14 day period, the affected licenses will be revoked. The user will also be warned when licenses are about to expire. When a license is within 7 days of expiration, the user will be presented with a warning once every two hours. If licenses are not renewed, they will expire and the affected functions will no longer be available.

Relevant Information

- License Sources
- Removing Licenses from the Controller

# Removing Licenses from the Controller

One way of removing an FMS Portable-installed licenses are described, for instructions how to remove server-installed licenses, please refer to the ToolsTalk 2 User Guide.

## Removing FMS Portable-Installed Licenses

1. Make sure the FMS Portable is inserted into the USB port in the controller.

2. [If the USB License Manager window is not visible] Select the License Assignment menu.

3. Select the USB icon in the top right of the window.

   The USB License Manager window pops up.

4. Select the right-pointing arrow next to the license you want to remove from the controller.

   Licenses that are assigned to virtual stations can be removed from the controller. However, the Virtual Station will become unusable as a result.

Relevant Information

- Unassigning licenses from a Virtual Station

# Configuration

In this section, you can find detailed information about how to create, modify, and verify product settings.

In this Section

- Working with the Tightening Tab
- Working with the Batch Sequence Tab
- Working with the Sources Tab
- Working with the Tool Tab
- Working with the Virtual Station Tab
- Working with the Configurations Tab
- Working with the Controller Tab
- Working with the Settings Tab

# Working with the Tightening Tab

WARNING

Risk of injury

A change in the configuration of the tightening program may cause unexpected torque, rotational direction, or speed in the system(s) where the tightening program is currently in use. This could result in severe bodily injury and/or property damage.

- Check the tightening program configurations after adding a new program or after applying changes to an existing program.

Changes made to tightening programs in any section need to be actively applied by clicking the Apply button in the bottom right corner of the GUI. Alternatively, changes can be undone by clicking the Undo button in the same location.

When navigating away from the section where changes have been made (by using the Back, Home or Result button), the user will be presented with a warning pop-up where the changes can also be applied or undone. The user cannot proceed without applying or undoing changes.

Controller features, such as the Low Reaction Tightening Strategies and controller-wide functions among others, require licenses distributed through the Functionality Management System (FMS). Whereas configuration of features is possible without specific licenses, the assignment and use of those features will require the correct license to be installed on the controller. Please refer to Licenses (FMS) for more detailed information on licenses.

The POWER FOCUS 6000 tightening programs need parameters to be set in order to perform tightening. Selecting a Strategy and either the Target torque or Target angle are mandatory. Other settings are optional, such as Soft start, Selftap, and Torque compensation. It is also possible to monitor the tightening as it progresses by adding limits within which the torque, or angle the nut turns, must remain.

The tightening procedure is divided into four steps: Start, Rundown, Tightening and Stop.

In this Section

- Tightening Programs
- Multistep Programs
- Step Configuration Stages
- Tightening Program Configuration - General Parameters

# Tightening Programs

By selecting the tightening program it is possible to choose the method for applying clamping force (or pre-load) to the joint. Different joints require different strategies for how to apply the desired clamping force and to minimize unwanted in-service effects.

- TurboTight strategy, enables the option to use Manual programming or Quick prog - for more information, see the paragraph TurboTight.

- Quick step, Two step and Three step strategies enable the choice of tightening towards a Target torque or a Target angle value.

- External result strategy, is used when OK tightenings are indicated by an external digital signal - for more information, see the paragraph External result.

All tightening programs require that you at least set the Target torque or Target angle value.

Parameter | Description | Default value
--- | --- | ---
Strategy | Available tightening programs. TurboTight: No additional tightening behavior is used as default. Only target values are used. Quick step: Adds an initial tightening step to reduce pre-load scatter. Two step: Adds a pause between the first and final tightening step to further counteract short-term relaxation effects. Three step: Tightens to a defined First torque value, then loosens the screw and immediately retightens it to Target torque or Target angle. Wrench - production: Tightening strategy to use with an ST Wrench. Wrench - quality: Strategy used for quality test of tightenings with an ST Wrench. Rotate: Rotates the spindle a specified speed and angle. External result: presents a predetermined tightening result instead of measured torque/angle. Multistep: Tightening strategy consisting of multiple configurable steps, with restrictions and monitors. | TurboTight
Target type | Defines the type of the target value in the final step. Target torque: The tightening aims towards the specified target value when performing the final step. Target angle: The tightening aims towards the specified target value when performing the final step. |
Target torque | Defines the target torque of the tightening of the final step. |
Target angle | Defines the target angle of the tightening of the final step. |
Target speed | Activates setting the tool speed for the final step manually or using the default speed. Auto: Uses a value that is calculated based on the Tool max speed. Manual: Specify the tool speed manually. | Auto
<Manual> | Tool speed during tightening or during the final step. |

Relevant Information

- External Result
- Target Torque Limits
- TurboTight

In this Section

- TurboTight
- Quick Step
- Two Step
- Three Step
- STwrench
- Pulsing Tool Strategies
- Rotate
- External Result
- Tightening Program and Error Reporting Validation
- Tightening Program Tool Compatibility Table

# TurboTight

TurboTight is the default tightening strategy and it is designed to perform a very fast and ergonomic tightening based on the maximum speed of the tool (Tool max speed). This strategy has two options:

- Quick prog, that requires only the Target torque to be set to perform the tightening.

- Manual, that allows the user to configure several tightening parameters.

To minimize the risk of unexpected jerk at the end of the tightening when using the TurboTight tightening strategy, make sure to activate Time monitoring.

To minimize the risk of unexpected jerk at the end of the tightening when using the TurboTight tightening strategy, make sure to set the Time Max Limit.

Time Max Limit is enabled by default, but it is necessary to setup the related values. In the tightening stage, set Angle Limit to From Rundown Complete.
Set Time Max as low as possible, without stopping the normal tightening. In the rundown stage, set Rundown Complete Torque so that it is triggered when the torque start to increase.

Depending on the joint properties, for example if the joint is very stiff or very soft, a different tightening strategy than TurboTight might be needed.

TurboTight is not available for Joint Control.

## Fine-Tuning the TurboTight Strategy

TurboTight tightening strategy points to the target torque, and the result can be below or above the target. The most important parameter for TurboTight tightening strategy is the speed. It is possible to keep maximum speed for most tightenings, but if all/some of the tightenings overshoot, decrease the speed in small steps. Rundown Complete Torque is not used for controlling of the tightening; it is only used for calculating of limits and results.

# Quick Step

Quick step is a tightening strategy used to reduce the joint’s preload scatter by adding an initial step with a given torque and speed, and then reducing the target speed in the final step.

Parameter | Description | Default value
--- | --- | ---
First torque | Target torque for the first step. |
First torque | Torque during first step. | 80% of Target Torque
First speed | Target speed for the first step. |
First speed | Tool speed during first step. | 50% of Tool max speed

# Two Step

The Two step strategy is very similar to the Quick step strategy except that it adds a small time delay between the first step and the final step, to further counteract short-term relaxation effects in the joint.

Parameter | Description | Default value
--- | --- | ---
First torque | Torque during first step. | 80% of Target Torque
First speed | Target speed for the first step. |
Pause time | Time between first and second step. | 50 ms

## Fine-Tuning the Two Step Strategy

When the First target is reached, the tool makes an immediate stop for a specified time before it continues with the final step. The First torque value and the Pause time should be chosen to improve ergonomics for hand-held tools.

# Three Step

The Three step strategy adds a loosening step between the first step and the final step, to overcome short-term relaxation effects due to embedment, and reduce preload scatter. This is sometimes used to condition the joint. This can be useful in, for example, joints with many adjoining surfaces and will have a greater effect on new parts than on reused ones, due to the smoothing of surfaces, which reduces embedment.

Conditioning the joint is done by tightening the first step to a given torque, First torque, and then releasing the load by turning the nut a specified Conditioning angle and then retightening the nut to its Target torque or Target angle.

The target torque can be lower than the torque reached during the first step after rundown. In order for the target torque to be lower than the first torque, set target torque (Tightening parameters > Tightening step > Final step > Target torque) to a value lower than First torque (Tightening parameters > Tightening step > First step > First torque).

If Angle is used as a target in the tightening program, the Target angle is measured from the position at the end of the loosening step (conditioning).

## Behavior of Measure torque at, and Measure angle to

The Max torque value and Value at peak torque measured under Result evaluation for Measure torque at and Measure angle to, respectively, represent the highest values measured over the entire tightening. This means that if the Target torque is set lower than the First torque, the Result evaluation value will be higher than the end value. In order to view the tightening's final value, both Measure torque at, and Measure angle to should be set to Value at shutoff.

Parameter | Description | Default value
--- | --- | ---
First torque | Torque during first step. | 80% of Target Torque
First speed | Tool speed during first step. | 50% of Tool max speed
Conditioning speed | Tool speed during the conditioning step. | 50% of Tool max speed
Conditioning angle | Angle to turn the socket during the conditioning step. | 180°

## Fine-Tuning the Three Step Strategy

When the First target is reached and the conditioning step is entered, the tool makes an immediate stop and reverse before it continues with the final step. This conditioning step may need to be fine-tuned to improve ergonomics for hand-held tools.

# STwrench

The STwrench is connected to a controller using a wireless connection and is configured through the controller GUI or the web GUI.

The STwrench is configured under the tightening menu in the same way as the other tightening strategies.

The STwrench has a Rapid Backup Unit (RBU). The RBU defines the wrench function and stores the tightening programs. The controller supports currently only the RBU of the type Production.

The STwrench End-fitting tool (socket) contains a RFID TAG with a programmable number. This wrench uses this number to automatically recognize the tool and which program that can be used. The RFID TAG also stores the torque and angle correction coefficients.

The STwrench has several programs both for production tightening and for quality control.

The STwrench can only support tightening programs supported by the tool (Wrench Production and Wrench Quality).

For more information about the STwrench, see the STwrench User Guide (printed matter number 9836 4134 01).

In this Section

- STwrench Start Step Parameters
- STwrench Rundown Step Parameters
- STwrench Tightening Step Parameters
- STwrench Loosening
- STwrench Stop Step Parameters

# STwrench Start Step Parameters

The parameters shown in the tables are available if one of the STwrench strategies are used. There are several combinations of strategies. Some of the parameters are only available for certain strategies and may not be visible in other strategies.

Parameter rules are automatically checked. If a violation occurs, the error indicator is displayed beside the incorrect parameters. Select the error indicator to display more information about the error.

Switching between strategies can result in the error indicator being shown. This indicates that the chosen combination is invalid, and needs to be corrected.

For more information about the STwrench, see the STwrench User Guide (printed matter number 9836 4134 01).

Parameters in the STwrench start step
Parameter name | Condition | Description | Default value
--- | --- | --- | ---
Tag number |  | On: after enabling TAG Check switch (Configurations > Tool Configuration > TAG Check > On), a correct TAG number is required to run the tightening program. Off: The TAG number is not checked. | Off
Required tag number | Tag number = On | The required TAG number for this tightening program. | 1
Rehit detection |  | The parameter options are: Complete or Off . | Off
Torque correction coefficient |  | In certain cases extensions may be needed to fit the application. In this case the wrench measurement must be compensated to show a correct value. For more information about to calculate the correction coefficient, see the STwrench User Guide (printed matter number 9836 4134 01). The parameter is stored in the RFID TAG in the End-fitting tool. | 1.0
Angle correction |  | In certain cases extensions may be needed to fit the application. In this case the wrench measurement must be compensated to show a correct value. To calculate the correction coefficient, please refer to the STwrench user guide. The parameter is stored in the RFID TAG in the End-fitting tool. | 0°

NOTICE

The correction coefficients alter the STwrench measurement. It may cause an improper reading. Before making any corrections, refer to the latest version of the STwrench User Guide (printed matter number 9836 4134 01).

# STwrench Rundown Step Parameters

The parameters shown in the tables are available if one of the STwrench strategies are used. There are several combinations of strategies. Some of the parameters are only available for certain strategies and may not be visible in other strategies.

Parameter rules are automatically checked. If a violation occurs, the error indicator is displayed beside the incorrect parameters. Select the error indicator to display more information about the error.

Switching between strategies can result in the error indicator being shown. This indicates that the chosen combination is invalid, and needs to be corrected.

For more information about the STwrench, see the STwrench User Guide (printed matter number 9836 4134 01).

Rundown complete is in the STwrench documentation defined as Cycle start , this is when the tightening step begins.

Parameters in the STwrench rundown step
Parameter name | Description | Default value
--- | --- | ---
Rundown complete torque | Definition of the Rundown complete point | Depends on the smarthead minload (usually 5% of nominal torque) in Nm
Ratchet time |  | 5000 ms

# STwrench Tightening Step Parameters

The parameters shown in the tables are available if one of the STwrench strategies are used. There are several combinations of strategies. Some of the parameters are only available for certain strategies and may not be visible in other strategies.

Parameter rules are automatically checked. If a violation occurs, the error indicator is displayed beside the incorrect parameters. Select the error indicator to display more information about the error.

Switching between strategies can result in the error indicator being shown. This indicates that the chosen combination is invalid, and needs to be corrected.

For more information about the STwrench, see the STwrench User Guide (printed matter number 9836 4134 01).

Parameters in the STwrench tightening step
Parameter name | Condition | Description | Default value
--- | --- | --- | ---
Target |  | Select the target from the drop-down menu. The parameter options are: Torque, Angle, Torque or Angle. | Torque
Target Torque |  | Defines the target torque for tightening step. | 0 Nm
Target Angle | Target = Angle | Defines the target angle for tightening step. | 360°
Torque limits | Target = Torque | Selection made by a switch. Auto or Manually position. |
Torque min | Torque limits = Manual | Torque value for the lower limit | 0 Nm
Torque max | Torque limits = Manual | Torque value for the upper limit | 0 Nm
Angle limits | Target = Angle | Selected from a drop-down menu. The parameter options are: Auto or Manually. Angle values for max and min can be or selected |
Angle limits | Target = Torque | Selected from a drop-down menu. The parameter options are: Off: No angle limit monitoring. From rundown complete: The monitoring window is set from when the Rundown complete torque is reached. From torque: The monitoring window is set from when the specific torque value is reached. |
Final angle monitoring torque |  | Torque value from when the angle limits are monitored | 18.75 Nm
Angle min | Angle limits = on or manually | Angle value lower limit | 324°
Angle max | Angle limits = on or manually | Angle value upper limit | 396°
Angle search limit | Angle limits = manually |  |
Measure torque at |  | Selected from a drop-down menu. The parameter options are: Max torque value Value at peak angle |
NOK on final less than target |  | Selection made by a switch. On or Off position. | Off
Change bolt limit |  |  | 50 Nm

Parameters in the STwrench tightening step if the strategy is Wrench - Production, and PVT compensate with snug
Parameter name | Condition | Description | Default value
--- | --- | --- | ---
Torque compensation point | Torque compensation = On |  | 0°
PCT distance | Torque compensation = On |  | 360°
PVT interval | Torque compensation = On |  | 180°
Delay monitoring | Torque compensation = On |  | 0°
Torque min | Torque compensation = On | Torque value for the lower limit | 1 Nm
Torque max | Torque compensation = On | Torque value for the upper limit | 20 Nm
Compensation value | Torque compensation = On | Selected from a drop-down menu. The parameter options are: Average torque Peak torque |

# STwrench Loosening

The parameters shown in the tables are available if one of the STwrench strategies are used. There are several combinations of strategies. Some of the parameters are only available for certain strategies and may not be visible in other strategies.

Parameter rules are automatically checked. If a violation occurs, the error indicator is displayed beside the incorrect parameters. Select the error indicator to display more information about the error.

Switching between strategies can result in the error indicator being shown. This indicates that the chosen combination is invalid, and needs to be corrected.

For more information about the STwrench, see the STwrench User Guide (printed matter number 9836 4134 01).

Parameters in the STwrench loosening step
Parameter name | Condition | Description | Default value
--- | --- | --- | ---
Loosening limit |  | If this parameter is set to a value greater than 0, Power Focus checks if a negative torque exceeding this value is applied during the tightening. In that case, the overall status of the tightening is marked as Not OK. This function is started when the wrench reaches the Cycle Start (before starting the tightening, a loosening is allowed and does not produce results). This function is used to detect unwanted loosening at the end of a tightening (for instance, when the wrench is disengaged from the joint). | 0 Nm

# STwrench Stop Step Parameters

The parameters shown in the tables are available if one of the STwrench strategies are used. There are several combinations of strategies. Some of the parameters are only available for certain strategies and may not be visible in other strategies.

Parameter rules are automatically checked. If a violation occurs, the error indicator is displayed beside the incorrect parameters. Select the error indicator to display more information about the error.

Switching between strategies can result in the error indicator being shown. This indicates that the chosen combination is invalid, and needs to be corrected.

For more information about the STwrench, see the STwrench User Guide (printed matter number 9836 4134 01).

Parameters in the STwrench loosening step
Parameter name | Condition | Description | Default value
--- | --- | --- | ---
End cycle time |  | It is applied when torque goes below the cycle start and gets to the third percentage value set on the STwrench LEDs. | 100 ms

# Pulsing Tool Strategies

The strategy can be selected if the controller software version supports the tightening program. Pulsing tools can achieve a higher torque compared to normal rotating tools.

In this Section

- Pulse Tightening Program
- Pulse Tightening with Direct Driven Electrical Tools
- Tightening using the TensorPulse Program
- Impulse Single Step Tightening Program

# Pulse Tightening Program

## Start

During the start step, the tool rotates in a speed mode without any pulsing.

Parameter name | Description
--- | ---
Soft start | Enables setting of the tool’s speed, angle and maximum torque to facilitate the bolt entering the thread. Selected by radio buttons. Off: Soft start is turned off. On: Soft start is turned on.
Speed | Defines the speed during the soft start.
Time | Defines the Soft start duration.
Angle | Defines the target angle to turn the spindle for the bolt to enter the thread.
Torque max | Defines the upper torque limit during the soft start. If Torque max is exceeded, the tightening is considered NOK.
Rehit detection | Early: Terminates the tightening immediately when an already tightened screw/bolt is detected. The tightening will be considered as NOK. Requires that Soft start is activated. Complete: Even though an already tightened screw/bolt is detected, the tightening is not terminated until all tightening steps have been executed. The tightening will be considered as NOK. To make a rehit detection when Soft start is not activated, the Rehit detection Complete option must be selected. Rehit detection Complete will not terminate the tightening until all tightening steps have been executed. The tightening will be considered a rehit if the speed fails to reach half the rundown speed, a rehit error is then indicated. Off: No rehit detection will be performed. Combination Soft start = Off and Rehit = Early is not allowed.
Positive | The TrueAngle compensation can detect tool rotation and make angle compensations within the set limits.
Negative | The TrueAngle compensation can detect tool rotation and make angle compensations within the set limits.
Use attachment tuning | Attachment tuning is selected by radio buttons.
Gear ratio | Socket rotation speed = Tool speed / gear ratio.
Efficiency tuning | For example 0.9 means 10% efficiency loss.

## Rundown

During rundown, the tool can use either speed mode, with a constant motor speed, or pulse mode. The selection is made depending on the encountered torque and the given torque limits within the configuration.

Parameter name | Description
--- | ---
High-speed rundown | The rundown step can be done in high-speed in order to minimize the time, without overshooting. This is achieved by letting the tool run at a higher speed for a specified angle length. When the angle has been reached, the speed will change to the lower speed specified in Rundown speed parameter. Only available for SRB tools. Length: Default 3600°, max 99999° Speed: Tool max speed must be higher than Rundown speed (rpm).
Rundown speed | Rundown speed can be set to either Max or Manual. If Rundown speed is set to Manual; enter the tool speed in rpm.
Rundown angle limits | Off: Rundown angle limits is turned off. From Trigger: Rundown angle limits is turned On. The system starts to monitor the tightening angle as soon as the tool trigger is pressed and reports if angle limits are violated. From torque: Rundown angle limits is turned On. The system starts to monitor the tightening angle from the specified torque value and reports if angle limits are violated.
Rundown angle monitoring torque | Torque value from where Rundown angle limits are set.
Angle min | Angle value for lower angle limit from starting point.
Angle max | Angle value for upper angle limit from starting point.
Time min | Minimum time for the step.
Time max | Maximum time for the step.
Rundown pulse limits | Selected from a shortcut menu: Off: Rundown pulse limits is turned off. From Trigger: Rundown pulse limits is turned On. The system starts to monitor the pulses as soon as the tool trigger is pressed and reports if the pulse limits are violated. From torque: Rundown pulse limits is turned On. The system starts to monitor the pulses from the specified torque value and reports if the pulse limits are violated.
Rundown pulse monitoring torque | Torque value from where the Rundown pulse limits monitor starts. The value must be set to a value greater than Continuous max torque.
Pulses min | Minimum number of pulses to reach the Rundown complete torque value.
Pulses max | Maximum number of pulses to reach the Rundown complete torque value.
Rundown complete torque | Defines the torque value for when snug is reached and the rundown is completed. The program proceeds with the tightening and starts with pulse mode, if not already done so during rundown.

## Tightening

Parameter name | Description
--- | ---
Target torque | Final target torque for the tightening.
Pulse Energy | The Pulse energy delivered in the action pulse expressed in a percentage of the maximum energy that the tool can deliver in each pulse.
Reaction force tuning factor | The energy delivered by the tool expressed in a percentage value. The reaction force tuning factor is based on the action energy and results in a comfortable reaction.
Residual torque correlation factor | The term Residual torque correlation factor is similar to a calibration and adjusts between the dynamic torque, measured in the electrical tool, and the residual torque, measured by a control tool.
Torque limits | Limits can be Automatically or Manually selected.
Torque min | Minimum torque for the step.
Torque max | Maximum torque for the step.
Angle limits | Off:Angle limits is turned off. From Rundown complete: Angle limits is turned On. The system starts to monitor the tightening angle as soon as Rundown complete is reached and reports if angle limits are violated. From torque: Rundown angle limits is turned On. The system starts to monitor the tightening angle from the specified torque value and reports if angle limits are violated.
Rundown angle monitoring torque | Torque value from where Rundown angle limits monitoring starts.
Angle min | Angle value for lower angle limit from the starting point.
Angle max | Angle value for the upper angle limit from starting point.
Time min | Minimum time for the step.
Time max | Maximum time for the step.
Pulse limits | Off: No pulse limit monitoring. From rundown complete: The monitoring starts when the Rundown complete torque is reached. From torque: The monitoring starts when the specific torque value is reached.
Final pulse monitoring torque | Torque value from when the pulse limits are monitored.
Pulses min | Minimum number of pulses to reach the final target.
Pulses max | Maximum number of pulses to reach the final target.
Premature torque loss detection time | A constant increase in torque is assumed when moving from rundown to tightening. A socket slip off, or a broken screw head can cause the torque to decrease. This may be detected in a monitoring window.

# Pulse Tightening with Direct Driven Electrical Tools

The principle below is applicable for direct driven electrical tools. It is applicable to the Atlas Copco SRB series of tools.

The pulse tightening uses a technique of pulsing the electrical current in the motor and has two distinct features:

- An action current that adds positive torque in the tightening direction.

- A reaction current that creates a comfort reaction by applying a reverse torque.

Pulse tightening principle

A | Action pulse to apply tightening force.
B | Reaction pulse for comfort

The figure shows the general principle of a current pulse tightening strategy. The detailed curve depends on the tool type and the tightening algorithm.

The pulse period consists of two phases as shown in the figure with an action current and a reaction current. Each action pulse adds torque to the tightening until the final target is reached. Each reaction pulse creates a counterforce that provides a comfortable reaction.

The energy level of the action phase and the reaction phase are configurable parameters. The combination of these two parameters creates an efficient tightening combined with operator comfort.

# Tightening using the TensorPulse Program

The principle below is applicable for direct driven electrical tool. It is applicable to the Atlas Copco SRB series of tools.

After each pulse period the resulting torque in the screw is increased. After a series of pulses, the final torque target is reached.

TensorPulse with maximum pulse energy

A | Maximum positive energy in pulse N
B | Maximum positive energy in pulse N+1
C | Increase in energy (torque)

The energy level in the action phase and reaction phase are user configurable parameters. The combination of these two parameters creates an efficient tightening combined with operator comfort. It is possible to set the amount of energy in the two phases as a percentage of the maximum energy that can be delivered in each period:

- Pulse energy; The amount of energy that is applied to each positive pulse as a percentage of the maximum energy that can be applied in the pulse period. The value is between 10-100%.

- Reaction force retention factor; The amount of energy that is applied to each reactive pulse as a percentage of the maximum energy that can be applied in the pulse period. The value is between 0-75%.

TensorPulse with reduced positive pulse energy

A | Reduced positive energy in pulse N
B | Reduced positive energy in pulse N+1
C | Resulting curve for torque build up using maximum pulse energy.
D | Resulting curve for torque build up using reduced pulse energy.

- A small Pulse energy (reduced energy) requires more pulses to reach the target torque as the torque is increased in smaller steps. Smaller steps provides better accuracy to terminate the tightening when the target is reached. Smaller pulses decrease tool movement and increases operator comfort.

- A correctly tuned Reaction force retention factor will create the desired operator comfort. If the factor is too high the operator feels a clockwise rotation of the tool. If the factor is too low, the operator feels a counter clockwise rotation of the tool.

- In an ideal configuration, the reaction energy does not create any loosening force. If the amount of pulses to reach the target value increases, the value is set too high and a small loosening occurs at each pulse.

The optimum values for the Pulse energy and the Reaction force retention factor need to be tuned for optimum performance of the tool and for best operator comfort.

# Impulse Single Step Tightening Program

## Rundown

Parameter name | Condition | Description | Default value
--- | --- | --- | ---
Rundown speed |  | Selected by radio buttons. Rundown speed can be selected between Max or Manual. | Max
Rundown speed | Rundown speed = manual | Specifies the tool speed during the rundown step. |
Rundown time limits |  | Selected from a shortcut menu: Off:Rundown time limits is turned off. From Trigger: Rundown time limits is turned On. The system starts to monitor the time as soon as the tool trigger is pressed and reports if the time limits are violated. From torque: Rundown time limits is turned On. The system starts to monitor the time from the specified torque value and reports if the time limits are violated. | Off
Rundown time monitoring torque | Rundown time limits = from torque | Torque value from where Rundown time limits monitor starts. |
Time min | Rundown time limits = On | Minimum allowed time for rundown. | 10ms
Time max | Rundown time limits = On | Maximum allowed time for rundown. | 5000ms
Rundown pulse limits |  | Selected from a shortcut menu: Off:Rundown pulse limits is turned off. From Trigger: Rundown pulse limits is turned On. The system starts to monitor the pulses as soon as the tool trigger is pressed and reports if the pulse limits are violated. From torque: Rundown pulse limits is turned On. The system starts to monitor the pulses from the specified torque value and reports if the pulse limits are violated. | Off
Rundown pulse monitoring torque | Rundown pulse limits = from torque | Torque value from where the Rundown pulse limits monitor starts. | 2.5Nm
Pulses min | Rundown pulse limits = On | Minimum number of pulses to reach the target. | 2
Pulses max | Rundown pulse limits = On | Maximum number of pulses to reach the target. | 50
Rundown complete torque |  | Defines the torque value for when snug is reached and rundown is completed. | 5Nm

## Tightening

Parameter name | Condition | Description | Default value
--- | --- | --- | ---
Target torque |  | Final target torque for the tightening. |
Pulse Energy |  | The Pulse energy delivered in the action pulse expressed in a percentage of the maximum energy the tool can deliver in each pulse. |
Residual torque correlation factor |  | The term Residual torque correlation factor is similar to a calibration and adjusts between the dynamic torque, measured in the electrical tool, and the residual torque, measured by a control tool. | 100%
Torque limits |  | Selected by radio buttons. Limits can be Automatically or Manually selected |
Torque min | Torque limits = manual | Minimum torque for the step. |
Torque max | Torque limits = manual | Maximum torque for the step. |
Time limits |  | Selected from a shortcut menu: Off:Time limits is turned off. From rundown complete: Time limits is turned On. The system starts to monitor the time as soon as rundown complete is reached and reports if the time limits are violated. From torque: Time limits is turned On. The system starts to monitor the time from the specified torque value and reports if the time limits are violated. | Off
Time monitoring torque | Time limits = from torque | Torque value from where the Time limits monitor starts. |
Time min | Time limits = On | Minimum allowed time for tightening. | 10ms
Time max | Time limits = On | Maximum allowed time for tightening. | 1000ms
Pulse limits |  | Selected from a shortcut menu: Off: No pulse limit monitoring. From rundown complete: The monitoring starts when the Rundown complete torque is reached and reports if the number of pulses is outside the limit. From torque: The monitoring starts when the specific torque value is reached and reports if the number of pulses is outside the limit. | Off
Final pulse monitoring torque | Pulse limits = from torque | Torque value from when the pulse limits are monitored. |
Pulses min | Pulse limits = on | Minimum number of pulses to reach the final target. | 2
Pulses max | Pulse limits = on | Maximum number of pulses to reach the final target. | 50
Premature torque loss detection time |  | A constant increase in torque is assumed when moving from rundown to tightening. A socket slip of, or a broken screw head can cause the torque decrease. This may be detected in a monitoring window. | 200 ms

# Rotate

The Rotate strategy is primarily a strategy for testing and demonstration purposes. When the tool is allowed to rotate freely, it turns the socket the specified angle using the lowest torque possible.

Parameter | Description | Default value
--- | --- | ---
Target speed | Target speed for the Rotate strategy. |
<Target speed> | Manual tool speed during the Rotate strategy. | 16.5% of Tool max speed
Target angle | Angle to turn the spindle. | 360°

# External Result

External result is a strategy used when an OK tightening is indicated by an external digital signal (and not by torque or angle values measured during tightening).

When the signal is sent, the Result view will show the value of the Target parameter provided in the tightening program (specified torque value, angle value, or text string). These (torque and angle) values do not represent actual measured values, but only inserted text.

Parameter | Description | Default value
--- | --- | ---
Torque <Target torque> | Numerical value for desired displayed target torque value | 0.00
Angle <Target angle> | Numerical value for desired displayed target angle value | 360°
Text | Alphanumerical string for desired displayed text. |

In this Section

- Running the External Result Tightening Strategy with a Tool Connected
- Running the External Result Tightening Strategy without a Tool Connected

# Running the External Result Tightening Strategy with a Tool Connected

1. On the Home view, select the Tightening Tab. Then, create a tightening program with External Result strategy.

2. Return to the Home view and select the Virtual Station Tab.

   In the Licenses window, the External Result Tightening Strategy with a Tool Connected feature requires a license to be assigned and used by a virtual station.

3. In the Tool window, select the necessary tool. Then, select the tool configuration.

4. In the Task window, select the tightening program with an External Result strategy.

5. Send EXTERNAL_OK signal to the Virtual Station.

6. Select Go Result button to display the results.
   Results are sent from the Tool configuration for the tool connected to the Virtual Station.

Relevant Information

- Assigning Licenses to a Virtual Station
- Connecting a Tool to a Virtual Station

# Running the External Result Tightening Strategy without a Tool Connected

1. On the Home view, select the Tightening Tab. Then, create a tightening program with External Result strategy.

2. Return to the Home view and select the Settings Tab. Then, select External Tool.

3. Select the Plus icon at the upper-right corner of the GUI to create an external tool.

   It is possible to create up to 10 External Tools configurations.

4. In the External Tool window, enter the model, the serial number and the description of the external tool.

   Serial Number is a mandatory text box.
   The serial number can be used to provide an identifier for the necessary tool, for example the manufacturer serial number. The maximum number of characters for the Serial Number text box is 32.

   Once the switch at the upper-right corner of the External Tool window is set to On, return to the Home view and select the Tool Tab. The added external tool appears in the list of the available tools.

5. Return to the Home view and select the Virtual Station Tab.

   In the Licenses window, the External Result Tightening Strategy without a Tool Connected feature requires a license to be assigned and used by a virtual station.

6. In the Tool window, select the necessary external tool. Then, select the tool configuration.

7. In the Task window, select the tightening program with an External Result strategy.

8. Send EXTERNAL_OK signal to the Virtual Station.

9. Select Go Result button to display the results (serial numbers).
   Serial numbers are sent from the External Tool configuration for the tool connected to the Virtual Station.

Relevant Information

- Assigning Licenses to a Virtual Station
- Connecting a Tool to a Virtual Station

# Tightening Program and Error Reporting Validation

The tightening program automatically validates with the parameter rules and tool properties as soon as new values are entered or changes are made. If the validation detects any errors they are reported with an error description.

In this Section

- Validation Error Reporting
- Validate a Tool with a Tightening Program

# Validation Error Reporting

If the validation gives an error, it is displayed with an icon next to the parameter or parameters causing the error. When you tap on the icon, a short description of the error is given.

Example (See image):

1. Target torque is set to 25 Nm with Final torque limits set to Torque min 23.75 Nm and Torque max 24.5 Nm (this value is hidden by the pop-up window in the image).

2. When you tap on the validation error icon next to the Torque max parameter, a short description of the error is given, saying that Target torque is greater than Torque max (Torque max <= Target torque).

3. To fix the error, adjust the Torque max value so that it is greater than Target torque, and the error icon will disappear.

# Validate a Tool with a Tightening Program

1. In the Tightening menu, choose Tightening program library or Multistep program library. If required, select a specific program in the list. Note that validation can be performed both for the entire list of programs, or for individual programs.

2. Select the tool icon in the upper right corner.

3. In the pop-up window, choose the tool to validate the tightening program against, and click Validate.

   If a tightening program is not compatible with the selected tool, it will be indicated by a red circle with an exclamation point.

# Tightening Program Tool Compatibility Table

The availability of tightening strategies depends on the licenses installed on the controller.

Tightening Strategies | ES | ST | STR | SR | SB+ | ETT | SL (low voltage) | QST | STB | SRB 2.0 ETP-SRB31-20 | SRB 2.1 ETP-SRB31-25 | SRB-HA | TBP / TBP-S | STW | External tool
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
Two step | X | X | X | X | X | X | X | X | X | X | - | X | - | - | -
Quick step | X | X | X | X | X | X | X | X | X | X | X | X | - | - | -
Three step | X | X | X | X | X | X | X | X | X | X | - | X | - | - | -
Turbo Tight | X | - | X | X* | - | X | - | - | - | X | X | - | - | - | -
Rotate | X | X | X | X | X | X | X | X | X | X | - | X | - | - | -
External Result | X | X | X | X | X | X | X | X | X | X | X | X | X | - | X
Tensor Pulse | - | - | - | - | - | - | - | - | - | X | X | - | - | - | -
Impulse - single step | - | - | - | - | - | - | - | - | - | - | - | - | X | - | -
Wrench production | - | - | - | - | - | - | - | - | - | - | - | - | - | X | -
Wrench quality | - | - | - | - | - | - | - | - | - | - | - | - | - | X | -

* Available only for SR31.

Tightening Features | ES | ST | STR | SR | SB+ | ETT | SL (low voltage) | QST | STB | SRB 2.0 ETP-SRB31-20 | SRB 2.1 ETP-SRB31-25 | TBP / TBP-S | STW | External tool
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
True Angle | - | - | X | - | - | X | - | - | - | - | - | - | - | -

# Multistep Programs

WARNING

Risk of injury

A change in the configuration of the tightening program may cause unexpected torque, rotational direction, or speed in the system(s) where the tightening program is currently in use. This could result in severe bodily injury and/or property damage.

- Check the tightening program configurations after adding a new program or after applying changes to an existing program.

Controller features, such as the Low Reaction Tightening Strategies and controller-wide functions among others, require licenses distributed through the Functionality Management System (FMS). Whereas configuration of features is possible without specific licenses, the assignment and use of those features will require the correct license to be installed on the controller. Please refer to Licenses (FMS) for more detailed information on licenses.

A multistep tightening is a tightening done in several steps. The number of steps and the type of steps vary depending on the tightening to be done. A multistep tightening program is highly configurable, including monitoring function and restrictions.

The multistep tightening strategy has not been implemented for STB tools.

## Product Essentials Tutorials

https://www.youtube.com/watch?v=x1PbTNkwzuE

In this Section

- Multistep GUI Interface
- Tightening Steps
- Step Monitors
- Step Restrictions
- Result Reporters
- Adding a Multistep Program
- Deleting a Multistep Program
- Settings for a Multistep Program
- Creating a Multistep Program
- Multistep Program Tool Compatibility Table
- STB Tools and Multistep

# Multistep GUI Interface

While multistep tightening programs can be selected from the controller screen, editing programs can only be done in the web GUI.

The interface for mutistep programs can be divided into three main areas.

On top there is a drop-down menu containing the Properties of the multistep tightening program. Here general properties such as program name, overal program monitor and validation can be filled out.

To the right there are three tabs containing the steps, monitors and restrictions that can be used to build the multistep program. To use any of the items, click on the appropriate tab, and drag the item in the list to the tightening area. Depending on its funtion, either drop the item between the beginning and the end of the program (for steps), or on top of a particular step (for monitors and restrictions).

The main area of the interface is made up of the tightening area. This is the area that includes all the steps in the tightening program.

At bottom left of the screen there are zoom buttons (+ and -), as well as a Delete button. Use the zoom buttons to zoom in and out on the tightening area.

# Tightening Steps

This section lists the tightening steps that are valid for the Power Focus 6000 and Power Focus 6000 StepSync Controllers.

## General Parameters

## Name

It is possible to rename each step, if needed.

## Rotational direction

Each of the tightening steps can run either forward, that is to make a tightening, or reverse, to loosen the screw slightly. The arrows indicate this direction. Many of the tightening steps have a direction hard-coded to forward, for example Tighten to Angle, or Tighten to Torque. Steps such as Loosen to Angle or Loosen to Torque have their direction automatically set to reverse.

The reverse setting is not allowed for tools configured with Gear Front Attachment (GFA) of type open end. The tightening direction of the tightening program must be the same as the tightening direction of the open end tool for a tightening to be allowed to be run. It is possible to assign a loosening program to a tightening program for an open end tool, but if the direction switch is set to run the loosening program, the tool will be locked.

## Step category

For each step, it is possible to choose a step category. By selecting step category, the NOK tightenings will be listed in the event result view with related detailed status together with the corresponding multistep error information. If no selection is made, the detailed status will be set to "uncategorized multistep error". The related detailed status can be customized.

## Angle window

A joint is considered Hard if the screw is tightened to its full torque, and it rotates 30 degrees (or less) after it has been tightened to its snug point. A Soft joint rotates 720 degrees or more, after it has been tightened to its snug point. The hardness parameter defines the Angle Window for the gradient calculation. The harder the joint - the smaller the angle window.

## Speed Ramp / Acceleration (only available in ToolsTalk 2)

For most of the steps, it is possible to specify how the acceleration to the target speed should be achieved. Three different settings are possible; Hard, Soft and Manual. The acceleration defined will be used whenever a step is started. Regardless whether the tool is already running with speed at the beginning of the step, the ramp will be used to accelerate to the target speed of the step. This process is the case even if the speed at the start of the step is higher, or lower than the target speed.

Speed ramp - Hard and Soft mode:

Acceleration | Speed ramp used
--- | ---
Hard | 2000 rpm/s (Speed Ramp between 1000 and 10000 rpm/s is a Hard acceleration)
Soft | 500 rpm/s (Speed Ramp between 200 and 1000 rpm/s is a Soft acceleration)

Speed ramp - Manual mode:

Parameter | Default value | Minimum limit | Maximum limit
--- | --- | --- | ---
Speed | 60 rpm | Must be > 0 | Must be <= Tool Max Speed
Acceleration | 500 rpm/s | Must be > 0 | Must be <= Tool Max Acceleration

## Using speed shifts

You can define 1-5 angle triggers or torque triggers during a step, where the speed will shift.

The speed shifts can be added in the Configuration field.

Within one step, all the speed shift triggers are based on the same property (either torque or angle). They cannot be mixed within one step.

To add a speed shift:

1. In the dialog box of a step that can have speed shifts, select Add speed shift. Then, select an angle range or a torque range.
   The Speed Shift Angle/Torque fields open.

2. Add values according to the table below:

   Parameter | Description
   --- | ---
   Angle/Torque trigger | Must be > 0
   Speed | Must be >0
   Speed ramp type | Hard or soft

The Torque triggers and Angle triggers must be less than the step target, depending on the type of the step and the trigger type.

The Torque trigger and Torque speed also validate against the Max torque and Max speed of the tool.
A warning or error indicator occurs whenever the Speed Shift settings exceed either the tool max values or step max values.

## Controlling braking behavior (Ergo stop/Inertia)

The braking behavior of a Multistep tightening program can be controlled at two possible locations in the program: in a step preceding a reversal of direction of the tightening, and/or at the final step of the tightening program. At other locations in the Multistep program, the braking parameters will not be available in the step's general settings. Braking can be set to either Ergo stop or Inertia. Inertia will brake the tool completely, while Ergo stop will allow for a more ergonomic slowing down of the tightening.

To set the type of braking, go into the settings for the step, and set the Brake configuration dropdown to Ergo stop or Inertia. Inertia has no additional parameters.

## Ergo stop parameters

Parameter | Description
--- | ---
Adaptive brake | Set the Adaptive Brake to On or Off
Ramp time | Only available when Adaptive Brake is set to Off. Insert time in ms.

## List of individual steps

The following tightening steps are not supported for tools configured with Gear Front Attachment (GFA) of type open end:

- A - Loosen to Angle

- TrR - Loosen to Trigger Release

- T - Loosen to Torque

- E - Engage

- SR - Socket Release

- DT - Tighten to DynaTork

- TP - TensorPulse

## C - Clutch

This step will run the tool with the programmed Speed in forward direction until the Clutch has been released. When the tool has reported the release of the Clutch the step will finish with OK status.

A tightening program using the Clutch step cannot have any other step assigned.

This step is only valid for the Clutch tools BCV-RE and BCP-RE.

Parameter | Description
--- | ---
Speed Control | One Speed or Two Speed
Final Speed | Sets the final speed of the program [rpm]
Speed Ramp | Switch where speed ramp can be chosen [Hard, Soft]
Rehit | Rehit detection set to On or Off
Rehit angle | Sets the rehit angle [°]

## CL - Clutch Loosening

This step will run the tool with the programmed speed in reverse direction until the tool trigger is released.

A loosening program using the Clutch step can't have any other step assigned.

This step is only valid for the Clutch tools BCV-RE and BCP-RE.

Parameter | Description
--- | ---
Final | Sets the speed of the program [rpm]

## W – Wait

In this step the tool waits until the Wait Type condition is fulfilled. The tool does not rotate while waiting, but Hold condition can be specified.

Parameter | Description
--- | ---
Wait Type | Time: Wait specified time. Signal (valid only for Power Focus 6000 StepSync): Wait until a rising edge on the signal Continue Step is received.
Wait Time | Number of seconds the tool will stand still - valid only when Time is selected for Wait Type.
Hold Condition | No hold: The tool is waiting without running. Hold torque: While waiting the tool strives to hold the torque it had when entering the step. Hold position: While waiting the tool strives to hold the position it had when entering the step.

## SR - Socket Release

This step runs the tool with speed n in the backward direction until the target angle is reached. The target angle is measured from the start of the step.

This step is only allowed to use as the last step in the tightening path of a multistep tightening program. However, it is possible to add a sync point after this step.

Parameter | Description
--- | ---
Target angle | The angle target. Default: 3 degrees, must be > 0
Speed ramp type | Hard, soft, or manual. Default: Hard. If you select Manual, the Speed ramp field opens.
Speed ramp | If Speed ramp type is Manual, this field opens. Default: 500 rpm/s.
Speed | Default: 60 rpm.

## DI – Run Until Digital Input

This steps runs the tool, in the direction defined by parameter Direction, until the input specified by Digital Input goes high or low depending on the value of Stop Condition.

This step is not available for STB tools.

Parameter | Description
--- | ---
Direction | Forward, or Backward
Digital Input | One of the following local digital inputs on the controller can be selected: Local DI 1 Local DI 2 Local DI 3 Local DI 4
Brake (Valid only for Flex and Power Focus 6000 StepSync). | If On the tool will be stopped when the target is reached. If Off the program goes directly to the next step without stopping the tool.
Stop Condition | Falling edge: The steps runs until a falling edge is detected after step start. Rising edge: The steps runs until a rising edge is detected after step start. Any edge: The step runs until a falling or a rising edge is detected after step start. Low: The step runs until low value is detected. High: The step runs until high value is detected.
Speed (rpm) | Default: 60 rpm.
Speed ramp type | Hard, soft, or manual. Default: Hard. If you select Manual, the Speed ramp field opens.
Speed ramp | Available if Speed ramp type is Manual. Default: 500 rpm/s.

## A – Tighten to Angle / Loosen to Angle

A – Tighten to Angle

This step runs the tool until the target angle is reached. The target angle is measured from the start of the step.

A – Loosen to Angle

This step runs the tool with the speed n in the backward direction until the angle target is reached. The target angle is measured from the start of the step.

Parameters

Parameter | Description
--- | ---
Target angle | The angle target. Must be > 0.
Speed | Default: 60 rpm.
Speed ramp type | Hard, soft, or manual. Default: Hard. If you select Manual, the Speed ramp field opens.
Speed ramp | If Speed ramp type is Manual, this field opens. Default: 500 rpm/s.
Brake (Valid only for Flex and Power Focus 6000 StepSync). | If On the tool will be stopped when the target is reached. If Off the program goes directly to the next step without stopping the tool.

## TrR – Loosen to Trigger Release

This step is valid only for the Power Focus 6000 controller.

This step runs in the backward direction until the tool trigger is released (loosen). It can only be used as a last step in a program.

For STB tools, this step is only applicable for loosening programs.

Parameter | Description
--- | ---
Speed | Numerical value for rotation speed; in rpm.
Speed Ramp Type | List of options where speed ramp can be chosen [Hard, Soft, Manual]

## TTTR – Tighten to Trigger Release

This step runs until the tool trigger is released (tighten). It can only be used as a last step in a tightening program.

Parameter | Description
--- | ---
Speed | Numerical value for rotation speed; in rpm.
Speed Ramp Type | List of options where speed ramp can be chosen [Hard, Soft, Manual]

## Tighten to yield, method 2 (YM2)

This step is valid only for Power Focus 6000 StepSync.

This step runs the tool with the specified speed in the forward direction until the yield point is detected.

Search for the yield point starts when the torque has reached Tt. The average of the torque over Af degrees is calculated. This procedure is repeated N rs times.

A reference slope is calculated with linear regression over the N rs points. After that, new average values are continuously calculated over A f degrees.

The actual slope is calculated with linear regression over the last N s average points. The yield point is reached when the slope is less than Py % of the reference slope.

Parameter | Description
--- | ---
Target torque | Must be > 0.
Filter angle | Default: 1. Must be > 0.
Number of samples | Default: 6. Must be >=4.
Number pf samples, reference | Default: 6. Must be >=4.
Yield point percentage | Default: 90%. Must be >20%.
Speed | Default: 60 rpm. Must be > 0.
Speed ramp type | Hard, soft, or manual. Default: Hard. If you select Manual, the Speed ramp field opens.
Speed ramp | If Speed ramp type is Manual, this field opens. Default: 500 rpm/s.
Brake (Valid only for Flex and Power Focus 6000 StepSync). | If On the tool will be stopped when the target is reached. If Off the program goes directly to the next step without stopping the tool.

## T - Tighten to Torque / Loosen to Torque

T – Tighten to Torque

This step runs the tool with the programmed speed in forward direction until the target torque is reached.

Parameter | Description
--- | ---
Target torque | The torque target. Must be > 0.
Speed ramp type | Hard, soft, or manual. Default: Hard. If you select Manual, the Speed ramp field opens.
Speed | Default: 60 rpm. Must be > 0.
Speed ramp | If Speed ramp type is Manual, this field opens. Default: 500 rpm/s.
Brake (Valid only for Flex and Power Focus 6000 StepSync). | If On the tool will be stopped when the target is reached. If Off the program goes directly to the next step without stopping the tool.

T – Loosen to Torque

This step runs the tool with the speed in the backward direction. For the step to be active, the torque must first exceed 110 % of the Target torque. The Target torque should be set to a positive value. After reaching the target torque, the step runs until the torque drops below the target torque.

Parameter | Description
--- | ---
Target torque | The torque target. Must be > 0.
Speed ramp type | Hard, soft, or manual. Default: Hard. If you select Manual, the Speed ramp field opens.
Speed | Default: 60 rpm. Must be > 0.
Speed ramp | If Speed ramp type is Manual, this field opens. Default: 500 rpm/s.
Brake (Valid only for Flex and Power Focus 6000 StepSync). | If On the tool will be stopped when the target is reached. If Off the program goes directly to the next step without stopping the tool.

## T+A – Tighten to Torque Plus Angle

This step runs the tool until the target torque is reached. From this point it continues to run an additional target angle.

Parameter | Description
--- | ---
Target torque | The torque target. Must be > 0.
Target angle | The angle target. Must be > 0.
Speed ramp type | Hard, soft, or manual. Default: Hard. If you select Manual, the Speed ramp field opens.
Speed ramp | If Speed ramp type is Manual, this field opens. Default: 500 rpm/s.
Speed | Default: 60 rpm.
Brake (Valid only for Flex and Power Focus 6000 StepSync). | If On the tool will be stopped when the target is reached. If Off the program goes directly to the next step without stopping the tool.

## T|A – Tighten to Torque or Angle

This step runs the tool with the speed n in the forward direction until the first of either torque target or angle target is reached. The torque and angle measurements start at the beginning of the step.

Parameter | Description
--- | ---
Target torque | Must be > 0.
Target angle | Must be > 0.
Speed | Default: 60 rpm. Must be > 0.
Speed ramp type | Hard, soft, or manual. Default: Hard. If you select Manual, the Speed ramp field opens.
Speed ramp | If Speed ramp type is Manual, this field opens. Default: 500 rpm/s.
Brake (Valid only for Flex and Power Focus 6000 StepSync). | If On the tool will be stopped when the target is reached. If Off the program goes directly to the next step without stopping the tool.

## T&A – Tighten to Torque and Angle

The tool runs until with the specified speed in the forward direction until both target torque and target angle are reached. The target torque and the target angle must be set to > 0.

Parameter | Description
--- | ---
Target torque | Must be > 0.
Target angle | Default: 0. Must be > 0.
Speed | Default: 60 rpm. Must be > 0.
Speed ramp type | Hard, soft, or manual. Default: Hard. If you select Manual, the Speed ramp field opens.
Brake (Valid only for Flex and Power Focus 6000 StepSync). | If On the tool will be stopped when the target is reached. If Off the program goes directly to the next step without stopping the tool.

## DT – Tighten to DynaTork

This step runs the tool with speed n in the forward direction until the Target torque is reached. The tool will then hold the current constant at the DynaTork Percentage of Target torque during the DynaTork time.

To avoid overheating of the tool, it is strongly recommended to never run DynaTork to more than 40% of the maximum torque of the tool.

Parameter | Description
--- | ---
Target torque | The torque target. Must be > 0.
DynaTork Time | The time DynaTork will be active.
DynaTork Percentage | The percentage of Torque target.
Speed ramp type | Hard, soft, or manual. Default: Hard. If you select Manual, the Speed ramp field opens.
Speed ramp | If Speed ramp type is Manual, this field opens. Default: 500 rpm/s.
Speed (rpm) | Default: 60 rpm.
Brake (Valid only for Flex and Power Focus 6000 StepSync). | If On the tool will be stopped when the target is reached. If Off the program goes directly to the next step without stopping the tool.

## Y – Tighten to Yield

This step is not available for STB tools.

This strategy runs the tool with the speed in the forward direction until the yield point is detected. The yield point is found by monitoring the torque gradient from the point where the torque goes above the Trigger Torque level, calculated based on Torque and Angle distance measurements. The Angle distance parameter is set according to the specified hardness of the joint.

Set the Gradient angle window (for hard joint, for soft joint or for manually setting of the Angle window). If Manual is selected, the Angle Window must be set. A joint is considered Hard if the screw is tightened to its full torque and it rotates 30 degrees or less after it has been tightened to its snug point. A Soft joint rotates 720 degrees or more after it has been tightened to its snug point. The hardness parameter defines the Angle Window for the gradient calculation. The harder the joint - the smaller the angle window.

Parameter | Description
--- | ---
Gradient Angle Window | Specifies Angle Window: For Hard Joint: Angle Window = 1 deg. For Soft Joint: Angle Window = 20 deg. Manual: Manually set Angle Window.
Angle Window | Available when Gradient Angle Window is set to Manual. Must be > 0 and <= 100.
Trigger Torque | The angle measurement starts at this trigger. Must be >= 0 and < Tool MaxTorque.
Damping | Frequency in which the gradient is being calculated. Must be > 0 and < 100 and < Angle window.
Yield Point Percentage | Must be >= 20 %
Speed | Default: 60 rpm. Must be > 0.
Speed ramp type | Hard, soft, or manual. Default: Hard. If you select Manual, the Speed ramp field opens.
Torque Filter Type | The type of the filter: None: No filtering of the torque is used. The raw values are used as-is in the gradient calculation. Five-point: The torque value used in the calculation are filtered using a sliding average filter over 5 torque samples. Low pass: The torque values is filtered with a simple discrete Infinite Impulse Response filter. Sliding Average: The torque values used in the calculation are filtered using a sliding average filter over a Number of Samples specified by the use.
Cut-off Frequency | Needs to be specified when Torque Filter Type is set to Low pass: 20 Hz 40 Hz 90 Hz 200 Hz 600 Hz
Number of Samples | Needs to be specified when Torque Filter Type is set to Sliding Average: 2 4 6 8 16 32
Brake (Valid only for Flex and Power Focus 6000 StepSync). | If On the tool will be stopped when the target is reached. If Off the program goes directly to the next step without stopping the tool.

## ThCT – Thread Cutting to Torque

The Thread Cutting to Torque function enables tightening where the Rundown torque required is greater than the Rundown complete torque, for example when tightening thin layers of metal using self-threading (or self-tapping) screws. The tool runs in forward direction until the Thread Cutting Angle (Aw) is reached. The thread cutting angle window is measured from when the torque passes Thread Cut Trigger Torque (Ttc) for the first time. From the point where Thread cutting angle is reached, the step continues to run until the Target Torque (Tt) is reached.

Parameter | Description
--- | ---
Target torque | Must be > 0.
Thread Cutting Angle Window | Default: 0. Must be > 0.
Trigger Torque | The angle measurement starts at this trigger.
Speed | Default: 60 rpm. Must be > 0.
Speed ramp type | Hard, soft, or manual. Default: Hard. If you select Manual, the Speed ramp field opens.
Brake (Valid only for Flex and Power Focus 6000 StepSync). | If On the tool will be stopped when the target is reached. If Off the program goes directly to the next step without stopping the tool.

## RD – Rundown

This step is not available for STB tools.

Rundown step is the part of the tightening from when the screw enters the thread until just before the screw head touches the underlying surface and snug point is reached. The torque required during rundown does not contribute to any clamping force.

This step runs the tool with the speed in the forward direction, and depending on the Rundown Type, Torque or Snug the step behavior is as follows:

Rundown Type: To Torque: The step stops when the specified target torque is found.

Rundown Type: To Snug: The snug gradient calculation starts at the specified torque trigger level Tt. If no torque trigger is set the gradient calculation is started at the start of the step.

The slope calculation is made between two angle points Ad degrees apart and is calculated as: (Tn – Tn-1) / (An – An-1) and as soon as two slopes after each other are larger than TSLOPE the snug point is found.

Parameter | Description
--- | ---
Rundown type | To Torque or To Snug.
Target torque | Default: "not set". Must be > 0.
Speed | Default: 60 rpm. Must be > 0.
Speed ramp type | Hard, soft, or manual. Default: Hard. If you select Manual, the Speed ramp field opens.
Speed ramp | If Speed ramp type is Manual, this field opens. Default: 500 rpm/s.
Trigger Torque | If Rundown type is To Snug, the Trigger torque field is displayed. Default: "not set". Must be > 0.
Delta Angle | If Rundown type is To Snug, the Delta angle field is displayed. Default: "0". Must be > 0.
Torque Rate | If Rundown type is To Snug, the Torque rate field is displayed. Default: "0". Must be > 0.
Brake (Valid only for Flex and Power Focus 6000 StepSync). | If On the tool will be stopped when the target is reached. If Off the program goes directly to the next step without stopping the tool.

## E - Engage

This step is not available for STB tools.

This step runs the tool in both directions until the socket engages the screw. The step continues until Target torque or Target angle is reached, provided that Continue if not Engaged is set to Yes. If Target Angle is reached in any direction, the direction is reversed. Limit the search iterations by entering Max Engage Attempts. If Target Torque is reached in any direction the step will finish with OK status.

## Ext - External Result

External result is a strategy used when an OK tightening is indicated by an external digital signal (and not by torque or angle values measured during tightening). This external signal can be provided through any means that can provide a digital signal into the Power Focus 6000 (e.g through the I/O bus).

When the signal is sent, the result view (logged data) will show the value of the Target parameter provided in the tightening program (specified torque value, angle value, or text string). These (torque and angle) values do not represent actual measured values, but only inserted text.

Parameter | Description
--- | ---
Torque <Target torque> | Numerical value for desired displayed target torque value. A signal could for example come from a Click Wrench and display <Target torque>.
Angle <Target angle> | Numerical value for desired displayed target angle value. A signal could for example come from a Click Wrench and display <Target angle>.
Text | Alphanumerical string for desired displayed text. For example: "Oil has been changed".

## MWR - Mechatronic Wrench

Mechatronic Wrench is a specialized step that can be used only in conjunction with the Mechatronic Wrench (MWR).

This step cannot be used in combination with other steps. No restrictions can be used with this step. By default, the step has three monitors: Peak Torque, Angle, and Click.

Parameter | Description
--- | ---
Loosening limit | Numerical value for negative torque (i.e. torque in the loosening direction) at which point the tightening result is marked as NOK (False direction of tightening (loosen)); in Nm.
Tool Size | Numerical value for the specific length of the end fitting tool installed on the MWR-TA; in mm.
Tool Bend | Numerical value for the end fitting tool installed on the MWR-TA; in °/Nm.
Rehit Angle Window | Numerical value for the angle for determining if the screw was already tightened if the torque is reached; in °.
Max Angular Rate | Numerical value for the max rate at which the screw can be tightened; in °/s.

## WP - Wrench Production

Strategy used for the quality test of the tightening performed with the STwrench.

Parameter | Description
--- | ---
Control Strategy | The Wrench Production step type can be configured with the following control strategies. Torque: This strategy guides the operator is reaching the desired target torque. Angle: This strategy guides the operator is reaching the desired target angle. Torque or Angle: This strategy guides the operator is reaching the desired target angle or desired target torque. Torque and Angle: This strategy guides the operator in tightening a bolt until both target torque and angle have been reached. Yield Point: With this strategy, the STwrench detects the yield point automatically. The torque limits specify the range in which the result is OK. Target angle specifies how far beyond the yield point the user may tighten. Loose: This strategy is used to loosen a tightened screw. PVT compensate with snug: This strategy guides the operator in reaching the desired target torque for joints with prevailing torque, when the prevailing torque level is higher than the final target.

Based on the control strategy selected, a combination of some of the parameters listed below will be displayed.

Parameters | Description
--- | ---
Target Torque | Defines the target torque for tightening step.
Measure torque at | Specifies where the torque will be measured. Choose between Peak torque or Peak angle. Peak torque: The torque value will be set to the peak torque value. Peak Angle : The torque value will be set to the torque measured at the peak angle.
Angle search limit | This is an offset that is used to the set the torque result value for a tightening. Measure torque at must be set to Peak Angle for this parameter to be available.
Ratchet time | Numerical value for ratchet time which is by default 5000 ms. This allows the operator to release the torque for a while and recharge during the tightening operation. If the Ratchet time is exceeded the result of the tightening is marked as NOK with the reason "Tightening timeout".
End cycle time | Numerical value in ms to indicate the end cycle time. Applied when torque goes below the rundown complete
Torque correction coefficient | The parameter is used to correct the torque reading when using an extension or torque multiplier on the wrench. Default value is 1.
Angle correction | The parameter is used to correct the angle reading when using an extension or torque multiplier on the wrench. Default value is 0.
Target Angle | Defines the target angle for tightening step.
Rehit detection | On or Off. Rehit detection can be used to determine when a tightening is a rehit based on the angle limit setting. Angle limit for rehit is enabled if Rehit direction is set to On.
Linear slope coefficient | Linear slope coefficient characterizes the joint stiffness in the linear part of the curve, as torque/angle slope in the Nm/Deg measurement unit.
Compensate value | Choose between Average torque and Peak torque. The Compensate value specifies how the PVT will be calculated. Average torque - The PVT will be based on an average calculated using the following: Delay monitoring PVT interval PVT distance Prevailing torque min Prevailing torque max Peak torque - The PVT will be based on the peak value measured before snug was detected.
Delay monitoring | PVT calculation will not start before this window has been passed, starts at tightening start.
PVT interval | Sets how many degrees the PVT window shall be calculated for, start from the PVT distance point.
PVT distance | Sets when the system shall start the PVT window (how many degrees prior to snug).
Prevailing torque min | Prevailing torque minimum limit.
Prevailing torque max | Prevailing torque maximum limit

## WQ - Wrench Quality

Strategy used for quality test of tightenings with the STwrench.

Parameter | Description
--- | ---
Control Strategy | The Wrench Quality strategy can be configured with the following control strategies. Residual Torque/Time: This strategy analyzes the torque trace as a function of time. The operator shall execute this operation with a single, steady, movement. The wrench automatically recognizes the breakaway and residual point. Residual Torque/Angle: This strategy evaluates the residual torque on a joint, looking for the residual point of the Torque/Angle trace. Residual Torque/Peak: This strategy evaluates the residual torque on a joint as the peak torque necessary to rotate the bolt further. Loose and Retighten: This strategy loosens a bolt and retightens it back to its original position Yield Point: With this strategy the wrench detects the yield point automatically. Target Angle specifies how far beyond the yield point the user may tighten.

Based on the control strategy selected, a combination of some of the parameters listed below will be displayed.

Parameters | Description
--- | ---
Ratchet time | Numerical value for ratchet time which is by default 5000 ms. This allows the operator to release the torque for a while and recharge during the tightening operation. If the Ratchet time is exceeded the result of the tightening is marked as NOK with the reason "Tightening timeout".
Torque correction coefficient | The parameter is used to correct the torque reading when using an extension or torque multiplier on the wrench. Default value is 1.
Angle correction | The parameter is used to correct the angle reading when using an extension or torque multiplier on the wrench. Default value is 0.
Target Angle | Defines the target angle for tightening step.
Rehit detection | On or Off. Rehit detection can be used to determine when a tightening is a rehit based on the angle limit setting. Angle limit for rehit is enabled if Rehit direction is set to On.
Linear slope coefficient | Linear slope coefficient characterizes the joint stiffness in the linear part of the curve, as torque/angle slope in the Nm/Deg measurement unit.

## TP - TensorPulse

Before using TensorPulse tightening step, it is mandatory that the following license type is installed on the controller:

- Low Reaction Strategies

TensorPulse is valid only for the following tools: ETV-STR61-100-13, ETV-STR61-70-13, ETV-STR61-50-10.

This step generates tightening pulses in the forward direction, until the torque target is reached.

If running TensorPulse tightening step, use the necessary PulseDrive socket/adapter.
If TensorPulse tightening step runs without the PulseDrive socket/adapter, all the tightenings are NOK. The step error “PulseDrive socket/adapter not detected” shows for no PulseDrive socket/adapter.

Parameter | Description
--- | ---
Torque Target - Ts | Torque Target must range from 0 through the maximum torque of the tool.
Pulse Energy - Pe | Pulse Energy is used to control the amount of energy/current in each pulse. Pulse Energy must range from 10% through 100 %. By default, it is set to 100%.
Retention Force Tuning Factor | Retention Force Tuning Factor is used to tune the reaction force when running TensorPulse step. It is the power that moves the tool in the opposite direction after each pulse. High tuning factor makes high reaction force and high pulse frequency; low tuning factor makes low reaction force and low pulse frequency. Retention Force Tuning Factor must range from 0 through 100 %. By default, it is set to 40%.

In the trace, the angle reversal means that the tool rotates backward to enable pulsing, but the bolt head does not necessarily rotate backward because of the PulseDrive socket/adapter.

Relevant Information

- Continue Step - 10128

In this Section

- Trace Setting

# Trace Setting

When the trace configuration is enabled on the program level, the trace resolution can be configured on step level. The setting for Trace Setting defines how the sampling should be done on each specific step.

With this trace recording the sample rates are not the same in all the steps, instead the sample rate depends on the configuration in each step. This means the trace is divided into one trace for each step.

Parameter | Description
--- | ---
Trace Setting | Program: Use the settings as defined on program level. Manual: The trace sample type from the program level will be used, that is, Time or Angle. Using a different sample rate will override the setting on the program level.
Sample Time | Choose the sample time from the drop-down list (0.25 - 1000 ms).
Sample Angle | Choose the sample angle from the drop-down list (0.25 - 20 degree).

The maximum number of samples in a trace is 4096. If a tightening produces more than 4096 samples a down-sampling process will take place. A down-sampling process is removing every second trace sample from the whole tightening and continuing recording with half the resolution. This process is repeated every time the 4096 sample limit is reached. Since the down-sampling process is done for all steps, the relation between the steps is the same.

Trace channel | Note
--- | ---
Torque | Available for all tools equipped with a torque transducer.
Angle | Available for all tools.
Speed | Available for all tools.
Torque Second | Only available for tools with two torque transducers.
Angle Second | Only available for tools with two angle transducers.
Current | Available for all tools.
Gradient | Available if some step/restriction/monitor produces the gradient values.

Relevant Information

- Settings for a Multistep Program

# Step Monitors

The step monitors are used to verify that the tightening was achieved according to the specification, for example, angle limits or torque. Each step has mandatory step monitors and optional step monitors. The mandatory monitors are included when dragging a new step to the multistep program. The optional monitors are flexible and can be placed as needed in the multistep program. Every step can have up to eight monitors each.

The following monitors are automatically added to every step that is added to the multistep tightening program.

Default step monitors
Step Monitor | Applicable steps
--- | ---
Angle | All
Peak Torque | All

## A – Angle

This step monitor measures the maximum angle reached during the monitor and checks that it is between High limit and Low limit. The angle measurement starts at the start of the monitor or, if specified, at the point where the torque passes Trigger torque for the first time during the monitor.

Parameter | Description
--- | ---
Type | Four angle types are available: Peak angle (default), Angle at peak torque, Shut off angle, and Angle at end.
Trigger torque | The angle measurement starts at this trigger.
Low Limit | Lowest acceptable angle.
High Limit | Highest acceptable angle.

## YA – Angle from Yield

This monitor measures the peak angle reached from the yield point and checks that the peak angle is within the limit.

This step monitor is not available for the STB tools.

Parameter | Description
--- | ---
Gradient Angle Window | Specifies Angle Window: For Hard Joint: Angle Window = 1 deg. For Soft Joint: Angle Window = 20 deg. Manual: Manually set Angle Window.
Angle Window | Available when Gradient Angle Window is set to Manual. Must be > 0 and <= 100.
Yield Point Percentage | Must be >= 20 %
Trigger Torque | The angle measurement starts at this trigger. Must be > 0 and < Tool MaxTorque.
Damping | Frequency in which the gradient is being calculated. Must be > 0 and < 100 and < Angle window.
Low Limit | Lowest acceptable angle. Must be >= 0
High Limit | Highest acceptable angle. Must be > 0
Torque Filter Type | The type of the filter: None: No filtering of the torque is used. The raw values are used as-is in the gradient calculation. Five-point: The torque value used in the calculation are filtered using a sliding average filter over 5 torque samples. Low pass: The torque values is filtered with a simple discrete Infinite Impulse Response filter. Sliding Average: The torque values used in the calculation are filtered using a sliding average filter over a Number of Samples specified by the use.
Cut-off Frequency | Needs to be specified when Torque Filter Type is set to Low pass: 20 Hz 40 Hz 90 Hz 200 Hz 600 Hz
Number of Samples | Needs to be specified when Torque Filter Type is set to Sliding Average: 2 4 6 8 16 32

## MT – Mean Torque

This monitor measures the average torque during the monitor and checks the calculated value is within the limits.

This step monitor is not available for the STB tools.

Parameter | Description
--- | ---
Type | Specifies start condition: Step Start: The measurement starts from step start and ends at the shut-off point. Torque Trigger: The measurement starts at the point where the torque passes Torque Trigger for the first time. It ends at the shut-off point. Angle Trigger: The measurement starts at the point where the angle is Angle Trigger, measured from the optional Trigger Torque, is reached. Without Trigger Torque, the Angle Trigger is measured from the start of the step. It ends at the shut-off point Angle Window: Measures during an Angle Window. The window starts at the point where the torque passes Trigger Torque for the first time plus an angle offset, Angle Trigger. Time Interval: Measures during the last Time Interval seconds of the tightening.
Torque Trigger | Available when Type is set to Trigger Torque, Angle Trigger or Angle Window. Must be >= 0 and < Tool Max Torque.
Angle Trigger | Available when Type is set to Angle Trigger or Angle Window. Must be > 0.
Angle Window | Available when Type is set to Angle Window. Must be > 0.
Time Interval | Available when Type is set to Time Interval. Must be > 0.
Low Limit | Lowest acceptable torque.
High Limit | Highest acceptable torque.

## PT – Peak Torque

This step monitor measures the maximum torque reached during the monitor, including any over shoot, and checks that it is between High limit and Low limit.

Parameter | Description
--- | ---
Low Limit | Lowest acceptable torque.
High Limit | Highest acceptable torque.

## PTCA – Post Thread Cut Angle

Measures the angle achieved during the monitoring and checks that it is between the specified angle limits. The Trigger Torque level is ignored until the end of the Thread cut angle window is reached. After that, the angle measuring starts as soon as the measured torque is above Trigger Torque. The parameter Stop Condition specifies where the angle measurement should end.

Parameter | Description
--- | ---
Trigger torque | Must be >= 0
Thread cutting angle window | Must be > 0
Angle measurement type | Peak angle Angle at peak torque Shut off angle Angle at end
Thread cut trigger torque | Must be >= 0
Low Limit | Must be >= 0
High Limit | Must be > 0 Must be > Low limit

## PTCPT – Post Thread Cut Peak Torque

Measures the maximum torque achieved during the monitoring, including any over-shoot, and checks that it is between the Torque limits. All torque values are ignored until the end of the Thread cut angle window has been reached.

Parameter | Description
--- | ---
Thread cut trigger torque | Must be >= 0
Thread cutting angle window | Must be > 0
Low Limit | Must be >= 0
High Limit | Must be > 0 Must be > Low limit

## PVTH – Post View Torque High

This monitor checks that all torque values in the Angle Window Length are below the High limit.

The Angle Window starts at the angle degrees set in Start Angle in reverse direction from the shut-off point. This then spans for the angle degrees set in Angle Window Length in reverse direction. If Start Angle is left blank, the Angle Window starts at the shut-off point. The torque values used in the monitor are based on the mean torque value, calculated over Number of Samples. If the total angle of the step is less than Start Angle plus Angle Window Length the monitor will report NOK.

Parameter | Description
--- | ---
Start Angle | Must be >= 0
Window length | Must be > 0
Number of samples | Minimum value =1 Maximum value = 80
High Limit | Highest acceptable torque.

## PVTL – Post View Torque Low

Same as monitor Post View Torque High, but this monitor checks that all torque values in the Angle Window Length are above Low Limit instead.

Parameter | Description
--- | ---
Start Angle | Must be >= 0
Window length | Must be > 0
Number of samples | Minimum value =1 Maximum value = 80
Low Limit | Lowest acceptable torque.

## PrT – Prevailing Torque

The monitor calculates the prevailing torque value in the Window Length and checks that it is between the Torque limits. The Angle Window starts at the angle degrees set in Start Angle in reverse direction from the shut-off point. This then spans for the angle degrees set in Angle Window Length in reverse direction. If Start Angle is left blank the angle window starts at the shut-off point. The calculated prevailing torque value is the mean or peak torque value (depending on the parameter set by the user) during the Window Length. The calculated value is saved as result data Prevailing Torque Measured. If Torque compensation is set to On, the Prevailing Torque Measured will be subtracted from all torque result values in consecutive steps. Any previously calculated prevailing torque compensation values will no longer be subtracted from torque result values. If Torque compensation is set to No, no subtraction will be made in consecutive steps.

If the total angle of the step is less than the Start Angle plus Window Length, then the monitor will report NOK.

Prevailing torque can be measured as an average of measured values, or at peak torque. To choose between these two modes, set the Use Value parameter to either Mean torque (for average values), or Peak torque (for peak value).

Parameter | Description
--- | ---
Torque Compensation | On or off.
Start Angle | Must be > 0
Window length | Must be >= 0
Low Limit | Must be > 0
High Limit | Must be >= 0
Use value | Mean torque (for average values), or Peak torque (for peak value).

## PC - Pulse Count

Before using Pulse Count step monitor, it is mandatory that the following license type is installed on the controller:

- Low Reaction Strategies

Pulse Count is valid only for the following tools: ETV-STR61-100-13, ETV-STR61-70-13, ETV-STR61-50-10.

This monitor measures the number of pulses and confirms if it is between the pulse count low limit and pulse count high limit.
If the torque trigger level is set, the check starts as soon as the measured torque is above the torque trigger level.

If running a tightening step with Pulse Count step monitor, use the necessary PulseDrive socket/adapter.
If the tightening step runs without the PulseDrive socket/adapter, all the tightenings are NOK. The step error “PulseDrive socket/adapter not detected” shows for no PulseDrive socket/adapter.

Parameter | Description
--- | ---
Pulse Count High Limit - n+ | The Pulse Count limits are used to determine if the measured number of pulses is OK or NOK. The measured number of pulses is OK if it is between the pulse count low limit and pulse count high limit. The measured number of pulses is NOK if: It is higher than the pulse count high limit. It is lower than the pulse count low limit. The trigger torque level is not reached. Pulse count high limit must range from 1 through 9999999. It must be greater than or equal to the pulse count low limit. Pulse Count High Limit text box can be empty.
Pulse Count Low Limit - n- | The Pulse Count limits are used to determine if the measured number of pulses is OK or NOK. The measured number of pulses is OK if it is between the pulse count low limit and pulse count high limit. The measured number of pulses is NOK if: It is higher than the pulse count high limit. It is lower than the pulse count low limit. The trigger torque level is not reached. Pulse Count Low Limit must range from 1 through 9999999. It must be lower than or equal to the Pulse Count High Limit. Pulse Count Low Limit text box can be empty.
Torque Trigger - Tt | Torque Trigger must range from 0 through the maximum torque of the tool. Torque Trigger text box can be empty.

## SOT – Shut Off Torque

The shut off point is the point where the step reaches its target. The torque is measured at the shut off point and checked to be between High limit and Low limit.

Parameter | Description
--- | ---
Low Limit | Lowest acceptable torque.
High Limit | Highest acceptable torque.

## SOC – Shut Off Current

The shut off point is the point where the step reaches its target. The current is measured at the shut off point and checked to be between High limit and Low limit .

Parameter | Description
--- | ---
Low Limit | Lowest acceptable current.
High Limit | Highest acceptable current.

## SSD - Stick Slip Detection

This step monitor detects and reports stick slip effects during a step. The detection is done by counting the number of times the torque falls below the Trigger Level. If the number of times is larger than Maximum Number of Oscillations then the stick slip error is reported. The monitor operates in two different modes, Dynamic or Fixed. The difference between the modes is the way that the Trigger level is calculated.

Dynamic Torque: Trigger Level is dynamically calculated as Peak Torque Percentage of the current max torque, which has been achieved so far during the monitoring. The monitoring is started as soon as the torque passes the Trigger Torque.

Fixed Torque: Trigger Level is the fixed Trigger Torque specified by the user. In this mode the percentage is not needed.

If the torque never reaches the Trigger Torque then the monitoring is not started, this will result in status NOK.

Parameter | Description
--- | ---
Type | Specifies what type of Stick slip detection that will be done in the monitor Stick Slip detection. Default: Dynamic torque.
Peak Torque Percentage | Default: 80%, Must be >=10 and < 100.
Trigger Torque | Default: 5, Must be >= 0 and < Tool max torque.
Maximum Number of Oscillations | Default: 5, Must be >= 3 and <20.

## Ti – Time

Measures the elapsed time during the monitor and checks that it is between the time limits. The time measurement starts at the start of the monitor and, if the Trigger Torque is specified, at the point where the torque passes Trigger Torque for the first time during the monitor.

Parameter | Description
--- | ---
Trigger Torque | Must be >= 0 and < Tool max torque.
Low Limit | Must be >= 0
High Limit | Must be > 0 Must be > Low limit

## TG – Torque Gradient

This monitor checks the gradient is within the limit.

Parameter | Description
--- | ---
Gradient Angle Window | Specifies Angle Window: For Hard Joint: Angle Window = 1 deg. For Soft Joint: Angle Window = 20 deg. Manual: Manually set Angle Window.
Angle Window | Available when Gradient Angle Window is set to Manual. Must be > 0 and <= 100.
End Point Check | If set to Yes, only the gradient measured at the shut off point of the step is checked to be within the limits.
Trigger Torque | The angle measurement starts at this trigger. Must be > 0 and < Tool MaxTorque.
Damping | Frequency in which the gradient is being calculated. Must be > 0 and < 100 and < Angle window.
Low Limit | Lowest acceptable torque gradient. Must be >= -100.
High Limit | Highest acceptable torque gradient. Must be > -100 and > Low limit.
Torque Filter Type | The type of the filter: None: No filtering of the torque is used. The raw values are used as-is in the gradient calculation. Five-point: The torque value used in the calculation are filtered using a sliding average filter over 5 torque samples. Low pass: The torque values is filtered with a simple discrete Infinite Impulse Response filter. Sliding Average: The torque values used in the calculation are filtered using a sliding average filter over a Number of Samples specified by the use.
Cut-off Frequency | Needs to be specified when Torque Filter Type is set to Low pass: 20 Hz 40 Hz 90 Hz 200 Hz 600 Hz
Number of Samples | Needs to be specified when Torque Filter Type is set to Sliding Average: 2 4 6 8 16 32
Angle Offset | Available when End Point Check is set to No. Specifies the degrees that the calculation of the gradient start after the trigger torque is passed for the first time.

## TAW – Torque in Angle Window

This monitor checks that all torque values in the angle window are within the torque limits.

Parameter | Description
--- | ---
Trigger Torque | Must be >= 0
Start Angle | Must be > 0
Window Length | Must be <= 0
Low Limit | Must be >= 0
High Limit | Must be > 0 Must be > Low limit
NOK if window is passed | If set to Yes, status of this monitor is NOK if the end of angle window is not reached.

## TRD – Torque Rate and Deviation

This step monitor measures and checks the torque rate, i.e. the ratio of torque vs. angle. The calculated torque rate is checked if it is within the torque rate limits defined by High Limit and Low Limit.

Parameter | Description
--- | ---
Trigger Torque | Torque of the angle start point.
Start Point Angle | When Start point angle has been measured from Trigger torque the measuring of the torque starts.
End Point Angle | Angle point where the measuring of the torque is stopped.
End Point Torque | Torque where the measuring of the torque is stopped.
Low Limit | Lowest acceptable torque.
High Limit | Highest acceptable torque.
Limit | Must be > 0

## Cl – Click

Monitor to enable click torque and click angle results. This monitor has no settings, and can only be used in conjunction with the MWR step.

## LD - Loosening Detection

This monitor can be used to check the torque and direction to see if a loosening is attempted when using the Wrench Production step strategy for an STWrench. If the applied torque is above the value set for Loosening Limit in the direction opposite to the configured thread direction of the program, the result shall be reported as NOK.

# Step Restrictions

The following sections describe the step restrictions available for the Power Focus 6000, PF8 controller and the Power Focus 6000 StepSync.

In the Power Focus 6000 StepSync controller, it is possible to use synchronisation points in the tightening program and when any condition that is set for a restriction is met, the tool will be stopped immediately and the program jumps to the next synchronization point (only valid for the Power Focus 6000 StepSync and Flex), or the end of the program. Whereas for Power Focus 6000 and PF8 controllers, the tool is stopped immediately and the program jumps to the end of the program.

To make sure the tightening stops if something unexpected happens, it is possible to add restrictions to the multistep tightening program. For each restriction, select Repairable = Yes to allow retry when tightening stops. For each of the steps in a multistep program it is possible to have up to four restrictions.

The following restrictions are automatically added to every step that is added to the multistep tightening program.

Default step restrictions
Step Restriction | Applicable steps
--- | ---
Step Restriction Maximum Time | All except External Result and MWR
Step Restriction Maximum Torque | Tighten to Angle Tighten to Torque+Angle Turbo Loosening Wait Socket release Run until Digital Input Tighten to Trigger Release
Step Restriction Maximum Angle | Tighten to Torque TurboTight Turbo Loosening Tighten to DynaTork Wait Run until Digital Input Loosen to Torque Thread Cutting to Torque Rundown Tighten to Yield Pulsing Rundown Snug TensorPulse

## CTh – Cross Thread

This restriction checks the angle from the point where torque passes Start torque (T1) to the point where the torque passes End torque (T2). If the angle measured from Start torque (T1) is higher than Maximum limit (Amax), the tool is stopped immediately.

When the torque passes End torque (T2), the measured angle is checked against the limit Minimum limit (Amin). If the angle is lower than this limit, the tool is stopped immediately.

Parameter | Description | In illustration
--- | --- | ---
Start Torque | Must be <=0. | T1
End Torque | Must be <=0. | T2
Minimum Limit | The low angle limit. | Amin
Maximum Limit | The high angle limit. | Amax

## A – Maximum Angle

This restriction measures the angle. If the measured angle reaches the Maximum Limit, the tool is stopped immediately. The angle is measured from the start of the restriction or, if specified, from the point where the torque passes Trigger Torque for the first time during the restriction.

Parameter | Description
--- | ---
Trigger Torque | If specified, this is the torque from where the angle is measured.
Maximum Limit | If this limit is reached the tool is stopped immediately.

## T – Maximum Torque

This restriction checks the torque. If the measured torque exceeds the Maximum limit, the tool is stopped immediately.

Parameter | Description
--- | ---
Maximum Limit | If the torque reaches this specified limit the tool is stopped immediately.

Ti – Maximum Time

This restriction checks the time. If Maximum Limit is reached, the tool is stopped immediately.

Parameter | Description
--- | ---
Maximum Limit | If this time is elapsed, the tool is stopped immediately.

## RH – Rehit

This restriction checks the torque. If the measured torque exceeds the Detection Torque, the tool is stopped immediately and the program jumps to the next synchronization point (for Power Focus 6000 StepSync), or the end of the program.

It is only possible to add step Rehit restriction to the first step of the multistep tightening program. Once the Rehit restriction has been added to the first step it shall not be possible to move the step to any other position within the tightening program. The Rehit restriction has to be deleted from the first step in order to move it to other position in the tightening program.

Parameter | Description
--- | ---
Detection Torque | If the measured torque exceeds the Detection Torque, the tool is stopped immediately and the program jumps to the next synchronization point (for Power Focus 6000 StepSync), or the end of the program. Must be greater than zero.
Angle Window (valid only for Power Focus 6000 StepSync) | The angle window is measured from the start of the step. If no Angle Window is set, the restriction is active during the whole step.

## RT – Rescinding Torque

This restriction checks the torque. If the measured torque drops below the condition of the restriction the tool is stopped immediately and the program jumps to the next synchronization point (for Power Focus 6000 StepSync), or the end of the program.

- Torque control processes
  The restriction condition is the measured torque. For the restriction to be active the torque must first exceed 110 % of the Rescinding Torque Limit.

- Angle control processes
  This restriction checks the maximum torque reached during the restriction. For the restriction to be active the torque must first exceed the Trigger Torque.

Torque control processes
Parameter | Description
--- | ---
Rescinding torque limit | Default: 10 Nm. Must be > 0.

Angle control processes (valid only for Power Focus 6000 StepSync)
Parameter | Description
--- | ---
Trigger Torque | Must be > 0.
Peak torque percentage | Default: 95. Must be >= 50.
Rescinding torque time | Default: 20. Must be >= 5 and <= 500.
Rescinding Torque Angle | Must be > 0.

Cable tools have the option to select Rescinding Torque for Angle. This restriction is controlled by two parameters: Peak Torque Percentage and Rescending Torque Time. Percentage sets the downward deviation from the last peak torque, and Rescending Torque Time sets the duration (between 5 and 500 ms) of that deviation. Only when both conditions (equal to or lower than the indicated percentage for the set duration) are met, will the program be interrupted and jump to the end.

## TG – Torque Gradient

This restriction checks the gradient and if it is outside the limits the tool is stopped immediately and the program jumps to the end of the program.

Parameter | Description
--- | ---
Gradient Angle Window | Specifies Angle Window: For Hard Joint: Angle Window = 1 deg. For Soft Joint: Angle Window = 20 deg. Manual: Manually set Angle Window.
Angle Window | Available when Gradient Angle Window is set to Manual. Must be > 0 and <= 100.
Trigger Torque | Must be > 0 and < Tool MaxTorque.
Damping | Frequency in which the gradient is being calculated. Must be > 0 and < 100 and < Angle window.
Minimum Limit | Must be >= -100.
Maximum Limit | Must be > -100 and > Low limit.
Torque Filter Type | The type of the filter: None: No filtering of the torque is used. The raw values are used as-is in the gradient calculation. Five-point: The torque value used in the calculation are filtered using a sliding average filter over 5 torque samples. Low pass: The torque values is filtered with a simple discrete Infinite Impulse Response filter. Sliding Average: The torque values used in the calculation are filtered using a sliding average filter over a Number of Samples specified by the use.
Cut-off Frequency | Needs to be specified when Torque Filter Type is set to Low pass: 20 Hz 40 Hz 90 Hz 200 Hz 600 Hz
Number of Samples | Needs to be specified when Torque Filter Type is set to Sliding Average: 2 4 6 8 16 32

## TAW – Torque in Angle Window

This restriction checks that the measured torque in the Angle Window Length is between the Torque limits. If the measured torque is outside the limits the tool is stopped immediately and the program jumps to the end. The Angle Window Length starts at the Start Angle from the point that the torque first passed the Trigger Torque. If Trigger Torque is not set, then the Start Angle begins at the start of the restriction.

If the end of the Angle Window Length is not reached, the status of the restriction is NOK.

Parameter | Description
--- | ---
Trigger Torque | Must be >= 0
Start Angle | Must be >= 0
Window Length | Must be >0
Minimum Limit | Must be >= 0
Maximum Limit | Must be <= Minimum limit

## TCD - Torque vs Current Deviation

This restriction verifies that all current measurements converted to the corresponding torque are, at most, the Maximum deviation away from the actual torque measured with the torque transducer. The restriction starts when the torque reaches Trigger Torque for the first time during the step and is active until the step reaches its target.

If Trigger Torque is never reached, the monitor will report OK.

Parameter | Description
--- | ---
Trigger Torque | Must be >= 0
Maximum Deviation | Default: 1, Must be > 0

## PCH - Pulse Count High

Before using Pulse Count High step restriction, it is mandatory that the following license type is installed on the controller:

- Low Reaction Strategies

Pulse Count High is valid only for the following tools: ETV-STR61-100-13, ETV-STR61-70-13, ETV-STR61-50-10.

This restriction gives a limit to the number of pulses, and makes sure that those are below the specified pulse count high limit.
If the measured number of pulses is higher than the pulse count high limit, the tool is stopped immediately and the program goes to the next synchronization point or the end of the program.
If the torque trigger level is set, the check starts as soon as the measured torque is above the torque trigger level.

If running a tightening step with Pulse Count High step restriction, use the necessary PulseDrive socket/adapter.
If the tightening step runs without the PulseDrive socket/adapter, all the tightenings are NOK. The step error “PulseDrive socket/adapter not detected” shows for no PulseDrive socket/adapter.

Parameter | Description
--- | ---
Pulse Count High Limit - n+ | Pulse count high limit must range from 1 through 9999999. Pulse Count High Limit text box can be empty.
Torque Trigger - Tt | Torque Trigger must range from 0 through the maximum torque of the tool. Torque Trigger text box can be empty.

# Result Reporters

The result reporters makes it possible to extract specific values of selected producer from the result. The result reporters belong to a step but has to be tied to the monitor/restriction which they read the values from. Only monitors or restrictions located in the same step as the result reporter can be selected. A result reporter is added to a step using drag and drop (in the same way as monitors and restrictions). Each result reporter is responsible for reporting a specific result value, for example, Rundown Angle, Final Torque, Prevailing Torque.

It is possible to tie a result reporter to:

- Program monitors

- Step monitors

- Step restrictions

Each result reporter defines a final value type:

- Final Angle

- Final Torque

- Prevailing Torque

- Self-tap Torque

- Current

- Rundown Angle

- Number of Pulses

## General Parameters

Parameter | Description
--- | ---
Producer | Specifies which monitor/restriction produces the value.
Value | Specifies which value to show from the selected producer.

Limitations:

- It is only possible to add a result reporter on a monitor/restriction belonging to a step in main path or a program monitor/program restriction.

- There may exist several reporters on a step if they are of different type.

- There may exist a result reporter of, for example, type final angle on every step and program monitor angle.

- For those monitor/restrictions that have more than one result value, it is possible to add more than one result reporter if the result reporters are of different types.

- There may not exist several result reporters of the same type on a step or on a program monitor/restriction.

- There is only one result reported for each possible final value type.

Rules:

- The internal number of a result item has to be the same as for the corresponding result reporter.

- The internal number of a monitor/restriction result has to be the same as the internal number of the monitor/restriction in the configuration.

- The step results has to be ordered according to the order of execution. The first executed step has to be first.

Possible values reported by a result reporter if present in the monitor/restriction/step:

- The monitors/restrictions measured value (as float or integer)

- The monitors/restrictions high and low limits

- Status

- Torque trigger and angle trigger

- Angle target and torque target (read from the step)

Possible values for status:

- Low

- OK

- High

- Other

- NotSet

The target values do not belong to any step monitor so the target values are taken from the step that the monitor belongs to.

# Adding a Multistep Program

1. In the Tightening menu, click on the Multistep program library.

2. Click on the Plus icon top right and choose the appropriate type of program in the pop-up window (Tightening or Loosening).

# Deleting a Multistep Program

1. In the Tightening menu, click on the Multistep program library.

2. In the list, click on the multistep tightening program you want to delete.

3. In the program itself, at the bottom left, click on Delete.

4. Click Yes in the pop-up window to confirm your choice.

# Settings for a Multistep Program

## General Settings

Parameter | Description
--- | ---
Name | A user defined name for the multistep program.
Thread Direction | Direction of the threads, either clockwise (CW) or counter clockwise (CCW).
Loosening Program | Indicate if a loosening program is available. Choose from the list of available loosening programs in the controller.
Type | Type of program, either Tightening or Loosening.
Program Start | Gives the torque level for generating a result. If left blank, the result is generated every time the tool is started; otherwise result is only generated from the set torque level.
Program End Torque | Gives the torque value that stops a multistep tightening. The signal 168 - Program End is true when, after a multistep tightening Program End Torque has reached, and Program End Timeout has elapsed. Default value for Program End Torque is Tool max torque * 0.03.
Program End Timeout | Gives the time value (in seconds) that stops a multistep tightening. The signal 168 - Program End is true when, after a multistep tightening Program End Torque has reached, and Program End Timeout has elapsed. Default value for Program End Timeout is 0 seconds.
True Angle Compensation | Turns True Angle Compensation on or off (default is Off).

## Attachment Tuning

Parameter | Description
--- | ---
Use attachment tuning | Select whether attachment tuning should be on or off.
Gear ratio | The gear ratio value can be between 0.5 and 4.0.
Efficiency tuning | The efficiency tuning value can be between 0.5 and 1.0.

## Program Monitor

Parameter | Description
--- | ---
Angle | Turn angle monitoring On or Off for the entire program. If Active in steps and Trigger Torque are left blank, angle monitoring will start at program start.
Active in steps | Sets a range of steps the angle monitoring is valid for. If no end step is specified, angle monitoring will stop at the last step of the program that is not a Socket Release step.
Type | Type of angle monitoring. Choose between: Peak Angle: the highest angle reached during the monitor Angle at Peak Torque: the angle at the point where the highest torque was reached during the monitor (Not available for STB tools) Shut Off Angle: the angle at the shut-off point of the step Angle at End: the angle at the end of the monitor, including the brake, if active.
Trigger torque | Sets the value of the trigger torque for angle monitoring. For STB tools, Trigger Torque will only activate in the tightening direction when executing a tightening program; and only in the loosening direction when executing a loosening program.
Low limit | Sets angle monitoring (program) lower limit.
High limit | Sets angle monitoring (program) higher limit.
Torque | Turn Torque monitoring On or Off for the entire program. If Active in steps is left blank, torque monitoring will start at program start.
Active in steps | Sets a range of steps the torque monitoring is valid for. If no end step is specified, torque monitoring will stop at the last step of the program that is not a Socket Release step.
Type | Type of angle monitoring: Peak Torque: the highest torque reached during the monitor. Shut Off Torque: the torque at the shut-off point of the step.
Low limit | Sets torque monitoring (program) lower limit.
High limit | Sets torque monitoring (program) higher limit.

## Program Restrictions

Parameter | Description
--- | ---
Maximum Time Limit | Set amount in seconds. This restriction checks the total time for the tightening and if it exceeds the Time High limit the tool is stopped immediately. The time is measured from the start of the program.
Maximum Torque Limit | This restriction checks the torque and if the measured torque exceeds the Torque High limit the tool is stopped immediately.

## Reporters

This enables the user to choose which values (from monitors/restrictions) shall be shown as final values. Click Add to choose a result reporter to be tied to a program monitor/restriction value.

Parameter | Description
--- | ---
Reporter | Select a result reporter.
Producer | Select which monitor/restriction produces the value.
Value | Select which value to show from the selected producer.

## Trace Configuration

The trace configuration can be done on program level or for each step. The default configuration is set on the program level and can be overridden in each step as needed.

Here, enabling this function allows the configuration to be done on program level.

Parameter | Description
--- | ---
Enabled | On: Enables the trace resolution configuration on program level. Off: The trace recording is done with the same resolution for the whole tightening. In this case, the trace points are evenly distributed in time over the whole tightening. For each time slot (0.25 ms) two values (the minimum and the maximum measured value) are displayed in the trace. The maximum number of samples in this format is 2000.
Sample Type | Sample Time: specifies how often samples should be stored in the trace by specifying a sample time in ms. Sample Angle: specifies how often samples should be stored in the trace by specifying a sample in deg.
Sample Time | Choose the sample time from the drop-down list (0.25 - 1000 ms)
Sample Angle | Choose the sample angle from the drop-down list (0.25 - 20 degree)

## Validation

Parameter | Description
--- | ---
Validate against tool values | Use On if tool is known and set Max Torque and Max Speed. Use Off if tool is not known.
Tool | Drop-down for choosing the tool to validate against.
Max torque | Max torque of the tool to validate against.
Max speed | Max speed of the tool to validate against.

Relevant Information

- Program End - 168

# Creating a Multistep Program

To create a multistep program, drag and drop steps, monitors and restrictions in the tightening area.

Steps can only be placed between the start and end points of the program, whilst monitors and restrictions can only be placed on steps.

Function |  | Description
--- | --- | ---
Start and end points |  | Start and end points of the multistep program. All steps must be placed between these two points.
Adding a step |  | Drag a step from the list and drop it in the desired position between the start and end points.
Moving a step |  | Click and hold a step and move it to the desired position
Showing step properties |  | Click on the step to reveal the properties
Closing step properties |  | Click anywhere in the tightening area to close the properties menu
Deleting a step |  | Open the step properties and click Delete at the bottom of the menu
Adding a restriction/monitor |  | Drag a restriction/monitor from the list and drop it on the appropriate step.
Moving a restriction/monitor |  | Click and hold the icon (checkmark for monitor, stop sign for restriction) and drag and drop it on the appropriate step
Showing restriction/monitor properties |  | Click on the restriction/monitor icon to reveal the properties menu
Closing restriction/monitor properties |  | Click anywhere in the tightening area to close the properties menu
Deleting a restriction/monitor |  | Open the restriction/monitor properties and click on Delete at the bottom of the menu
Step error |  | When a validation error occurs in a step, that step will be marked. Note that when the step properties are opened, the parameter causing the error will also be marked.
Monitor/Restriction error |  | When a validation error occurs in a monitor or restriction, that monitor or restriction will be marked. Note that when the monitor/restriction properties are opened, the parameter causing the error will also be marked.
Forbidden placement |  | When a particular placement (of a step, monitor or restriction) is not allowed, the placeholder icon will not be shown.

# Multistep Program Tool Compatibility Table

The availability of steps, monitors and restrictions depends on the license installed on the controller.

The table below shows which steps, monitors and restrictions are available for the various tools.

Supported Tools | ES | ST | STR | IXB | SR | SL (Low Voltage) | BCV-RE/BCP-RE | MWR | STB | QST | STW | External Tool
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
PF6000-Handheld | X | X | X | - | X | X | X | X | X | X | X | X
PF6000-StepSync | - | X | X | - | X | X | - | - | - | X | - | -
PF6000-Fixtured | - | - | - | - | - | - | - | - | - | X | - | -

Step Type | ES | ST | STR | IXB | SR | SL (Low Voltage) | BCV-RE/BCP-RE | MWR | STB | QST | STW | External Tool
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
Tighten to Angle | X | X | X | X | X | X | - | - | X | X | - | -
Tighten to Torque | X | X | X | X | X | X | - | - | X | X | - | -
Tighten to Trigger Release | X | X | X | X | X | X | - | - | X* | - | - | -
Tighten to Torque + Angle | X | X | X | X | X | X | - | - | X | X | - | -
Tighten to Torque AND Angle | X | X | X | X | X | X | - | - | X | X | - | -
Tighten to DynaTork | X | X | X | X | X | X | - | - | X | X | - | -
Wait | X | X | X | X | X | X | - | - | X | X | - | -
Socket Release | X | X | X | X | X | X | - | - | X | X | - | -
Run until Digital Input | X | X | X | - | X | X | - | - | - | X | - | -
Tighten to Torque or Angle | X | X | X | X | X | X | - | - | X | X | - | -
Loosen to Angle | X | X | X | X | X | X | - | - | X | X | - | -
Loosen to Torque | X | X | X | X | X | X | - | - | X | X | - | -
Loosen to Trigger Release | X | X | X | X | X | X | - | - | X* | - | - | -
Thread Cutting to Torque | X | X | X | X | X | X | - | - | X | X | - | -
Synchronization Point | - | - | - | - | - | - | - | - | - | X## | - | -
Engage | X | X | X | X | X | X | - | - | - | X | - | -
Rundown | X | X | X | X | X | X | - | - | - | X | - | -
Tighten to Yield | X | X | X | X | X | X | - | - | - | X | - | -
Tighten to Yield M2 | - | - | - | - | - | - | - | - | - | X | - | -
External Result | X | X | X | - | X | X | X | - | X | X** | - | X
Clutch | - | - | - | - | - | - | X | - | - | - | - | -
Clutch Loosen | - | - | - | - | - | - | X | - | - | - | - | -
Mechatronic Wrench (MWR) | - | - | - | - | - | - | - | X | - | - | - | -
Torque Calibration | - | - | - | - | - | - | - | - | - | X# | - | -
Wrench Production | - | - | - | - | - | - | - | - | - | - | X | -
Wrench Quality | - | - | - | - | - | - | - | - | - | - | X | -

Monitors (Evaluated at End of Step) | ES | ST | STR | IXB | SR | SL (Low voltage) | BCV-RE/BCP-RE | MWR | STB | QST | STW | External Tool
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
Time | X | X | X | X | X | X | - | - | X | X | - | -
Angle | X | X | X | X | X | X | - | X | X | X | X | -
Peak Torque | X | X | X | X | X | X | - | X | X | X | X | -
Shut Off Torque | X | X | X | X | X | X | - | - | X | X | - | -
Torque Rate Deviation | X | X | X | X | X | X | - | - | - | X | - | -
Post Thread Cut Angle | X | X | X | X | X | X | - | - | X | X | - | -
Post Thread Cut Peak Torque | X | X | X | X | X | X | - | - | X | X | - | -
Torque in Angle Window | X | X | X | X | X | X | - | - | X | X | - | -
Post View Torque High | X | X | X | X | X | X | - | - | X | X | - | -
Post View Torque Low | X | X | X | X | X | X | - | - | X | X | - | -
Angle from Yield | X | X | X | X | X | X | - | - | - | X | - | -
Stick-Slip detection | X | X | X | X | X | X | - | - | - | X | - | -
Prevailing Torque | X | X | X | X | X | X | - | - | X | X | - | -
Shut Off Current | X | X | X | X | X | X | - | - | X | X | - | -
Click | - | - | - | - | - | - | - | X | - | - | - | -
Torque Calibration | - | - | - | - | - | - | - | - | - | X# | - | -
Loosening Detection | - | - | - | - | - | - | - | - | - | - | X | -

Restrictions (Immediate Stop) | ES | ST | STR | IXB | SR | SL (Low voltage) | BCV-RE/BCP-RE | MWR | STB | QST | STW | External Tool
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
Maximum Torque | X | X | X | X | X | X | - | - | X | X | - | -
Maximum Angle | X | X | X | X | X | X | - | - | X | X | - | -
Maximum Time | X | X | X | X | X | X | - | - | X | X | - | -
Cross Thread | X | X | X | X | X | X | - | - | X | X | - | -
Torque Gradient | X | X | X | X | X | X | - | - | - | X | - | -
Rescinding Torque - Torque control process | X | X | X | X | X | X | - | - | X | X | - | -
Rescinding Torque - Angle control process | X | X | X | X | X | X | - | - | - | X | - | -
Torque Vs Current Deviation | X | X | X | X | X | X | - | - | - | X | - | -
Torque in Angle Window | X | X | X | X | X | X | - | - | X | X | - | -
Rehit | X | X | X | X | X | X | - | - | X | X### | - | -

Program Monitor Type (Evaluate at end of program) | ES | ST | STR | IXB | SR | SL (Low voltage) | BCV-RE/BCP-RE | MWR | STB | QST | STW | External Tool
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
Program Monitor Angle | X | X | X | X | X | X | - | - | X | X*** | - | -

Program Restriction Type (Immediate Stop) | ES | ST | STR | IXB | SR | SL (Low voltage) | BCX | MWR | STB | QST | STW | External Tool
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
Program Restriction Torque High | X | X | X | X | X | X | - | X | X | X | X | -
Program Restriction Time High | X | X | X | X | X | X | - | X | X | X | - | -

* The STB tool shall only allow loosen to trigger/tighten to trigger release step in a multistep loosening/tightening program.

** External result is not supported in a PF6000-Fixtured/StepSync system.

*** Program Monitor Angle is not supported in a PF6000-Fixtured/StepSync system.

# Only supported by PF6000-Fixtured systems.

## Only supported by PF6000-Fixtured and PF6000-StepSync systems.

###　Not supported by PF6000-Fixtured systems.

# STB Tools and Multistep

Due to the wireless nature of STB tools, some multistep functions and behaviors may differ. Besides the general limitations listed here, descriptions of multistep functions will be additional information on STB tools where necessary.

## Program Validation

All tightening programs will be validated for compatibility with STB tools before the program is downloaded to the tool. If the chosen tightening program is not compatible with the tool, the tool will be locked. When this error occurs, it will trigger event 5030, "Configuration complexity exceeded".

To unlock the tool, reduce the complexity of the tightening program, or choose a different tightening program altogether.

# Step Configuration Stages

The controller tightening programs need parameters to be set in order to execute the programs. Selecting a Strategy and either the Target torque or Target angle are mandatory. Other settings are optional. It is also possible to monitor the tightening as it progresses by adding limits within which the torque or angle rotation must remain.

The tightening procedure is divided into four stages: Start, Rundown, Tightening and Stop.

Typical tightening curve

The figure is typical of how tightenings are described. The curves represent how speed, torque and angle vary over time. All tightening strategies are represented in this way. Parameters, monitors and limits are also shown in detailed figures.

A task is defined from the time a trigger is pressed until the tightening target is reached, or an error occurs.

A combination of a tightening strategy together with specific parameter settings forms a tightening program.

The user can create many different tightening programs, and one of them is selected at runtime.

In this Section

- Start Stage
- Rundown Stage
- Stop Stage
- Loosening a Screw
- Stage Parameter Descriptions

# Start Stage

The optional Start step initiates the tightening, enables socket and thread finding, and the option to detect rehits.

In this Section

- Direction
- Soft Start
- Rehit Detection
- Current Monitoring
- TrueAngle Compensation

# Direction

Direction defines the tightening direction of the spindle to clockwise (CW) or counterclockwise (CCW). The rotation of the spindle will always be in this direction, except when loosening and during the conditioning step used in the Three step strategy.

Parameter | Description | Default value
--- | --- | ---
Thread direction | Defines the tightening direction of the spindle. | Clockwise

# Soft Start

During Soft start it is possible to set the speed, the maximum torque and the the rotation angle to help the screw to enter the thread, and to prevent the tool being jerked out of position when the tool trigger is pressed.

Parameter name | Description | Default value
--- | --- | ---
Soft start | Enables setting of the tool’s speed, angle and maximum torque to facilitate the screw entering the thread. Off: Soft start is turned off. On: Soft start is turned on. | On
Speed | Defines the speed during Soft start. | 35 rpm
Angle | Defines the angle to turn the spindle for the screw to enter the thread. | 90°
Torque max | Defines the upper torque limit during Soft start. If Torque max is exceeded, the tightening is aborted and an error message is given. The tightening will be considered NOK. | 1.25 Nm

# Rehit Detection

When Rehit detection is activated, it is possible to detect a screw that has already been tightened.

Parameter | Description | Default value
--- | --- | ---
Rehit detection | Detects attempts to tighten an already tightened screw. Early: the Rehit detection Early option terminates the tightening immediately when a rehit is detected and ends the tightening in the most ergonomic possible way. To be able to use the Rehit detection Early option, Soft start must be set to On. This is because the Soft start torque max value is used as the torque limit beyond which the tightening is considered a rehit. The tightening is considered as NOK and a rehit error is indicated. Complete: to make a rehit detection when Soft start is not used, the Rehit detection Complete option must be used. Rehit detection Complete does not terminate the tightening until all tightening steps have been executed and consequently takes longer. The tightening is considered a rehit if the speed never reaches half the rundown speed, and a rehit error is indicated. The tightening is considered as NOK. Off: no rehit detection is performed. | Early

# Current Monitoring

Current monitoring provides an extra security to monitor the tightening torque and is a complement to the torque sensor in the tool.

At final target torque, the rotor current is measured and converted to a torque value. If the calculated torque is within 10% of the measured torque, the tightening is considered to be OK.

Parameter | Description | Default
--- | --- | ---
Current monitoring | Switch with On - Off position. Off: Current monitoring is disabled and the tool torque is measured by the torque sensor. On: the current is measured at final torque target and converted to a torque value. The calculated torque is compared to the measured torque. If the difference is within 10%, the tightening is considered OK. | Off

Current monitoring is not implemented for Turbo Tight, Rotate, Pulsing and STwrench strategies.

# TrueAngle Compensation

Certain tools are equipped with a gyro and measure the tool rotation during tightening. If the tool is rotated during tightening, the angle measurement may be corrupted. This leads to faulty tightening if made to angle references. For variations within specified limits, the controller can compensate for these rotations and make a correct tightening.

If the tool rotation is outside specified limits, the tightening is aborted and the result status NOK is reported. Additional information reports Tool movement exceeded.

Parameter | Description | Default
--- | --- | ---
TrueAngle compensation | Available for all tightening strategies except Rotate. Tools which have a crowfoot installed as an attachment do not support the parameter TrueAngle compensation. | On
Tool movement limits - Negative | Only visible if TrueAngle compensation is on. Defines the maximum negative rotation of the tool. If the value is exceeded the tightening is terminated and an error is reported. Expressed in a numeric angle value. Min value: 1 Max value: 180 | 30
Tool movement limits - Positive | Only visible if TrueAngle compensation is on. Defines the maximum positive rotation of the tool. If the value is exceeded the tightening is terminated and an error is reported. Expressed in a numeric angle value. Min value: 1 Max value: 180 | 30

Only tools with gyro have the capability to measure the tool movement.

# Rundown Stage

The part of the tightening from when the screw enters the thread until just before the screw head touches the underlying surface and snug is reached. The torque required during rundown does not contribute to any clamping force.

Parameter | Description | Default value
--- | --- | ---
Rundown speed | Defines the speed during the Rundown step | Tool max speed

In this Section

- Selftap
- Rundown Torque Limits
- Rundown Angle Limits
- Post View Torque
- Rundown Complete

# Selftap

The Selftap step enables tightening where the rundown torque required is greater than the Rundown complete torque, for example when tightening thin layers of metal using self-threading (or self-tapping) screws. The selftap window starts when the torque value reaches SelftapTorqueMin/2. The torque must reach over SelftapTorqueMin, but not pass SelftapTorqueMax, during the angle window.

Parameter | Description | Default value
--- | --- | ---
Selftap | Activates the Selftap step. | Off
Speed | Defines the speed during Selftap. | Soft start speed or 5% of ToolMaxSpeed
Length | Defines the angle to turn the socket during Selftap. Measured from the end of the Start step. | 360°
Torque min | Torque value for lower Selftap limit. | 0 Nm
Torque max | Torque value for upper Selftap limit. | Tool max torque

# Rundown Torque Limits

The friction between the nut and joint can vary. This can cause the torque needed to run a nut down a thread, before engagement with the joint surface takes place, to vary as well. These effects could be, for example, hole interference, prevailing torque or varying lubrication.

Monitoring the rundown torque can be useful when running down a lock nut which has a plastic insert in the threads to help the fastener resist vibration. This will require a higher torque, known as prevailing torque, to overcome the interference.

Parameter | Description | Default value
--- | --- | ---
Rundown torque limits | Sets Rundown torque limits to On or Off. Off: No limits are set. On: Torque limits and angle interval are set. | Off
Offset | Angle offset before the Angle interval begins. | 0°
Length | Angle defining the Rundown torque limit section. | 360°
Torque min | Torque value for lower Rundown torque limit. | 0 Nm
Torque max | Torque value for upper Rundown torque limit. | 19% of Target torque

# Rundown Angle Limits

By monitoring the angle of rotation during rundown, errors such as missing washers or screws with incorrect thread size or length can be detected. For example, threads that are too long would require a greater turning angle for the screw to reach snug.

Parameter | Description | Default value
--- | --- | ---
Rundown angle limits | Activates Rundown angle limits. The angle limits are set relative to when the tool trigger is pressed or when a specified torque value is reached. Angle limits will not be checked during Selftap if Selftap is activated. Off: No limits are set. From trigger:The system starts to monitor the tightening angle as soon as the tool trigger is pressed and reports if angle or time limits are violated. From torque: The system starts to monitor the tightening angle from the specified <From torque> value and reports if angle or time limits are violated. | Off
<From torque> | Torque value from where Rundown angle limits are set. | 10% of Target Torque
Angle min | Angle value for lower angle limit from starting point. | 100°
Angle max | Angle value for upper angle limit from starting point. | 1000°
Time min | Minimum time (in milliseconds) for the step. Measured from the start of the step. | 10 ms
Time max | Maximum time (in milliseconds) for the step. Measured from the start of the step. | 5000 ms

# Post View Torque

Some joints have a torque peak prior to Rundown complete. Post view torque makes it possible to monitor torque values during two specified angular intervals. The interval starts are defined as an angle prior to Rundown complete and torque is then monitored for a specified angular interval.

Post view torque is therefore similar to Rundown torque limits except that the maximum and minimum limits can be positioned independently of each other and can differ in length to better control the outcome of the rundown step.

Parameter | Description | Default value
--- | --- | ---
Post view torque | Post view torque makes it possible to monitor torque values during two specified angular intervals. | Off
Torque min | Torque value for lower Post view torque limit. |
Torque min offset | Angle offset before the Post view torque min interval begins. | 720°
Torque min length | Angle length defining the Post view torque min section. | 90°
Torque max | Torque value for upper Post view torque limit. |
Torque max offset | Angle offset before the Post view torque max interval begins. | 360°
Torque max length | Angle length defining the Post view torque max section. | 90°

# Rundown Complete

Rundown complete sets if the screw has reached snug. It ends the Rundown step so that the tightening step can be entered.

Parameter | Description | Default value
--- | --- | ---
Rundown complete | Specifies how to control when snug is reached. At torque: Specifies the torque value for when the rundown step is completed. | At torque
<At torque> | Defines the torque value for when snug is reached and the rundown step is completed. Rundown complete must be smaller than First torque in multi-step strategies or Target torque in the TurboTight strategy. |

# Stop Stage

The Stop stage terminates the tightening so that the socket can be released.

## Soft Stop

Soft stop causes the tightening stop in a more ergonomic fashion.

Do not stop tools within the time interval of 50-300 ms, as this is known to make it feel like an uncomfortable stop.

Parameter | Description | Default value
--- | --- | ---
Soft stop | Turns the Soft stop on or off. Off: No Soft stop is used. On: Soft stop is activated. When target torque is reached, the tool speed is immediately decreased to 75%. Then the speed is decreased to zero in at most 40 ms. | Off

# Loosening a Screw

By setting the loosening parameters, you can control the behavior of loosening for a specific tightening program. Specify the loosening speed and torque to ensure that the screw is unscrewed as desired, so that the screw thread does not break, regardless of what tool you use.

A loosening is considered OK when Run-up torque is reached. However, the screw will probably not have been fully run up by then. The screw should now be able to be turned using a low torque and the speed can be increased. The operator will need to proceed with the loosening until it is considered finished.

Parameter name | Description | Default value
--- | --- | ---
Detection torque | The minimum torque required to begin performing a loosening operation and produce a loosening result. | 7% ToolMaxTorque
Run-up torque | When the torque falls below Run-up torque, the loosening is considered to be OK. Note! Depending on variations in screw length, the system cannot determine when the screw has been run up completely. This is for the operator to decide. | 3.5% ToolMaxTorque
Loosening speed | Loosening speed will be attained when Run-up torque is reached. | ToolMaxSpeed

# Stage Parameter Descriptions

# Target Torque Limits

By setting the Target torque limits , it is possible to discard a tightening should the torque result not fall within the specified torque limits. A too high torque can cause the screw to deform as a result of passing the yield point, and can even break, or can cause the stripping of threads. Not enough torque result in the clamping force not being enough to withstand the forces for which the joint is designed.

Parameter | Description | Default value
--- | --- | ---
Torque limits | The tightening is considered as NOK if the torque result is outside the range defined by Torque min and Torque max. Auto: Torque limits are automatically set to the default values specified for Torque min and Torque max. Manual: Enables the Torque limit values to be set manually. | Auto
Torque min | Torque value for lower torque limit. Can be entered if Manual has been selected. | 95% of Target torque
Torque max | Torque value for upper torque limit. Can be entered if Manual has been selected. | 120% of Target torque

The parameter Measure torque at can have different values. By default the torque is measured at torque peak. The possible values of the parameter are listed in the table below.

Name | Description
--- | ---
Max torque value | Measures the highest torque value during the tightening.
Value at peak angle | Measures the torque value at the highest angle value.
Value at shutoff | Measures the last torque value before entering the break step.

# Target Angle Limits

With Target angle limits set, it is possible to monitor whether the nut is turned the desired angle during the tightening.

Parameter | Description | Default value
--- | --- | ---
Angle limits | Choose the section of the tightening, in degrees, in which to monitor the angle. Off: No limits are checked. From Rundown complete: The monitoring window is set from when the Rundown complete torque is reached. From torque: The monitoring window is set from when the specified torque value is reached. Torque must be greater than Rundown complete torque. From First target: The monitoring is set from when First target is reached. This option is not available if TurboTight is chosen. Auto: The angle monitoring limits are automatically calculated by the controller Manual: The angle monitoring limits are manually entered. | Off
<From torque> | Torque value from where angle limits are set. |
<From torque> | Torque value from where angle limits are set. | 75% of Target Torque
Angle min | Angle value for lower angle limit | 90°
Angle max | Angle value for upper angle limit | 720°
Time min | Minimum time (in milliseconds) for the step. Measured from the start of the step. | 10 ms For TurboTight: 0 ms
Time max | Maximum time (in milliseconds) for the step. Measured from the start of the step. | 1000 ms For TurboTight: 40 ms

Position 1-4 are valid if the target is torque. Position 5-6 are valid if the target is angle.

The parameter Measure angle at can have different values. The parameter is only available when angle monitoring is turned on for the tightening program used. By default the angle is measured at Max angle value. The possible values of the parameter are listed in the table below.

Name | Description
--- | ---
Value at peak torque | Measures the angle at the highest torque value.
Max angle value | Measures the highest angle during tightening.
Value at shutoff | Measures the last angle value before entering the break step.

# Torque Compensation

By using torque compensation, the actual clamping force applied to the joint can be better determined and the scatter in the applied clamping force can be reduced.

The torque compensation point is set by referring back to a specified angle from Rundown complete and calculating a value for the torque used during rundown. This is then compensated for when creating the preload in the screw by adding the torque value calculated in the torque compensation point to the Target torque.

Parameter | Description | Default value
--- | --- | ---
Torque compensation | Enables adjustment if the Target torque for torque used in the rundown step. Off: No compensation is made. On: Manually sets the Torque compensation point. | Off

# Residual Torque Correlation Factor

The term Residual torque correlation factor is similar to a calibration and adjusts between the dynamic torque, measured in the electrical tool, and the residual torque, measured by a control tool.

The Residual torque correlation factor is available for all tools running the TurboTight strategy and the TensoPulse tightening strategy. It is also available for the battery pulse tools that are supported by the controller.

When using a Residual torque correlation factor that differs from 100, the reported Final torque is no longer the dynamic torque measured by the tool transducer.

The dynamic torque measurement uses an internal torque transducer that constantly measures the torque. When the target torque is reached, the tool stops and the result is evaluated and reported. The measured final torque in the transducer is affected by the joint condition, the tool speed, gears and sockets.

The residual torque is measured after the tightening is completed. It is the torque needed to continue or restart the tightening to a higher level. The residual torque is determining the clamping force in the joint.

A dynamic torque measurement is highly repetitive but may differ between tool type and tool speed. | A handheld calibrated torque wrench provides high accuracy measuring the residual torque but has higher variations due to joint relaxation, torque decay, friction or operator technique.

The Residual torque correlation factor is a compensation between the dynamic torque and the residual torque. The factor should be determined by conducting tests. The selected tightening program is performed a few times and the dynamic torque is recorded. The tightenings are also manually measured to determine the residual torque.

The Residual torque correlation factor can be calculated by dividing a residual torque by a dynamic torque. TheResidual torque correlation factor is presented as percent and is by default 100%. This means the reported dynamic torque value has not been modified.

Parameters | Function
--- | ---
Target torque | The tool target torque set for the tightening using the TurboTight strategy.
Final dynamic torque | The final torque reported as the result of the performed tightening.
Dynamic torque | The dynamic torque measured by a reference transducer.
Residual torque | The desired residual torque that ensures the desired clamping force.
Residual torque correlation factor | The compensation factor between residual torque and dynamic torque

An example of how torque tuning can be used:

The TurboTight strategy is selected. The joint shall be tightened to 12 Nm to reach the desired clamping force. The following set up is made:

Example settings | Value | Function
--- | --- | ---
Target torque | 12 Nm | The programmed desired target torque in the controller
Residual torque correlation factor | 100 | The compensation factor between residual torque and dynamic torque

A number of tightenings are made. After each tightening the joint is checked with a calibrated torque wrench. The average is calculated and the following result has been found:

Initial parameters and results | Value | Function
--- | --- | ---
Target torque | 12 Nm | The programmed target torque in the controller.
Final torque | 12 Nm | The final torque reported as the result of the performed tightening.
Dynamic torque | 12 Nm | The uncompensated measured torque from the tool transducer.
Residual torque | 10 Nm | The residual torque measured with a calibrated torque wrench or other test tool.
Residual torque correlation factor | 100 % | The compensation factor between residual torque and dynamic torque

The testing shows that the residual torque is too low to produce the desired clamp force. The Residual torque correlation factor is calculated to 0.83, which is 83 %. An adjustment of the tuning factor is made and the following result is obtained.

Final parameters and results | Value | Function
--- | --- | ---
Target torque | 12 Nm | The programmed target torque in the controller.
Final torque | 12 Nm | The final torque reported as the result of the performed tightening.
Dynamic torque | 14.5 Nm | The uncompensated measured torque from the tool transducer.
Residual torque | 12 Nm | The desired residual torque that ensures the desired clamping force.
Residual torque correlation factor | 83 % | The compensation factor between residual torque and dynamic torque.

What this shows is that we need to tighten a bit more than the specified target, to compensate for differences and to reach the desired torque in the joint.

It is important that the correlation is made with the same tool type and parameter configuration that will be used in production.

# Trigger Lost

In the Result Evaluation window of the program tightening stage, NOK on trigger lost switch controls whether or not it is allowed to release the tool trigger before the target condition has been reached. The setting can be set to On or Off. Below is a description of the two states.

Switch setting | Description
--- | ---
On | Releasing the trigger before reaching the target condition will result in a NOK tightening.
Off | Releasing the trigger before reaching the target condition will result in an OK tightening as long as all other conditions have been met.

The default behavior is that premature trigger release shall not be allowed.

Availability

The NOK on trigger lost is available in the following tightening strategies: Rotate, Quick Step, Two Step, Three Step, and Impulse - Single Step.

For the tightening strategies Rotate, Quick Step, Two Step and Three Step, Trigger Lost setting is only available when the Target of the program is set to Angle (not Torque).

# Tightening Program Configuration - General Parameters

Changes made to tightening programs in any section need to be actively applied by clicking the Apply button in the bottom right corner of the GUI. Alternatively, changes can be undone by clicking the Undo button in the same location.

When navigating away from the section where changes have been made (by using the Back, Home or Result button), the user will be presented with a warning pop-up where the changes can also be applied or undone. The user cannot proceed without applying or undoing changes.

The general tightening program settings is used to set up and manage the tightening programs by naming tightening programs, to make general tightening settings such as selecting tightening strategy, Manual or Quick prog mode, and to set the tightening program target value.

For more information about tightening parameters, see Start Stage, Rundown Stage, Tightening Strategies, and Stop Stage.

For more information about Loosening parameters, see Loosening a screw.

Relevant Information

- Loosening a Screw
- Rundown Stage
- Start Stage
- Stop Stage
- Tightening Programs

In this Section

- Name
- Strategy
- Target
- Time Monitoring (elapsed time)
- Attachment Tuning

# Name

Use the Name field to give the tightening program a name. This name will be stored with the tightening results and sent to ToolsNet (if applicable). The name can be maximum of 32 characters long.

# Strategy

Strategy sets the tightening strategy to be used with the tightening program.

For more information about the available strategies and the relevant parameters, see "Tightening Strategies".

Relevant Information

- Tightening Programs

# Target

The Quick step, Two step, and Three step strategies enable the choice of tightening towards either a Target torque or a Target angle value. When TurboTight is activated, only the Target torque option is available.

# Time Monitoring (elapsed time)

Time monitoring is available for all tightening strategies except Rotate. Time monitoring can be activated when angle limits are activated. Time monitoring is available for the rundown step and the final step of the tightening step.

To minimize the risk of unexpected jerk at the end of the tightening when using the TurboTight tightening strategy, make sure to activate Time monitoring.

Since handling the trace takes time, there is always a short difference between the Program elapsed time compared to Step elapsed time . This is especially noticeable in programs containing only one step.

When using an STB tool it is not possible to use time monitoring if all monitoring options are switched on.

# Attachment Tuning

Attachment tuning gives the possibility to compensate for front attachments on the tool. The compensation can be made for each tightening program.

An operator can hot swap an attachment and then select a tightening program tuned for that specific attachment.

Attachment tuning is available for all conventional strategies except for the STwrench.

1. In Tightening program settings, set Attachment tuning enabled to Yes

2. Click on Tightening parameters > Edit

3. Click on the start step.

4. Under Attachment tuning, set Use attachment tuning to Yes

5. Set the necessary parameters for Gear ratio and Efficiency tuning (see table below).

Parameters for Attachment tuning
Attachment tuning | Description | Default
--- | --- | ---
Attachment gear ratio | The Attachment gear ratio is needed to compensate the angle. Minimum: 0.5 Maximum: 3.6 Socket rotation speed = Tool speed / gear ratio | 1.0
Efficiency tuning | Attachment gear ratio combined with the Efficiency tuning is needed to compensate the torque. Minimum: 0.5 Maximum: 1.0 For example 0.9 means 10% efficiency loss. | 1.0

# Working with the Batch Sequence Tab

Controller features, such as the Low Reaction Tightening Strategies and controller-wide functions among others, require licenses distributed through the Functionality Management System (FMS). Whereas configuration of features is possible without specific licenses, the assignment and use of those features will require the correct license to be installed on the controller. Please refer to Licenses (FMS) for more detailed information on licenses.

Batch sequences are used to perform a specified number of tightenings in a specific order. Each batch sequence is given a name.

In this Section

- Batch Sequence Settings
- Batch Configuration

# Batch Sequence Settings

A batch sequence can consist of up to 99 batches, with a batch size of up to 250 tightenings. The batches in a batch sequence are carried out in the order listed, or by using a Socket selector to choose which batch to run.

Batch settings parameters
Parameter name | Description | Default value
--- | --- | ---
Lock tool on Batch sequence compl. | A batch sequence is completed when the batch sequence counter is equal to the batch sequence size. On: The tool is locked and a tightening program or batch sequence must be selected to continue performing tightenings. Off: After completion, the batch sequence is ready to be repeated. | On
Free order | No: The configured batches will be executed in the order listed, provided they have been configured to perform tightenings. If socket has been specified, the system will prompt for the socket when the batch is to be performed. Yes: The configured batches can be executed in any order. The operator must indicate to the system which batch is to be executed by using a Socket selector. A batch is regarded as complete when all joints have been completed. | No
Increment on NOK | Makes it possible to increment the batch counter value even though the tightening is reported as NOK. For Max consecutive NOK to work (the maximum number of times a single bolt can be tightenened), Increment on NOK must be set to No. Setting this parameter to Yes, will allow the sequence to move on to the next tightening. | No
Max consecutive NOK | Maximum consecutive not OK tightenings (NOK) are a defined maximum allowed number of NOK consecutive tightenings in a batch. If the Max consecutive NOK number is reached, the event Too many NOK tightenings (4020) is displayed. | 0
Decrement on loosening | Decrements the counter within the currently active batch. Completed batched cannot be decremented. Never: The setting is off. Counter is not decremented when loosening is performed in the active batch. Always: The batch counter is decremented when a loosening is performed. When last tightening was OK: If the preceding tightening was OK, the batch counter is decremented when a loosening is performed. | Never
Sequence abort timer | On: The selected batch sequence can be aborted within a specified time limit Off: The selected batch sequence cannot be aborted. | Off
Abort time (10-600) | The number of seconds during which the selected batch sequence can be aborted. | 10

# Batch Configuration

A batch is set up to perform a specified number of consecutive tightenings using the same tightening program. Batches must have tightening program and batch size specified in order to run.

Batch configuration parameters
Parameter | Description
--- | ---
Tightening program | The tightening program to use with the batch.
Batch size | Number of tightenings the batch will perform. Max. number of tightenings in one batch is 250. Batch size 0 will give the batch an infinite number of tightenings.
Identifier number | When using a Socket selector, this is the socket position used to activate the batch.

# Working with the Sources Tab

External signals used as tasks for tightenings are configured in the Sources menu. Sources are accessories or similar connected to a virtual station. Two types of source tasks are available:

- Source Tightening task

- Source Batch task

Source Tightening is used to select a single tightening program.

Source Batch is used to select a batch sequence, a series of tightening programs.

For more information about selection of tasks, see Assigning a Task to a Virtual Station.

In this Section

- Source Tightening
- Source Batch Sequence

# Source Tightening

The tightening menu shows a list of source tightening configurations. Separate lists can be linked to a Virtual Station by going to the Virtual Station in question, and choosing Task, Change task. There, a Source can be chosen as a task. Source tightenings link a specific tightening program to an identifier number. When the identifier number is sent to the controller (either by external digital signal, or, in cases where a socket selector is used, by lifting the corresponding socket in the selector) the linked program will run over and over until a different signal is sent (or socket is picked up). There is no batch counting.

Source Tightening lists can be set either in Control or Confirm mode.

When set to Control, an external source selects a tightening program by requesting an identifier number. In case of a socket selector, the identifier number is linked to a corresponding socket in the socket selector, and by lifting the socket the tightening program is selected.

In Confirm mode, the socket selector cannot be used as a controlling source. In this mode identifier numbers are linked to both a tightening program and a specific socket (indicated in an additional column in the list). When an identifier number is requested (by an external signal), the corresponding socket is prompted in the socket selector and the tightening program is activated when the operator lifts the socket (other sockets are disabled). If no socket is specified (that is, set to 0 in the Socket column), the tightening program is activated directly and the socket status is ignored.

## Product Essentials Tutorials

https://www.youtube.com/watch?v=vVAaKtp3O5k

In this Section

- Creating a Source Tightening

# Creating a Source Tightening

Changes made to tightening programs in any section need to be actively applied by clicking the Apply button in the bottom right corner of the GUI. Alternatively, changes can be undone by clicking the Undo button in the same location.

When navigating away from the section where changes have been made (by using the Back, Home or Result button), the user will be presented with a warning pop-up where the changes can also be applied or undone. The user cannot proceed without applying or undoing changes.

1. Go to the Sources menu, then select Tightening on the left navigation.

2. Click the plus icon in the top right of the workspace.

3. Give the Source Tightening a name and select the correct Selector mode (Control or Confirm, depending on what is required).

4. By default, only one editable Identifier number will be available when creating a new Source Tightening. At the bottom of the screen, click the plus icon to add more.

5. Give every item an identifier number

   If a socket selector is used, the identifier numbers will correspond to the positions in the socket selector, i.e. Identifier number 1 corresponds to socket number 1 in the socket selector.

6. Choose a tightening program to link to each identifier number by clicking on Program and choosing from the list of tightening programs.

## Sources - max consecutive NOK

Max consecutive NOK can be set per Source Tightening or per individual program included in the Source Tightening.

Setting the max consecutive NOK per Source Tightening

1. Set Max consecutive NOK per program to No

2. Set the value in the Max consecutive NOK field.

Setting the max consecutive NOK per program

1. Set Max consecutive NOK per program to Yes

2. For every program in the Identifier selector configuration section, set the value in the Max NOK column.

Relevant Information

- Source Tightening

# Source Batch Sequence

The Source Batch configuration is found under the Batch option in the Sources menu.

The controller can be configured to select a batch sequence based on either an identifier number or an identifier string.

Input | Description
--- | ---
Identifier number | The number must be a positive integer number that can originate from an accessory or from an external control entity.
Identifier string | The string must consist of ASCII characters and can originate from a scanner or from an external control entity.
Socket selector | The use of one or several socket selectors.

## Product Essentials Tutorials

https://www.youtube.com/watch?v=-dTjDz6ravw

In this Section

- Creating a Source Batch
- Configuring Significant Positions to Read in Barcode String
- Combining Identifier Strings

# Creating a Source Batch

1. Go to the Sources menu, then select Batch sequence on the left navigation.

2. Click the plus icon in the top right of the workspace.

3. Give the Source Batch a name

4. Set the Abort on new identifier to Yes if scanning a new identifier string should abort the previous scan.

5. Select the Identifier method (String for text, or Number for numerical strings)

6. Set Free order to On if the strings should be able to be scanned in any order.

   Identifier strings can be made up of up to 4 different strings. When free order is set to No, the strings need to be scanned in a specific order for the system to recognize the string.

7. If required, add an identifier string by clicking on the Plus icon in the Identifier string configuration section.

8. Click on the Name label for the identifier string you want to change the properties of (pop-up window). The following properties can be indicated per string:

   - Name - the name of the string

   - Length - the length of the string. See Combining Identifier Strings for more information on concatenating strings.

   - Significant positions - used to specify which characters in the barcode string to read when putting together the string to match with your pre-defined string. The number of significant positions must match the number of characters in the pre-defined strings.

   - Saved positions - indicate which parts of each string used in the Source Batch is saved, and how they are represented in the log. In this field, indicate the positions in the string that need to be saved. Positions can constitute only parts of the entire string. If the field is left empty, the entire (concatenated) string will be saved. The table below shows some examples of saved position combinations.

     Saved position values are comma-separated (without spaces), and ranges are indicated using a hyphen.

   Identifier string | Positions
   --- | ---
   String 1: 1234567 | 1-7
   String 2: abcdef | 8-13
   String 3: GHIJKL | 14-19
   String 4: 890 | 20-22

   Saved position examples
   Saved positions | Saved results
   --- | ---
   (empty) | 1234567abcdefGHIJKL890
   1-3,9,11,15,20-22 | 123bdH890
   8-12,1-7,19,20-21 will be changed automatically to: 1-12,19-21 | 1234567abcdeL89

   The ID field in the string properties window cannot be altered, but can only be used to navigate between the different strings.

   An error may occur when Free order is set to On, and the lengths of the different strings are duplicated. The scanned sequence will then not activate a tightening program. To remedy this error, set Free order to Off, or adjust the string lengths.

9. Click Edit.

10. In the Edit window, indicate which strings (in the String contains column) should be linked to which Batch sequence (in the Activates column). Click the plus icon at the bottom to add more strings.

    Wildcards can be used when typing the "string contains". The wildcard(s) can be used at any position in the string. No Batch sequence is activated in case of an ambiguous matching result.

    The wildcard is a . (period)

Relevant Information

- Combining Identifier Strings
- Configuring Significant Positions to Read in Barcode String

# Configuring Significant Positions to Read in Barcode String

The positions in the barcode string are associated with a number between 1 and 1024. The first position of the string is 1 and the last is 1024.

The significant positions must be specified following the rules described in the table below. Barcode strings:
Description | Significant positions | Valid configuration | Barcode string to match with pre-defined string
--- | --- | --- | ---
Significant positions in order | 1,2,3,7,8 | Ok | ABCGH
Significant positions in optional order | 7,1,2,3,8 | Ok | GABCH
Range of numbers | 1–3,7-8 | Ok | ABCGH

# Combining Identifier Strings

The identifier string that is used for matching is a combination of up to four strings from a factory management system or up to four scanner inputs that need to be combined into one string.

The Add and Delete command buttons manage how many strings are combined. The following parameters are available:

Parameters for combining identifier strings
Parameter | Description
--- | ---
Check box | Select an entry if it is to be deleted.
Name | The string must be given a name.
Length | The length of the string must be known and must be entered. This is important to be able to combine the correct string identifier.
Significant positions | The comma-separated positions or ranges (separated by hyphen) in the combined string that are used for matching.
Saved positions | The comma-separated positions or ranges in the strings that will be saved in the result.

If more than one identifier string is to be used, perform the following steps:

1. Press the Add command button to create a new entry in the table.

2. Issue the string a name.

3. Enter the length of the string.

4. Repeat steps 1-3 for every string to be added. Up to four strings can be combined.

The Start-End parameters in each row define the individual string positions in the combined string identifier that is used in the next step of the matching process.

The first part in the task selection process using an identifier string as an input, is to define which positions in the string that are to be activated:

- Enter the significant positions, to define which positions in the identifier string will be used for matching. The positions must be either comma-separated, or by range.

# Working with the Tool Tab

A tool must be connected to the controller for the Tool menu to show information.

In this Section

- Tool Information
- Tool Connection
- Tool Health
- Tool Maintenance
- Tool Calibration
- Tool Motor Tuning
- Open End Tuning
- WLAN and Bluetooth for Wireless Tools

# Tool Information

The Tool information view contains information used for giving service personnel accurate information about the tool connected to the controller, so that they can give adequate help and support, or for operators to see what tool is connected to the controller.

Tool information
Information | Description
--- | ---
Model | Tool model denomination.
Max torque | The maximum torque the tool can use for a tightening.
Min speed | The minimum rotation speed of the tool.
Max speed | The maximum rotation speed of the tool.
Min final speed | The minimum final rotation speed of the tool (only for BCP/BCV-RE tools).
Max final speed | The maximum final rotation speed of the tool (only for BCP/BCV-RE tools).
Gear ratio | The ratio of the angular velocity of the input gear to the angular velocity of the output gear.
Serial number | The tool’s serial number may be needed when the correct version of the Product instruction is required, in order to get the correct spare parts or service instructions.
Software version | Tool software version.
Product number | The tool’s Product or Ordering number.

## Tool TAG information

Tool TAG information is only available if the tool type is a STwrench.

STwrench tool information
Information | Description
--- | ---
TAG id | The programmable RFID TAG identification number that is programmed into the End-fitting tool (Socket).
Torque correction coefficient | In certain cases extensions may be needed to fit the application. In this case the wrench measurement must be compensated to show a correct value. To calculate the correction coefficient, refer to the latest version of the STwrench User Guide (printed matter number 9836 4134 01). The parameter is stored in the RFID TAG in the End-fitting tool.
Angle correction coefficient | In certain cases extensions may be needed to fit the application. In this case the wrench measurement must be compensated to show a correct value. To calculate the correction coefficient, refer to the latest version of the STwrench User Guide (printed matter number 9836 4134 01). The parameter is stored in the RFID TAG in the End-fitting tool.
Nominal torque | The smartHEAD of the STwrench contains the torque transducer and defines the wrench’s nominal torque. For more information, refer to the latest version of the STwrench User Guide (printed matter number 9836 4134 01).

NOTICE

The correction coefficients alter the STwrench measurement. It may cause an improper reading. Before making any corrections, refer to the latest version of the STwrench User Guide (printed matter number 9836 4134 01).

# Tool Connection

The tool connection area shows which virtual station the tool is connected to.

Relevant Information

- Connecting a Tool to a Virtual Station

# Tool Health

The Health view contains information about tool temperature.

## Tool temperature

Tool temperatures (both for cabled and battery tools) are monitored continuously by the POWER FOCUS 6000. Supported temperature units are degrees Celsius (°C) and degrees Fahrenheit (°F), with Celsius being the default unit. It is possible to switch between the two units without requiring a controller restart. When the tool motor temperature or tool electronics temperature exceeds max temperature, the tool is locked and an alert (2014) is shown. The tool is once again unlocked when the tool temperature drops below the temperature limit.

Tool temperature is not available for the STwrench.

## Monitoring Tool Temperature

From the display or through the web GUI, users can access the latest tool electronics and tool motor temperatures measured together with the timestamp when the measurement was taken.

1. On the Home view, tap on the Tool Tab.

2. Both tool electronics temperature and tool motor temperature are listed under Health.
   For pulse tools, the Tool pulse unit temperature is also listed.

3. Click on either entry to access a list of peak temperatures and their timestamps.

# Tool Maintenance

The tool stores a service interval number and counts how many tightenings can be performed before a tool maintenance, or service is needed.

## Setting the Maintenance Alarm

1. On the Home view, tap on the Settings Tab, then select Tool.

2. Set the Service indicator alarm to On.

3. Return to the Home view, tap on the Tool Tab, and then select the tool you wish to set the alarm for.

4. Enter a value in the Service interval box.

   Service intervals can only be set in multiples of 10 000. Any number other than multiples of 10 000 is rounded off to the nearest multiple of 10 000.

   When working with pulse tools, both service intervals for number of tightenings and number of pulses is set. Whichever interval is reached first will trigger the alarm.

Maintenance parameters
Field | Description
--- | ---
Last service | Date and time when last service was performed. The Last service date is set at the repair workshop. The Last service date is set to current date and time when the Reset service count button is pressed.
Total tightenings at service | Total number of tightenings performed by the tool since it was used for the first time. This value is made available at service, and will remain the same until next service.
Remaining tightenings | Total number of tightenings left until the service interval is reached.
Service interval | Number of tightenings to be performed between two service events. Can be set in multiples of 10 000.
Total pulses at service | [pulse tools only] Total number of pulses performed by the tool since it was used for the first time. This value is made available at service, and will remain the same until next service.
Remaining pulses | [pulse tools only] Total number of pulses left until the service interval is reached.
Service interval | [pulse tools only] Number of pulses to be performed between two service events. Can be set in multiples of 10 000.
Reset service counter | Reset of the Remaining tightenings counter and sets Last service date to current date.
Reset service data | [pulse tools only] Reset of the Remaining tightenings counter as well as oil status and sets Last service date to current date.

# Tool Calibration

Tool calibration is used to control how well a tool corresponds to a reference transducer.

The calibration value stored in the tool memory is used to adjust the torque value given by the tool’s torque transducer so that the correct torque value is displayed on the controller. The controller displays the date when the tool was last calibrated.

Calibration parameters
Field | Description
--- | ---
Last calibrated | Date and time when last calibration was performed.
Calibration value | Torque value to calibrate against.
Next calibration date | Date when the next calibration of this tool is needed.

In this Section

- Preparing the Calibration
- Calibrating the Tool
- Calibrating a Tool Through the STa6000 or STpad

# Preparing the Calibration

1. Make sure the tool and controller are set up to perform tightening.

2. Set up the tool with a torque reference transducer (such as the STa6000, STpad or JSB Bench).

   Refer to the torque reference transducer User Guide for set-up instructions.

3. Select a Tightening program with a target torque corresponding to a tightening normally used with your tool.

   See Basic Tightening setup for a tutorial on setting up and activating a suitable tightening program.

# Calibrating the Tool

The calibration value used for the tool is calculated from the torque readings read from the controller, and the torque reference transducer through the equation below:

New calibration value = Old calibration value × Mean (Reference values / Power Focus values)

1. On the Home view, tap on Tool Tab and select the tool to be calibrated. Then, go to Calibration.

2. Take note the old calibration value found in the Calibration value text box.

3. Make at least three tightenings and use the torque values read from the controller and the reference transducer (ACTA or similar) for calculating the mean torque values.

4. Calculate the new calibration value using the New calibration value equation.

5. Store the new calibration value in the tool memory by entering the calculated value in the Calibration value text box and tapping Apply.

After calibration is completed, perform a tightening to verify that the new values are correct.

# Calibrating a Tool Through the STa6000 or STpad

## Connecting the STa6000/STpad

The STa6000/STpad can be connected to the controller in two ways:

- Connecting the STa6000

Connection | Remarks
--- | ---
COM port | Connect the Atlas Copco USB to Serial adapter to the controller's USB port using the ACTA Serial cable. Connect the STa6000 to the Serial Adapter using a USB cable.
Ethernet port | Connect the ethernet cable between the STa6000 and the controller's Factory Ethernet port, or the factory network.

- Connecting the STpad

Connection | Remarks
--- | ---
COM port | Connect the STpad to the Controller's COM port using the ACTA Serial cable.
Ethernet port | Connect the ethernet cable between the STa6000 and the controller's Factory Ethernet port, or the factory network.

## Performing the QA Calibration through the STa6000 or STpad

1. Make sure the tool is connected and assigned to a virtual station on the controller.

   Single tightening programs cannot be used for calibration purposes. Make sure a batch program is selected.

2. On the Home view, tap on Tool Tab. Then click on QA Calibration, and set the QA Calibration to On.

3. Select the virtual station the tool to be calibrated is connected to, and select the connection type to be used (TCP of COM port).

   Note that the default port for communication is 4561

4. Connect the STa6000/STpad to the controller, and select the correct virtual station.

5. Start the calibration from the STa6000/STpad.

   The STa6000/STpad requests controller information, including tool information and tightening program.

6. Execute the tightening. When the calibration device detects a tightening, it requests the tightening result from the controller.

7. Repeat the above step until all tightenings in the batch have been executed.

   Once completed, the STa6000/STpad creates a report, as well as calculate a new calibration value for the tool.

8. Select Store in the STa6000/STpad to send the new calibration value to the controller, which in turn writes it to the tool.

During calibration, if the tightening program is changed, or the sequence/batch is updated, the calibration is terminated.

There is no limit in the batch size used for calibration purposes. However, the STa6000 can only display two digits as batch size. Thus, the counter on the Sta6000 reads 00 for 100.

After calibration is completed, perform a tightening to verify that the new values are correct.

# Tool Motor Tuning

A motor tuning adjusts the tool’s motor control unit to optimize the performance and minimize loss.

For cable tools a motor tuning should be performed on each specific combination of controller and tool together. STB tools can be moved to another controller without the need to perform a new motor tuning.

Before performing the motor tuning, make sure the tool is connected to a virtual station and that the controller is set up to perform tightening.

The motor tuning takes approximately 1 minute to perform and rotates the spindle in both clockwise (CW) and counterclockwise (CCW) directions before it is finished.

For tools configured with open end Gear Front Attachment (GFA), remove the open end extension from the tool before performing the motor tuning.

## Performing tool motor tuning

1. On the Home view, select the Tool Tab. Then, select the tool to be motor tuned and go to Motor tuning.

2. Select Perform, and then press the trigger on the tool.

3. Select OK to start the Motor tuning.

   Follow the instructions on the screen and keep pressing the tool trigger until the motor tuning is done.

   - If the motor tuning is successful, an OK event is displayed.

   - If the motor tuning is not successful, or the tool trigger was released before the motor tuning is done, an NOK event is displayed.

# Open End Tuning

The open end tuning function is available for tools configured with open end Gear Front Attachment (GFA).
The function calculates the true gear ratio of both the tool and the extension combined, and saves it to the tool.
The tuning takes approximately 2 minutes to perform.

When the open end tuning is completed, the tool must be calibrated with the open end extension attached.

## Performing open end tuning

1. On the Home view, select the Tool Tab. Then, select the tool to be tuned and go toOpen End Tuning.

2. Select Perform, and then press the trigger on the tool.

3. Follow the instructions on the screen and keep pressing the tool trigger until the open end tuning is done.

   - If the open end tuning is successful, an OK event is displayed.

   - If the open end tuning is not successful, or the tool trigger is released before the tuning is done, an NOK event is displayed.

# WLAN and Bluetooth for Wireless Tools

The POWER FOCUS 6000 controller has built-in wireless LAN and Bluetooth radio modules that enable the connection of wireless tools to a controller using a pairing process. When the pairing is established, the tool will connect to the controller automatically as soon as the tool is in range of the controller. A tool paired with a controller is only able to connect to that specific controller even if another controller is set up to use the same radio channel.

The WLAN radio module in the controller can connect to three tools at a time, while the Bluetooth module allows for six simultaneous connections.

In this Section

- Pairing mode for STB tool and STwrench
- Bluetooth Requirements
- Wireless Tools Restrictions
- Pairing a Wireless Tool to a Controller
- Connecting BCP/BCV-RE Tools

# Pairing mode for STB tool and STwrench

## Placing the STB Tool in Pairing Mode

1. Disconnect the (charged) battery from the tool.

2. Press the tool trigger while re-attaching the battery.

3. When the tool LEDs are off, release the tool trigger.

4. When the tool LEDs are on again, press the tool trigger.

5. When the tool LEDs are off again, release the tool trigger. Both LEDs start to flash (after approximately 10 seconds).

6. The tool is now in pairing mode. The LEDs keep flashing when the tool is in pairing mode.

Do not start the Power Focus pairing procedure before both LEDs on the tool are flashing. Initiate pairing within 30 seconds or the tool might time out.

When the tool is placed in pairing mode, tap the connection type to start the pairing process.

## Placing the STwrench in pairing mode

1. Turn on the STwrench.

2. During the cell and gyroscope adjustment, press the UP, RIGHT and BARCODE buttons on the STwrench keyboard in that order.

3. At the end of the zero adjustment, the wrench is in pairing mode.

When the tool is placed in pairing mode, tap the connection type to start the pairing process.

# Bluetooth Requirements

In order to use Bluetooth with the POWER FOCUS 6000, the following requirements need to be met:

- POWER FOCUS 6000 software 2.6 or higher

- A wireless tool equipped with a Bluetooth module

- Tool software boot version 9.1.6 or higher

- Tool software app version 3.6.1 or higher

# Wireless Tools Restrictions

When all WLAN (3) or Bluetooth slots (6) are filled, additional wireless tools paired with the controller will replace existing paired tools. There are a few rules governing this replacement.

In the case of WLAN, one of the previously paired tools will be replaced at random.

In the case of Bluetooth, offline tools will be replaced first, followed by online tools. Tools linked to a Virtual Station will never be replaced. When pairing an additional Bluetooth-equipped tool to a controller that already has six wireless Bluetiooth tools linked to Virtual Stations, make sure to remove one of the paired tools from one of the Virtual Stations before pairing the additional tool. The tool disconnected from the Virtual Station will then be replaced by the new tool.

# Pairing a Wireless Tool to a Controller

The pairing of a Mechatronic Wrench to a controller is done differently than other wireless tools, and requires an MWRKit to be connected to the controller. Please refer to the tool's Product Instructions for more detailed information.

Before you start the pairing process:

- Make sure WLAN or Bluetooth is enabled in the Controller (Depending on the wireless tool you want to pair)

- Make sure there are pairing slots available (3 for WLAN and 6 for Bluetooth)

- Check which radio channel to use

- Check how to put the tool into pairing mode. See the STB user guide (9836 3043 01) for instructions on how to do this, or follow the instructions below

- If possible, have a clear line of sight between tool and controller

- Make sure no other tools are being paired with the controller at the same time

1. Enable the internal WLAN by going to the Settings > WLAN. Drag the Enabled switch to On

   If the WLAN Enabled switch is set to Off it is not possible to pair a tool to the controller. Tools already connected to the internal WLAN are disconnected when the Enabled switch is set to Off.

2. Set the radio channel to be used with the wireless tool. On the Home view, tap on Settings Tab, and click WLAN.

3. In the Radio channel area, tap the channel list and choose the appropriate channel.

   Changing the channel will permanently disconnect all wireless tools paired with the controller.

4. Return to the Home view, and tap on Tool Tab. Then, tap the pairing icon in the upper right corner.

5. Put the tool in pairing mode. See Putting the wireless tool into pairing mode.

6. In the Pairing dialog box, click Perform to start the pairing process.

7. The pairing process will end with one of the following results:

   - Pairing successful - The tool has been paired to the controller using the selected channel.

   - Pairing unsuccessful - This can be due to any of the following reasons:

     - No tool detected during the pairing process. Make sure the tool is in range and in pairing mode, and then click Close and try again.

     - More than one tool was found during the pairing process. Make sure no other tool is in pairing mode, and then click Close and try again.

     - Pairing already in progress. Make sure no one else is performing the pairing process on the controller, and then click Close and try again.

     - Pairing failed. Click Close and try again.

An IRC-W Infrastructure tool is a tool that is using the factory's wireless infrastructure to connect to the controller. The tool configurations, ADHOC or Infrastructure Mode, are set in ToolsTalk Service 2. A tool configured as an IRC-W Infrastructure tool can also connect as an ADHOC connected tool, using the controllers own built-in network. But when the tool restarts, it will revert to an IRC-W Infrastructure configured tool.

# Connecting BCP/BCV-RE Tools

The process for connecting BCV and BCP tools to the controller is slightly different than for other types of tools.

1. On the Home view, tap on the Settings Tab. Then, select BCP/BCV-RE Connections.

2. Add a new BCP/BCV-RE Connection configuration by clicking on the Plus (+) icon top right.

3. Turn on the configuration and provide a name in the name field.

4. Fill in the Server port and the Server host of the tool you want to connect in the respective fields. You can find both of these in the tool's Loader Software.

The tool should now be connected to the controller. Assign it to a Virtual Station in order to use it with a tightening program.

# Working with the Virtual Station Tab

Virtual stations are configured in the Virtual Station menu.

A virtual station is a software abstraction of a physical station and can be set up to use a specific tool and remotely execute different tasks using the tool.

In POWER FOCUS 6000, it is possible to set up a number of virtual stations per controller. Each virtual station can be connected to one tool and one or more accessories.

By using virtual stations, the operator can operate multiple tools and run different tasks using the same controller. It is possible to connect one cable tool and multiple STB tools simultaneously to the controller.

When configuring different tools, make sure the selected start signal in Start source matches the selected tool and that the selected task can be run on the specific tool.

Before any tightening can begin a task must be selected in the virtual stations menu. A task is of one of three types:

- Tightening program

- Batch sequence

- Sources

The selection can be made manually by the operator or by external signals.

## Product Essentials Tutorials

https://www.youtube.com/watch?v=Ay0zO5fGSD8

In this Section

- Creating a Virtual Station
- Assigning Licenses to a Virtual Station
- Unassigning licenses from a Virtual Station
- Connecting a Tool to a Virtual Station
- Configuring Task Window in a Virtual Station
- Configuring Protocols Window in a Virtual Station
- Configuring Accessories Window in a Virtual Station
- Configuring Fieldbus Window in a Virtual Station

# Creating a Virtual Station

Controller features, such as the Low Reaction Tightening Strategies and controller-wide functions among others, require licenses distributed through the Functionality Management System (FMS). Whereas configuration of features is possible without specific licenses, the assignment and use of those features will require the correct license to be installed on the controller. Please refer to Licenses (FMS) for more detailed information on licenses.

Create a virtual station

To create a new virtual station:

1. Tap on the plus sign.

2. Edit the name and other parameters.

To remove a virtual station: Tap on delete at the bottom of the list of parameters.

The list of virtual stations created is presented in the order of creation.

If no tool configuration is available when assigning a tool, a new tool configuration is automatically created and assigned to the virtual station.

This auto-created tools configuration will have Start source set to Trigger only and trace set to Off. For STB tools Start request will be set to On.

# Assigning Licenses to a Virtual Station

To make virtual stations working, it is needed to assign them a Virtual Station Type license.

1. Select the Virtual Station menu and select the virtual station you want to assign licenses to.

2. In the Licenses section, select the arrow in the Virtual station type field

   The Change License Type window appears.

3. Select the Virtual Station Type you want to assign to the virtual station.

4. [If additional Virtual Station Features need to be assigned] Select Edit in the Features field.

   The Select Features window appears.

5. Check all features you want to assign to the virtual station, then select OK.

# Unassigning licenses from a Virtual Station

1. Select the Virtual Station menu, then select the virtual station you want to unassign licenses from.

2. In the Licenses section, select the name of the license in the Virtual Station Type field.

   The Change License Type window appears.

3. Select the name of the assigned Virtual Station Type you want to unassign.

   The Change License Type closes and the Virtual Station Type field will say None. All features will be removed from the controller as well.

When a Virtual Station is deleted, the licenses associated with that Virtual Station will automatically be returned to the Pool.

# Connecting a Tool to a Virtual Station

A virtual station can only have one tool connected. Just one of the tools connected to a controller can be a cable tool. Added virtual stations can connect wireless tools paired to the controller.

Each virtual station needs to have one tool configuration, in addition to the tool. The tool configurations are created in the Configurations menu.

1. Go to the Virtual station menu and tap the virtual station you want to connect the tool to.

2. In the Tool area, tap Choose tool to open the list of available tools.

   Or, if a tool is already chosen, tap Change tool to open the list of tools available to change to.

3. In the list of available tools, tap the desired tool to connect it to the virtual station.

   Tools not available will be greyed out. To connect such a tool, it must first be disconnected from its virtual station.

4. When connecting a new tool a tool configuration is attached. If there are more than one configuration available a list of tool configurations is shown.

5. To replace the tool configuration for the virtual station:

   - Click on the arrow beside the name of the current configuration.

   - Choose another of the configurations in the list.

   It is not possible to deselect a configuration, only to select another available configuration.

Relevant Information

- Tool Configuration

# Configuring Task Window in a Virtual Station

The selected task can either be running a tightening program, running a batch sequence or enabling the task using a source configured in the Sources menu.

The task can be monitored from the controller and the result of the task can be presented together with any events that may have occurred during the operation.

In this Section

- Configuring Manual Mode in a Virtual Station

# Configuring Manual Mode in a Virtual Station

Manual mode for Virtual stations is used for performing tasks while the tool is in locked mode. In cases where the tool is locked for a certain reason (e.g. because the tool is outside its TLS footprint) there still may be a need to perform certain tasks with the tool, such as performing emergency work. By configuring manual mode for the virtual station, users can determine what signals are sent when entering manual mode (Entering signals), what task can be performed while in manual mode (Secondary task), and what signals are sent when leaving manual mode (Leaving signals).

Since desired scenarios can vary between different users (i.e. which signals to send upon entry and exit and what task to perform), manual mode is fully configurable for each virtual station.

Configuration consists of three elements: entering signals, leaving signals and secondary task (note that by primary task is meant the (automatic) task that is assigned to the virtual station under Task).

1. Go to the Virtual station menu and click on the virtual station to configure, then under Task, click on Set manual mode

2. In the Manual mode configuration screen, set the secondary task. This determines which task shall be run when in manual mode.

   If no secondary task is set, the primary task will be used during manual mode.

   All task types (tightening, batch sequence, source) can be set for the secondary task as for the primary task.

3. Set the entering signals to be sent by clicking the plus icon at the bottom of the Entering section. See the parameters for entering signals below.

4. Set the leaving signals to be sent by clicking the plus icon at the bottom of the Leaving section. See the parameters for leaving signals below.

There is a limit of 99 signals that can be set for entering and leaving.

In this Section

- Entering and Leaving Signals

# Entering and Leaving Signals

The parameters for entering and leaving signals are the same.

There are two types of signals: Boolean and integer/string type. For Boolean type signals, an on/off (true/false) switch is used. For integer/string type signals, a text field is used where the (I/O) signal or string can be indicated.

Signal | Type | Default value
--- | --- | ---
Abort sequence | Boolean | Off
Acknowledge events | Boolean | Off
Activate tool scanner | Boolean | Off
Clear results | Boolean | Off
Disable Fieldbus | Boolean | Off
Disable Open Protocol Commands | Boolean | Off
Disable Tool scanner | Boolean | Off
Dynamic batch size | Integer | 0
External identifier | Integer | 0
External monitored [1-8] | Boolean | Off
Flash Tool Green Led (external protocol) | Boolean | Off
Generic IO [1-10] | Integer | 0
Id for dynamic batch size | Integer | 0
Reset batch | Boolean | Off
Reset batch sequence | Boolean | Off
Reset bistable relay | Boolean | Off
Reset Too Many NOK | Boolean | Off
Select input | Integer | 0
Set bistable relay | Boolean | Off
Unlock tool on complete | Boolean | Off
Unlock tool on disable | Boolean | Off

# Configuring Protocols Window in a Virtual Station

Under the tab Protocols, in the Virtual Station menu, you'll find a list of available communication protocols depending on the current license in use. The Open Protocol is available for all licenses.

To gain access to functionality through Open Protocol, a unique port for each Virtual Station needs to be defined.

1. Set the Open Protocol switch to On.

2. Enter the Server port number.

3. Enter the PLC Index value between 1 to 6.

   PLC Index is used to map where in the shared memory the Open Protocol commands are to be written. The default value is 1 but it is possible to enter values 1 to 6

4. Choose the action to be applied when the connection to the client is lost.

   The Disconnect setting controls the action applied when a connection error occurs:

   - None - The tightening program continues normally.

   - Lock tool - The tool is locked after finishing the current tightening normally.

   - Unassign task - The tightening is aborted after finishing the ongoing task. Except for plain tightening programs or Batch sequences where the task will be removed after finishing.

   - Always lock tool - The tool is locked after finishing the current tightening, regardless of result.

5. Use legacy counter

   The legacy counter setting counts all tightenings in a sequence and outputs that number to secondary systems. To enable this setting, set Use legacy counter to Yes.

6. MID2500 loosening program

   This setting allows for the selection of a MID2500 loosening program from the list.

7. Tap or select Apply when ready.

As the default value for SoftPLC Index is always 1 and no checks are made to see if it is in use, there is a possibility that you may have configured the system so that the same index is configured several times when adding Virtual stations. In this case, the Soft PLC will not be able to determine from which Virtual Station the incoming MID is originating from.

# Configuring Accessories Window in a Virtual Station

For connecting and disconnecting QIF accessories to and from a virtual station, see Connecting QIF accessories to a virtual station and Connecting QIF accessories to a virtual station.

For troubleshooting with the help of I/O diagnostics of an accessory, see Digital Signal Diagnostics.

Relevant Information

- Connecting QIF Accessories to a Virtual Station
- Digital Signal Diagnostics
- Disconnecting QIF Accessories From a Virtual Station

In this Section

- Digital Signal Diagnostics
- Diagnostics Configuration
- Normal Operations
- Monitor Digital Signals
- Force Digital Signals

# Digital Signal Diagnostics

During deployment and during troubleshooting of a controller, a diagnostic tool is very helpful. It is available for the analysis under the Info tag for a device configuration or a fieldbus mapping in the Virtual station menu.

The controller can operate in normal mode or in diagnostics mode. In normal mode the digital input and output signals operate normally and are routed between the internal controller logic and to an external accessory or a connector.

The diagnostics mode is divided into monitor mode and forced mode. In the monitor mode signals operate normally, but provide live monitoring of the signal behavior. In forced mode the connection between the controller internal logic and the external accessory is opened and the input and output signals can be forced to a desired state.

It is possible to diagnose digital signals for one device or one fieldbus at a time.

# Diagnostics Configuration

Diagnostics for a specific accessory or fieldbus is accessible through the Info option in the Virtual Station view for the accessory or fieldbus.

1. Tap Info and on the next screen tap Diagnostics.

2. Activate Monitor mode or Forced mode with the switch.

3. The statuses of input signals and output signals are available under the respective tabs.

It is only possible to access the diagnostics from one single user or function at a time. If the diagnostics is already in use an information message is shown on the screen.

# Normal Operations

In normal operations mode external input signals are passed to the internal controller logic and controller output signals are passed to an external target, without any intervention from the diagnostics module.

A | Controller internal state machine and logic functions
B | Digital output signal path
C | Digital input signal path
D | Diagnostics module

# Monitor Digital Signals

In the diagnostics mode all signals passed to and from the controller internal logic can be monitored. A signal tap is connected in the diagnostics module and the signal states are displayed on the web GUI or the controller GUI.

A | Controller internal state machine and logic functions
B | Digital output signal path
C | Digital input signal path
D | Diagnostics module
E | User interface
F | Output signal tap
G | Input signal tap

# Force Digital Signals

In the diagnostics mode all signals passed to and from the controller internal logic can be forced to a desired state. The signal lines are opened in the diagnostics module. From the user interface both input and output signals can be forced to steady states. The user interface is either the web GUI or the controller GUI.

While signals are forced, the controller operates normally. When leaving the diagnostics mode and the forced mode all signals are set to the current operating state of the controller. This may lead to a change-of-state for digital outputs, which can create unwanted actions.

A | Controller internal state machine and logic functions
B | Digital output signal path
C | Digital input signal path
D | Diagnostics module
E | User interface
F | Forced output signal insertion point
G | Forced input signal insertion point

# Configuring Fieldbus Window in a Virtual Station

The Fieldbus entry in the GUI shows the fieldbus mapping assigned to the controller.

To analyze the fieldbus configuration click on perform in the diagnostics field for the fieldbus mapping. Read more about the diagnostics tool in the Virtual station - Accessories section of this chapter.

To configure Fieldbus mappings, ToolsTalk 2 is required.

Virtual station - Fieldbus

# Working with the Configurations Tab

## Product Essentials Tutorials

https://www.youtube.com/watch?v=PY1WGo3YYIw

In this Section

- Tool Configuration
- Digital Signals
- Triggering Manual Mode
- Selector Configuration
- General Virtual Station
- Configuring QIF Accessories
- Configuration of the Scanner

# Tool Configuration

In Configurations >Tool configuration menu it is possible to configure the available accessory functions on the tool.

Different functions are available depending on the tool type.

## Configuring Accessory Functions on the Tool

1. Select Filter by tool type. Then, select the necessary tool.

2. Select Edit to configure the necessary functions.

   A configuration assigned to a virtual station cannot be deleted.

3. If available, configure Tool LEDs, Function button, Buzzer and Direction switch by selecting the related box.
   Each box shows a number which corresponds to the number of the specific function (for example, 1 corresponds to Tool LEDs, 2 to Function button, 3 to Buzzer, and 4 to Direction switch).

4. If available, configure the General settings, Start condition, and Accessory bus according to the customer needs.

## General settings

The general settings for the tool can be set in the General settings section.

Parameter | Description | Default value
--- | --- | ---
Inactivity timeout | Determines if the tool turns the power off after a set period of inactivity, or not. | On
<Inactivity timeout> | If Inactivity timeout is set to On, it sets the number of minutes before the shutdown. | 120 min
Front LED | Sets the behavior of the front LED (above tool trigger). Available only for wireless tools. When it is set to Off, the front LED does not lit when the trigger is pressed. | On
Duration after trigger released | Sets how long the front LED stays lit after the tool trigger is released (in seconds). For cable tools, the front LED stays lit for 10 seconds after the tools trigger is pressed. | 0 sec
Trace | Enables the graphical representation of the tightening. For multistep programs, trace is always on from Trigger pressed. For wireless tools, select Trigger pressed or Rundown complete for making the trace. | Off
TAG check | Enables TAG checking on the tool. The tool locks if the TAG supplied with the program is not equal to the one inserted into the STwrench smartHEAD. TAG check is available only for STwrench or when no tool is selected when validating the tool configuration. | Off
TAG selection | It is used for selecting a Tightening Program/Batch or Batch Sequence by using Batch Sequence/Source Tightening/Source Batch. The Tightening Program/Batch or Batch Sequence has a TAG number configured that corresponds to the TAG number of the TAG inserted into the STwrench smartHEAD. On the STwrench display, the operator is informed about which Tightening Program/Batch or Batch Sequence is selected for the TAG inserted into the STwrench smartHEAD. TAG selection is available only for STwrench or when no tool is selected when validating the tool configuration. | Off

Relevant Information

- TAG Check
- TAG Selection

In this Section

- Configuration of the Tool LEDs
- Configuration of the Function Button
- Configuration of the Buzzer
- Configuration of the Direction Switch
- Configuration of the Start Condition
- Configuration of the Accessory Bus

# Configuration of the Tool LEDs

The different LED indicators on the tool are configured to be controlled by one of the available output signals.

## Blue LED

The blue LED will be lit for a configurable duration of time, or configured to be lit until the following tightening. It is lit on the signal chosen by the configuration.

## Result indicator

The result indicator decides how and for how long the LEDs are lit on tightening results. A pre-configured pattern is selected from a shortcut menu. This pattern can be a combination of tightening results.

Result indicator signals
Signal | Description
--- | ---
Off | No LEDs are activated after the tightening, regardless of the result
Green | If a result indicator is selected, a green light is the default signal if the tightening is terminated correctly (OK).
Red:high:yellow:low | If the tightening is terminated incorrectly (NOK); a red LED indicates that the final value is too high, or a yellow LED indicates that the value is too low. Red and yellow can be lit simultaneously (e.g. in case of too high torque, and too low angle).
Red:high(prio):yellow:low | If the tightening is terminated incorrectly (NOK); a red LED indicates that the final value is too high, or a yellow LED indicates that the value is too low. Red and yellow cannot be lit simultaneously. Only red is lit in case of simultaneous high and low values.
Red:NOK:yellow:low | A red LED indicates that the tightening is terminated incorrectly (NOK). An additional yellow LED can indicate if the value is too low.
Red:NOK | A red LED indicates that the tightening is terminated incorrectly (NOK). No additional LEDs are shown.

## LED ring

The LED ring decides how the LEDs behave between the tightenings. The LED ring consists of three circles of LED lamps. One circle of red LEDs, one circle of yellow LEDs and one circle of green LEDs. Each circle can have a steady signal or a flashing signal. This provides a total of six different signals that can be connected to the LED ring.

- A LED is turned on only when no tightening is ongoing and when the controlling output signal is activated.

- A LED is turned off when the maximum time is exceeded. Only applicable if the signal type is an Event.

- A LED is turned off when the next tightening is started.

- A LED is turned off when the controlling output signal is deactivated. Only applicable if the signal type is an State.

# Configuration of the Function Button

Use the function button on the tool to control up to six of the available input signals. The button’s three possible condition states are combined with the two possible states of the direction switch.

Function button states | Direction switch states
--- | ---
Single push | CW
Single push | CCW
Double push | CW
Double push | CCW
Pressed | CW
Pressed | CCW

Two configurable parameters controls the push time.

Parameter | Description | Default value
--- | --- | ---
Push detection interval | For single push: the maximum push time (in milliseconds) between the button being pressed and the button being released. | 300 ms
Next push interval | For double push: the maximum time (in milliseconds) between the button being released after the first push, and the buttong being pressed again. | 300 ms

# Configuration of the Buzzer

The buzzer is configured by assigning a sound to a signal selected from a list of available signals.

The sound consists of a set of parameters described in the table. A signal with a sound can be prioritized between 1 and 10 where 1 is highest priority and 10 the lowest. By default a signal and sound has the priority 5. Up to 20 sounds can be assigned to signals.

Parameter | Description
--- | ---
Frequency | Exact frequency in Hz.
Time on | Time (in ms) that the buzzer makes a sound.
Time off | Time (in ms) that the buzzer is quiet.
Repetition | Number of times the buzzer repeats the on/off sequence.
Volume | The buzzer volume, in percentage of max volume.

# Configuration of the Direction Switch

The direction switch on the tool can be configured to trigger certain input signals when switched quickly (with a duration of 500 ms) from clockwise (CW) to counter clockwise (CCW) and back, or vice versa.

## Systems in Remote start

When the system uses remote start and the user wants to trigger a signal assigned to a direction switch in Tool configuration, one needs to assign the respective signal and use the signal 10029 - Select Loosening with a required duration of 500 ms to trigger it. For this to work, an extra configuration step in ToolsTalk is needed. Under Hardware configuration in ToolsTalk, a configuration must be set for the tool by clicking on the tool icon.

# Configuration of the Start Condition

The start conditions for a tool, such as start request, start source, trace, and TAG conditions for STwrench are configured here. The functions are described in the respective sections.

In this Section

- Start Request
- Start Source
- Trace Configuration
- TAG Check
- TAG Selection

# Start Request

Start request enables the requirement of having a persistent connection between the tool and controller for an STB tool. This to make sure that the tool is always up to date with tightening program or batch settings, and with other settings on the controller, when performing tightening.

When Start request is set to On the tool gets locked if the tool loose connection with the controller. This means that if the tool loses connection in the middle of a tightening or a batch sequence, the tool will finish the ongoing tightening and then stop. The tool will be locked until it has reestablished the connection.

Parameters available for the start request
Parameter | Description | Default value
--- | --- | ---
Start request | Lock the tool when the tool loose connection with the controller. On: The tool is locked from performing tightening if it loose connection with the controller.. Off: The tool can continue to perform tightening although it has lost connection with the controller. | On

# Start Source

Use the tool start source to set how to start the tool. The default value is Trigger only.

Start Source is available only for certain tool types.

Options for start source
Start source | Description
--- | ---
Trigger only | Press the tool trigger to start the tightening.
Trigger OR Push | Press the tool trigger or push the tool against the joint to start the tightening.
Trigger AND Push | Press the tool trigger and push the tool against the joint to start the tightening.
Push only | Push the tool against the joint to start the tightening.
Digital input | Have a signal using digital input to trigger the start of the tightening.
Safety trigger | Two triggers (as with trigger and push) activated within 500 ms from each other to start the tightening.

# Trace Configuration

Traces provide users with a graphical representation of the tightening. Traces can begin either from when the trigger is pressed or from after rundown complete.

Parameter | Description | Default value
--- | --- | ---
Trace | Enables the result to be viewed in graphic form. Off: No trace is made. Trigger pressed: The trace is drawn from when the tool trigger is pressed. Rundown complete: The trace is drawn from when Rundown complete is reached. | Off

The maximum number of trace points is 2000 (200 for STB tools). If the maximum number of trace points is exceeded, every other result will be erased (effectively halving the sampling rate). Tracing will continue as long as the tightening is active, and every time the maximum number of trace points is reached, half of the trace points will be erased to allow the tracing to continue. Tracing will stop when the final stage of the tightening has finished.

# TAG Check

TAG check feature enables TAG checking on the tool. When the TAG check is enabled both on the Power Focus 6000 and the STwrench, the tool locks if the TAG supplied with the program is not equal to the one inserted into the STwrench smartHEAD.

The TAG number is specified differently, depending on the work task.

In case of Generic Tightening Strategies, the TAG number is specified in the Tightening Program.

In case of Multistep Tightening Strategy, the TAG number depends on what has been selected in Sources/Batch Sequence menu.

- If running Source Tightening (Sources > Tightening > Source Tightening > Selector mode - Confirm), the TAG number is specified in the Socket box.

- If running Batch Sequence (Batch sequence > Sequence library > Sequence > Batch configuration - Edit), the TAG number is the Identifier Number.

- If running Source Batch (Sources > Batch sequence > Source Batch), the TAG number is specified in the Batch Sequence as per above section.

In case of Batch Sequence and Source Batch, set Free order - in the Batch Sequence - to No.

TAG check is available only for STwrench.

TAG check options | Description
--- | ---
Off | The tool does not lock, regardless of the inserted TAG.
On | The tool is locked as long as the TAG number is not equal to the TAG number specified in the tightening strategy configuration.

# TAG Selection

TAG selection feature is used for selecting a Tightening Program/Batch or Batch Sequence that has a TAG number configured that corresponds to the TAG number of the TAG inserted into the STwrench smartHEAD.

TAG selection is available only for STwrench.

TAG selection options | Description
--- | ---
Off | The STwrench does not signal the controller to select Tightening Program/Batch or Batch Sequence.
On | Select the Tightening Program/Batch or Batch Sequence according to the TAG number configured in the Batch Sequence/Source Tightening/Source Batch.

# Configuration of the Accessory Bus

Tool accessories are connected to the tool through the accessory bus. The tool accessories are configured separately for each tool configuration on the controller.

Accessory bus configurations
Type | Description
--- | ---
ST selector | A small display and buttons used to select tasks or programs according to the configuration.
TLS tag | Tool Location System tag used to provide output signaling to the operator.
EHMI | A small display and buttons used to select tasks or programs according to the configuration.

In this Section

- ST Selector
- TLS Tag
- EHMI

# ST Selector

The ST selector is a tool accessory. It is installed on the tool and connected to the tool accessory bus. It has a small display, two input buttons and output LEDs.

## Display

The display shows one information at a time and has four different pages that can be configured to display different preset items on every page.

Parameter | Description
--- | ---
Page 1 | Select the mesage to be displayed from the list:. Final torque Final angle Batch count Remaining batch Generic IO 1 Generic IO 2 Generic IO 3 Generic IO 4 Generic IO 5 Generic IO 6 Generic IO 7 Generic IO 8 Generic IO 9 Generic IO 10 Selected tightening program Selected batch sequence id Target torque Target/Final torque
Page 2
Page 3
page 4

## Switch time

Parameter | Description
--- | ---
Switch time | Select the time to display one message before the next message is displayed.

## Buttons

The two buttons can be configured to act upon the displayed information and used to step through listed items.

Parameter | Description
--- | ---
Left button | Select one action from the shortcut menu.
Right button | Select one action from the shortcut menu.

## Status LEDs

The status LEDs can be activated or deactivated.

Parameter | Description
--- | ---
Enable result LEDs | Select the desired On or Off radio button.
Enable extra LEDs | Select the desired On or Off radio button.

The result LEDs are red, green and yellow, and show the same information as the main tool LEDs.

The two extra LEDs can show Batch OK and Batch sequence OK. Both these LEDs are turned off at the next tightening.

# TLS Tag

The Tool Location System (TLS) tag, is a tool accessory. The TLS tag is installed on the tool and connected to the tool accessory bus. The TLS tag is part of the Ubisense positioning system and is handled independently from the controller. In addition to the positioning, the TLS tag can be used to provide information to the operator. Selected output signals can generate different LED light combinations.

Up to 10 different output signals can be mapped to a light priority.

TLS tag configuration parameters
Parameter | Description
--- | ---
Signal | Select a signal to trigger the LED light from a shortcut menu. For a signal of the type Event, select the duration of the signal.
Color | Select a color for the LED.
Priority | 10 priority levels are available for the sounds where one (1) is the highest priority level. Default priority level is five (5).

For two simultaneous signals, the signal with the highest priority wins. When two signals with the same priority triggers the LED, the first arriving signal wins.

An output signal can be of type Event or of type State.

A state signal is active as long as the state is active.

An event signal is active during a configurable time.

# EHMI

The EHMI is a tool accessory. It is installed on the tool and connected to the tool accessory bus. It has a graphical display, three function buttons, and optionally a scanner. The display is a subset of the controller GUI with the possibility to select tightening programs, batch sequences, and to view results from tightenings. The interaction with the controller is through function buttons.

In the EHMI configuration it is possible to decide if the function buttons are On or Off.

EHMI buttons
Parameter | Description
--- | ---
Enable function buttons | On = The buttons have full functionality to configure settings within the visible menus. Off = The function buttons can only be used to acknowledge a necessary dialog on the EHMI.

# Digital Signals

# Input Signals

Input signals are system commands that are carried out by using for example buttons or switches on an accessory, either a tool accessory or a QIF accessory, or by connecting the signal to an I/O input plug.

The input signal Lock tool must not be configured for more than one accessory for each virtual station.

# Output Signals

Output signals are states or events of the system. They can be linked to either a tool accessory or a QIF accessory.

# Triggering Manual Mode

Manual mode can be activated by a switch or an external system. For example (indicated below), a button on an operator panel can be configured to activate manual mode.

1. Go to the Configurations menu and choose Operator panel in the left navigation.

2. If no configuration for an operator panel exists, click the plus icon at the top right of the work space, otherwise continue to the next step.

3. In the configuration you want to alter, click Edit.

4. In the Operator panel configuration window, click on the position [A,B,C,D,E,F,G,I] to configure.

5. In the Position configuration window, click on the Component list. In the list, click One way key switch.

6. Click on the Turn signal list. In the list, choose Manual mode (use the arrow buttons to navigate within the list if necessary).

7. Close the Position configuration window.

If the user needs to be notified that Manual mode has been entered or left, then events 4070 and 4071 have to be configured, respectively.

Relevant Information

- Configuration of Events

# Selector Configuration

# Digital Input Information

Information about the connected digital inputs can be found by tapping Tightening and then Digital inputs on the Sources menu.

# Socket Selector Configuration

Socket selector is a socket tray with LEDs that can be used to guide the user through, for example, a Batch sequence. When using more than one tightening program, it is convenient to use a selector. When a socket is lifted, the corresponding tightening program is selected. Several socket selectors can be connected to each virtual station.

Information about the connected socket selectors can be found by tapping Tightening and then Socket selector on the Sources menu.

In this Section

- Configuring the Socket Selector
- Connecting a Socket Selector to a Virtual Station

# Configuring the Socket Selector

1. Go to Configurations, then Socket selector and click on the plus at the top right to create a new configuration

2. Give the configuration a name

3. Click on Edit

4. Click Add or Remove for the correct number of socket slots, then select all the slots that need to be active (indicated in blue)

# Connecting a Socket Selector to a Virtual Station

1. On the Virtual station menu, go to the virtual station to use and then go to Accessories and tap Choose accessories.

2. Under Accessories, click Choose accessories, then navigate to the Socket selector tab.

3. In the Configuration column (left), select a configuration you want to use with the socket selector (see Configuring the Socket Selector)

4. In the Connected accessories column (right), select the socket selector you want to use.

# Setting up a Socket Selector via I/o Bus

1. Connect the socket selector to the controller's I/O bus.

2. Under Virtual station > Accessories > Choose accessories > Socket selector, check that the selector shows up in the Connected accessories column (right)

# Setting up a Selector 6 via Ethernet Cable/Wireless

Selector 6 main overview

Selector front view

A | Holder for socket or bit
B | Indicator LEDs for the position
C | Sticker area
D | Mounting holes in each corner
E | Service port
F | Battery status LED (only available on wireless versions)
G | WLAN status LED (available on some selectors)
H | Battery (only available on wireless versions)
I | Mobility module (only available on wireless versions)

Selector 6 connection overview

Selector bottom view

A | Connector cover
B | External DC power in; Kycon (DC DIN) connector
C | Ethernet in, upstream connection; M12 D-coded female connector
D | Selector back side
E | Digital input and output connector
F | Ethernet out, downstream connection; M12 D-coded female connector
G | Battery

Selector 6 service port overview

Service interface

A | RJ45 Service port
B | RBU slot
C | Function button

General set-up

1. On the controller, go to Settings > Network and under Factory Ethernet port, check the IP address (only required when setting up via wireless connection).

2. Open the service port cover on the selector. The cover is secured by a 2 mm allen screw.

3. Connect an ethernet cable between a PC and the RJ-45 connector in the service interface.

4. Make sure the selector powered, either by PoE, by external power supply or by battery.

5. Open a web browser window in the PC.

6. Type the web address 169.251.1.1 and press the Enter key. The web server in the selector will respond and show the selector web interface.

7. Select Settings in the left navigation (this is selected by default). The Settings workspace shows the configuration menus and is divided into five different settings: Basic settings, Service port, Ethernet in, WLAN, and the POWER FOCUS 6000.

8. In the Ethernet in section, select External mode On or Off for the desired LED control source.

9. The next steps in the set-up depend on how the socket selector will be connected to the controller (Ethernet cable directly to the controller (default), Ethernet cable to factory network, or wireless to factory network). See the instructions below for your set-up.

Setting up socket selector - Ethernet wired to controller (default)

1. Ethernet ports (RJ45) for connecting devices and daisy-chaining controllers are only available in newer PF6 models. In order to connect Selector 6 via Ethernet cable to older controller models, an adapter cable should be used to connect the Ethernet cable to the controllers COM PORT.

2. In the Ethernet In section, select PF6000 (default) in the Connected to drop-down.

3. Click the Save button in top right of the workspace.

4. Remove the ethernet cable from the service port.

5. Close the service port with the lid and secure it with the allen screw.

   The socket selector shows up in the Connected accessories list (Virtual station > Accessories > Choose accessories > Socket selector)

Setting up Selector - wired to factory network

1. In the Ethernet In section, select Factory net from the Connected to drop-down

2. Select DHCP On or Off for dynamic or static IP address configuration. If a static IP address is required, in the IP address field, enter the IP address for the socket selector.

3. In the PF6000 section, enter the controller IP address (see above) for the controller the selector will be connected to.

4. Click the Save button in top right of the workspace.

5. Remove the ethernet cable from the service port.

6. Close the service port with the lid and secure it with the allen screw.

   The socket selector shows up in the Connected accessories list (Virtual station > Accessories > Choose accessories > Socket selector)

Setting up socket selector - wireless to factory network

1. In the Ethernet In section, select Factory net from the Connected to drop-down

2. In the WLAN section, fill out the following parameters:

   - Enable: set radio button to YES

   - SSID: fill out the SSID name for the socket selector

   - Password: fill out the password for the wireless network to be connected to

   - Encryption type: choose the correct encryption type for the wireless network (WPA-PSK, or WPA2-PSK, EAP-TLS)

3. In the PF6000 section, enter the controller IP address (see above) for the controller the selector will be connected to.

4. Click the Save button in top right of the workspace.

5. Remove the ethernet cable from the service port.

6. Close the service port with the lid and secure it with the allen screw.

   The socket selector shows up in the Connected accessories list (Virtual station > Accessories > Choose accessories > Socket selector)

# General Virtual Station

In General Virtual Station, different specific result reporting and tightening settings can be saved. Different filters can be created, filtering out specific results. In the tightening settings, characteristics like the tool unlocking behavior can be set. These configurations can then be assigned to virtual stations.

## Adding and editing a configuration

1. In the Configurations menu, click on the General Virtual Station tab, and click on the plus sign in the top right corner.

2. Give the new configuration a name and click on Edit.

3. In the Result filter for reporting window, set the switch to On for those parameters you want to include in the results. By default, all parameters are set to On.

   Turning on a result filter prevents the respective result from being sent, but the result is still shown on the controller.

   The following parameters can be set in the Result filter for reporting section:

   - Loosening

   - Batch increment

   - Batch decrement

   - Reset batch

   - Bypass Tightening Program

   - Abort sequence

   - Reset batch sequence

4. In the Tightening Settings window, set a value for any of the parameters listed. By default, all parameters are set to Off.

   The following parameters can be set in the Tightening Settings section:

   - Unlock tool on loosening - makes sure that the tool is locked after a NOK tightening.

   - Disable loosening - makes sure that an operator is not loosening a bolt that their processes do not allow to be loosened.

   - Disable tightening - makes sure that an operator is not tightening a bolt that their processes do not allow to be tightened.

Unlock tool on loosening options
Unlock tool on loosening | Description
--- | ---
Off | A disabled tool will remain disabled regardless of the loosening status.
On OK | A disabled tool will be unlocked after an OK loosening has been performed.
Always | A disabled tool will be unlocked as soon as a loosening has been performed, regardless of the loosening status.

Disable loosening options
Disable loosening | Description
--- | ---
Off | Disable loosening is Off. It is always possible to loosen a bolt.
On OK tightening | Disable loosening for an OK tightening. An operator cannot loosen a bolt that was terminated with tightening OK.
On NOK tightening | Disable loosening for an NOK tightening. An operator cannot loosen a bolt that was terminated with tightening NOK.
Always | Disable loosening is always ON. An operator can never loosen a bolt.

Disable tightening options
Disable tightening | Description
--- | ---
Off | Disable tightening is Off. An operator can always tighten a bolt.
On OK tightening | Disable tightening after an OK tightening, An operator cannot tighten another bolt if the current tightening was terminated with OK.
On NOK tightening | Disable tightening after a NOK tightening. An operator cannot tighten another bolt if the current tightening was terminated with NOK.
After every tightening | Disable tightening is activated after every tightening. An operator cannot tighten another bolt until the current tightening is terminated.

## Allowing a disabled tool to unlock after loosening

- In the general virtual station configuration assigned to the virtual station to which the tool is connected, set the Unlock tool on loosening to On OK or Always.

In order to enable the setting above, the following conditions need to be met:

- The Disable loosening parameter cannot be set to Off or Always.

- The Disable loosening parameter cannot be set to the same value as the Disable tightening.

- The tightening program used must have loosening enabled.

When the tool is locked for either tightening or loosening due to a disable state, it can be unlocked by any of the following input signals:

- Master Unlock - 10005

- Unlock Tool on Disable - 10059

Unlocking a disabled tool through the input signals specified is not possible if Lock tool on loosening is set to Always.

## Assigning a configuration to a virtual station

Each virtual station can have its own configuration associated with it, or multiple virtual stations can share the same configuration. For a configuration to come into effect it needs to be assigned to a virtual station.

1. Go to the Virtual Station menu and select the Virtual Station you want to assign the configuration to.

2. Under General, the first General Virtual Station configuration will be chosen by default. Click on the configuration name.

3. In the pop-up window, select the desired configuration from the list. The pop-up window will be closed upon selection.

In this Section

- Configuring Result Presentation Settings

# Configuring Result Presentation Settings

The Result Presentation Settings window allows a user to show the final torque without the PrT compensation value included, and PrT compensation value on the Live results.

## Configure the Result Presentation Settings Window

1. On the Home view, select the Configurations tab. Then, on the left, select General Virtual Station.

2. In the wanted Configuration window, select Edit.
   The Edit Configuration screen appears.

3. In the Result Presentation Settings window, set the relevant switches to ON or OFF depending on the wanted results.

   If the Show PrT Compensation Value on Live Result switch is set to ON, the Live Results window displays the PrT compensation value.

   If the Show Final Torque with PrT Compensation switch is set to ON, the Live Results window displays the final torque with the PrT compensation included.

   Setting the switches in the Results Presentations Settings window to either ON or OFF has no impact unless:

   - The multistep program has a tightening step including a Prevailing Torque step monitor with the Compensation switch set to ON.

## Result Presentation Settings

Here are the different configuration options in the Results Presentations Settings window.

Show PrT Compensation Value on Live Result: ON Show Final Torque with PrT Compensation: ON | Show PrT Compensation Value on Live Result: ON Show Final Torque with PrT Compensation: OFF | Show PrT Compensation Value on Live Result: OFF Show Final Torque with PrT Compensation: ON | Show PrT Compensation Value on Live Result: OFF Show Final Torque with PrT Compensation: OFF
--- | --- | --- | ---
Point and click at items on image to see if there is more information: | Point and click at items on image to see if there is more information: | Point and click at items on image to see if there is more information: | Point and click at items on image to see if there is more information:

In this Section

- Show Final Torque with PrT Compensation: ON / Show PrT Compensation Value on Live Result: ON
- Show Final Torque with PrT Compensation: OFF / Show PrT Compensation Value on Live Result: ON
- Show Final Torque with PrT Compensation: OFF / Show PrT Compensation Value on Live Result: OFF
- Show Final Torque with PrT Compensation: ON / Show PrT Compensation Value on Live Result: OFF

# Show Final Torque with PrT Compensation: ON / Show PrT Compensation Value on Live Result: ON

## Show Final Torque with PrT Compensation: ON

The Live Result window shows the Final Torque with the PrT compensation value included.

If the eHMI and ST Selector are on and configured, they show the Final Torque with the PrT compensation value included.

## Show PrT Compensation Value on Live Result: ON

The Live Result window shows the PrT compensation value with the related compensation icon ().

If there are several compensation values, the compensation value applied to the latest available step appears.

Configuring the Show Final Torque with PrT Compensation and Show PrT Compensation Value on Live Result switches does not impact:

- The final torque values sent to ToolsNet and ToolsTalk: the final torque values with PrT compensation are always sent to ToolsNet and ToolsTalk.

- The final torque value displayed with the historical results.

- The traces based on live and historical results.

- The values in Open Protocol messages.

- The signals.

- The protocol adapters.

Relevant Information

- Stored Results

# Show Final Torque with PrT Compensation: OFF / Show PrT Compensation Value on Live Result: ON

## Show Final Torque with PrT Compensation: OFF

The Live Result window shows the Final Torque without the PrT compensation value included. Since the Final Torque does not include the PrT compensation value, it shows in italic.

## Show PrT Compensation Value on Live Result: ON

The Live Result window shows the PrT compensation value with the related compensation icon ().

If there are several compensation values, the compensation value applied to the latest available step appears.

Configuring the Show Final Torque with PrT Compensation and Show PrT Compensation Value on Live Result switches does not impact:

- The final torque values sent to ToolsNet and ToolsTalk: the final torque values with PrT compensation are always sent to ToolsNet and ToolsTalk.

- The final torque value displayed with the historical results.

- The traces based on live and historical results.

- The values in Open Protocol messages.

- The signals.

- The protocol adapters.

Relevant Information

- Stored Results

# Show Final Torque with PrT Compensation: OFF / Show PrT Compensation Value on Live Result: OFF

## Show Final Torque with PrT Compensation: OFF

The Live Result window shows the Final Torque without the PrT compensation value included. Since the Final Torque does not include the PrT compensation value, it shows in italic.

## Show PrT Compensation Value on Live Result: OFF

The Live Result window does not display the PrT compensation value and the related compensation icon ().

Configuring the Show Final Torque with PrT Compensation and Show PrT Compensation Value on Live Result switches does not impact:

- The final torque values sent to ToolsNet and ToolsTalk: the final torque values with PrT compensation are always sent to ToolsNet and ToolsTalk.

- The final torque value displayed with the historical results.

- The traces based on live and historical results.

- The values in Open Protocol messages.

- The signals.

- The protocol adapters.

Relevant Information

- Stored Results

# Show Final Torque with PrT Compensation: ON / Show PrT Compensation Value on Live Result: OFF

## Show Final Torque with PrT Compensation: ON

The Live Result window shows the Final Torque with the PrT compensation value included.

If the eHMI and ST Selector are on and configured, they show the Final Torque with the PrT compensation value included.

## Show PrT Compensation Value on Live Result: OFF

The Live Result window does not display the PrT compensation value and the related compensation icon ().

Configuring the Show Final Torque with PrT Compensation and Show PrT Compensation Value on Live Result switches does not impact:

- The final torque values sent to ToolsNet and ToolsTalk: the final torque values with PrT compensation are always sent to ToolsNet and ToolsTalk.

- The final torque value displayed with the historical results.

- The traces based on live and historical results.

- The values in Open Protocol messages.

- The signals.

- The protocol adapters.

Relevant Information

- Stored Results

# Configuring QIF Accessories

A total of 15 QIF accessories can be connected to one controller. It is possible to add several scanners to each controller.

All QIF accessories connected to the controller can be connected to the same virtual station. One of each type of accessory and multiple socket selectors.

The functions of the QIF accessory can be connected to various input and output signals.

In this Section

- Connecting QIF Accessories to a Virtual Station
- Disconnecting QIF Accessories From a Virtual Station

# Connecting QIF Accessories to a Virtual Station

To connect a QIF accessory to a virtual station:

To connect a QIF accessory to a virtual station:

1. Configure the accessory in the Configurations menu.

2. Connect the accessory to the controller I/O bus.

3. In the Virtual station menu, choose the virtual station and then tap Choose accessories under Accessories.

4. On the appropriate accessory tab, tap both the accessory and the configuration to connect them.

   1. Connected accessories show up in All connections.

# Disconnecting QIF Accessories From a Virtual Station

To disconnect a QIF accessory or a scanner from a virtual station:

1. On the Virtual station menu, choose the virtual station and then tap Choose accessories under Accessories.

2. Under All connections, tap the disconnect icon on the right to disconnect.

# Configuration of the Scanner

In this menu, scanner configurations can be added. Scanners can be configured to either have scanned strings handled by the controller, or passed through to a an external system. When the scanned string is passed through, the controller does not select a task based on the string, but instead passes the string to an external device via an output signal.

## Adding a scanner and enabling pass through

1. Go to Configurations > Scanner, and select the Plus sign at the top right.

2. Give the scanner configuration a name.

3. To enable pass through, select Edit, and set Pass Through Mode to On.

Relevant Information

- Connecting QIF Accessories to a Virtual Station

In this Section

- Scanner Configuration

# Scanner Configuration

A scanner is used to read a barcode string or a QR code containing information to choose the appropriate batch sequence.

The scanner is configured in the Sources tab.

The scanner reads the characters you specify and puts them together to form a string of text. This text string is matched to the pre-defined strings you have specified in the controller, and if they match, the batch sequence linked to your pre-defined string is selected.

Barcode strings of a length of up to 1024 characters can be read and they can contain characters in the positions 32-126 in the ASCII table. If the barcode contains a string longer than 1024 characters, the remaining part of the string, from position 1025 and forward, is discarded.

In this Section

- Configuring the Scanner
- Valid Scanners

# Configuring the Scanner

The scanner itself must be set up using a US keyboard, and the scanner will emit a carriage return character to terminate the barcode string.

# Valid Scanners

For a list of scanners verified for use with the POWER FOCUS 6000 controller, contact your local Atlas Copco sales representative.

# Working with the Controller Tab

The system administration tasks for the POWER FOCUS 6000 controller are handled in the Controller menu. The menu is accessed through the controller GUI, the web GUI, or the Tools Talk 2 GUI.

In this Section

- Intelligent Application Module
- Software
- Hardware
- Export/Import
- StepSync

# Intelligent Application Module

The Intelligent Application module (IAM) is a non volatile storage that is located in the controller. The storage module contains all the controller programs, configurations and results. Certain modules may also include additional loaded feature items.

For a complete list of available IAMs and their capabilities, please consult an Atlas Copco sales representative.

IAM information

# Software

The version number of two versions of software available in the POWER FOCUS 6000 controller are under the Software tab.

Installing a second version of the controller software is useful when performing upgrades on multiple controllers. When production is ready for switching to the upgraded software, activation of the new software version is done locally on the controller GUI, from a remote computer with the web GUI, or with Tools Talk.

A new software distribution can be installed either by connecting a USB flash drive containing the software to the controller’s USB port, or by using the web GUI.

The software update option is visible only when accessing the controller GUI from a PC. When a mass storage device with a valid software version is inserted in the USB port a prompt to update the software will appear.

The software update file must not be unzipped and must be stored in a folder named PFImages in the root directory on the USB flash drive.

An unexpected failure during software upgrade might lead to loss of data.
Before upgrading software versions, it is recommended to take a backup of the controller configuration by exporting “All controller information”.

Relevant Information

- Exporting "All Controller Information"

In this Section

- Updating Controller Software through USB
- Updating Controller Software through Web GUI
- Activating the Software on the Controller

# Updating Controller Software through USB

1. Connect the USB flash drive to the controller: the installation wizard starts automatically.

   If several software versions are available on the USB flash drive, a list with the different software upgrade files is displayed.

2. Select the software upgrade file to install and follow the instructions to finish the installation.

The USB flash drive needs to have a partition available and be formatted to work for Linux. Possible formats are for example FAT or NTFS.

Manually restart all Sync Member controllers after upgrading to a new software version or downgrading from a new software version.

Relevant Information

- StepSync

# Updating Controller Software through Web GUI

1. On the Controller menu, go to Software, and select Software update. Then, click Browse.

2. Browse and choose the .zip file with the software and follow the instructions to complete the installation.

Manually restart all Sync Member controllers after upgrading to a new software version or downgrading from a new software version.

Relevant Information

- StepSync

# Activating the Software on the Controller

The controller can store two installed software versions. By using the Software activation, it is possible to choose which software version to use. Software activation can be performed either locally from the controller GUI or remotely from the web GUI.

The activation process requires a restart of the controller.

1. On the Controller menu, go to Software.

2. Swipe the Software activation switch to stored and follow the instructions.

# Hardware

The Hardware tab contains Controller information, such as model designation and serial number, Health, Touch screen calibration, and information about the various electronics boards in the controller.

In this Section

- Health

# Health

The Health view contains information about battery status and controller temperature.

## Battery status

Controller > Hardware > Health

The POWER FOCUS 6000 battery, located inside the controller's front panel serves as backup power for some system elements, such as the internal clock. The status of the battery is updated once a day, as well as at controller restart. When the battery is close to being completely depleted, a warning (3011) will be displayed. The battery shall be replaced as soon as possible when the warning pops up.

## Controller temperature

Controller > Hardware > Health

Controller temperature is monitored continuously by the POWER FOCUS 6000. Supported temperature units are degrees Celsius (°C) and degrees Fahrenheit (°F), with Celsius being the default unit. It is possible to switch between the two units without requiring a restart of the controller. When the controller temperature exceeds max temperature, the drive stage is disabled and an alert (3010) is shown. The drive stage is once again enabled when the controller temperature drops below the temperature limit.

From the display or through the web GUI, users can access the latest controller temperature measured together with the timestamp when the measurement was taken.

# Export/Import

The Export/Import Tab supports the user to make one of the following operations: Export, Import, and Automated backup.

The Export window supports the user to export controller configurations, settings, results, and events. In addition, it is possible to export tool logs, which can be shared with Atlas Copco Service personnel to troubleshoot problems with the tool(s).

The Import window supports the user to import controller configurations and settings.

It is only possible to have one active Export or Import at the time. Any attempt to start a new Export/Import while there is an ongoing Export/Import is rejected.

The Automated backup window supports the user to generate automatically a backup file.

It is possible to export/import data through one of the following devices:

- USB flash drive (formatted and with a partition to work for Linux: possible formats are, for example, FAT or NTFS)

- Web GUI

- ToolsTalk 2

During the Export/Import process a progress bar informs the user that an export/import is ongoing. The time to perform an export/import is depending on the numbers of results, events, and log files.

## Export/Import Between Controllers

Controllers may have different IAM types that could have different capabilities.
A controller can export all the configurations that are applicable for the current type of IAM module.

A controller cannot import a file exported from a different type of IAM module. This is applicable also when using ToolsTalk 2.

## Product Essentials Tutorials

https://www.youtube.com/watch?v=0axnEB95gkQ

Relevant Information

- Automated Backup
- Exporting "All Controller Information"
- Exporting "Logs from Connected Tools"
- Exporting "Results"
- Exporting "Settings and Configurations"
- Importing Controller Configurations and Settings

In this Section

- Exporting "All Controller Information"
- Exporting "Settings and Configurations"
- Exporting "Logs from Connected Tools"
- Exporting "Results"
- Importing Controller Configurations and Settings
- Automated Backup

# Exporting "All Controller Information"

It is possible to export controller configuration, settings, results, and events for further processing. Part of the export is done both from the cable tool, as well as connected wireless tools.

All data included in the export is stored in a file "PFExport_<IAM name>_<datetime (lowest value displayed for time is seconds)>.tar.gz", which includes the following files and directories:

- "PFExport_<datetime>_Results.csv" – All available results

  The results are exported in a CSV formatted text file. The latest performed result is the first in the CSV file.

  It is possible to export the following result information for tightenings and loosenings:

Result Information | Power Focus 6000 - Tightening Programs | Power Focus 6000 - Multistep Programs | StepSync
--- | --- | --- | ---
Identity number | - | - | X
Type of tightening | X | X | X
Virtual Station name | X | X | X
VIN (Identifier String) | X | X | X
Date and Time | X | X | X
Unique tool identifier | X | X | -
Batch Sequence Name | X | X | -
Batch Sequence Counter | X | X | -
Batch Count | X | X | -
Bolt name | - | - | X
Total status | - | - | X
Total status info | - | - | X
Status | X | X | X
Status info | X | X | X
Mode Name | - | - | X
Tightening program/Multistep Name | X | X | X
Stopping error | - | X | X
Errors | - | X | X
Failing Step | - | X | X
Channel | - | - | X
Target Torque (Nm) | X | X | -
Final Torque (Nm) | X | X | X
Target Angle (deg) | X | X | -
Start Final Angle (Nm) | X | X | X
Final Angle (deg) | X | X | X
Rundown Angle (deg) | X | - | -
Residual torque correlation factor | X | X | -
Elapsed time (s) | - | X | X
Angle low limit (deg) | X | X | X
Angle high limit (deg) | X | X | X
Torque low limit (Nm) | X | X | X
Torque high limit (Nm) | X | X | X
Number of pulses | X | - | -
Current at shutoff (A) | X | X | X
TrueAngle compensation (deg) | X | X | -
Time to rundown complete (ms) | X | - | -
Time to final torque (ms) | X | - | -
Target Text | X | X | -
Step Data | - | X | X
Selftap Torque | X | X | X
Prevailing Torque | X | X | X
Rundown Angle Trigger | X | X | X

The field delimiter and number format depends on the language settings:

Language | Date/time | Field delimiter | Number format
--- | --- | --- | ---
English (en_US) | MM/dd/yyyy hh:mm:ss | , | 123.456
Czech (cs) | dd.MM.yyyy hh:mm:ss | ; | 123,456
German (de_DE) | dd.MM.yyyy hh:mm:ss | ; | 123,456
Spanish (es_ES) | dd/MM/yyyy hh:mm:ss | ; | 123,456
French (fr_FR) | dd/MM/yyyy hh:mm:ss | ; | 123,456
Korean (ko_KR) | yyyy-MM-dd hh:mm:ss | , | 123.456
Italian (it_IT) | dd/MM/yyyy hh:mm:ss | ; | 123,456
Japanese (ja_JP) | yyyy/MM/dd hh:mm:ss | , | 123.456
Portugese (pt_BR) | Dd/MM/yyyy hh:mm:ss | ; | 123,456
Russian (ru_RU) | dd.MM.yyyy hh:mm:ss | ; | 123,456
Swedish (sv_SE) | yyyy-MM-dd hh:mm:ss | ; | 123,456
Chinese (zh_CN) | yyyy/MM/dd hh:mm:ss | , | 123.456

For PF6000-StepSync, all available results are in the file named “PFExport_<datetime>_Results.csv.zip”.

- "PFExport_<datetime>_Events.csv" - All available events

  The following event information are exported in a CSV formatted text file:

  - Severity

  - Date

  - Time

  - Code

  - Description

  - Virtual Station that triggered the event (only exported for PF6000-Handheld)

  - Carrier (only exported for PF6000-StepSync)

  - Channel (only exported for PF6000-StepSync)

- "/settings" - Settings and configurations (used by Import)

For fieldbus exported settings and configurations:

- General Fieldbus configuration (including IP address)

- Fieldbus configuration

- Fieldbus mapping (Virtual station mapping to ProcessDataFrame)

- "jsonConfigurations.zip" - Multistep Tightening and Loosening programs are exported as .json files (to be used with MID2500)

- "atlas_sys_d.zip" - Logfiles from Drive application

- "atlas_sys_i.zip" - Logfiles from IT application

- "atlas_protocol_log.zip" – Logfiles from external protocol adapters

- “ExportInfo.txt” - Text document containing information about the IAM and Controller

- "atlas_plc.zip" - PLC configuration

- “licenseInformation.zip” – License Information and System Capabilities

## How to Export "All Controller Information"

1. On the Home view, select the Controller Tab. Then, on the left side, select the Export/Import Tab .

2. In the Export window, open the drop-down menu and select All controller information.

3. In the Export window, select Export.
   At the end of the exporting process, an exporting pop-up window confirms that the export is done.
   A PF/IXBExport_<IAM name>_<datetime>.tar.gz file is automatically downloaded.

# Exporting "Settings and Configurations"

It is possible to export only controller configurations and settings.

The exported data are stored in a compressed file identified with the IAM name and exported date and time.
The data in the file include all configurations and settings of the controller, so that the export file can be imported and setup another controller with the same or newer release version.
The exported data include information about the IAM and Controller, and also pre-formatted Multistep Tightening and Loosening programs to be used with the MID2500 solution.

## How to Export "Settings and Configurations"

1. On the Home view, select the Controller Tab. Then, on the left side, select the Export/Import Tab .

2. In the Export window, open the drop-down menu and select Settings and configurations.

3. In the Export window, select Export.
   At the end of the exporting process, an exporting pop-up window confirms that the export is done.
   A PFExport_<IAM name>_<datetime>.tar.gz file is automatically downloaded.

# Exporting "Logs from Connected Tools"

The export of tool logs enables a service technician to share the tool log data with Atlas Copco Service personnel to troubleshoot problems with the tool(s).

It is possible to export tool logs from the following tools: STB, SRB and TBP/TBP-S.

To export the tool logs, the tool has to be connected to the controller. It is not necessary for the tool to be assigned to a Virtual Station.

All data included in the tool log export is stored in a file "PFExport_<IAM name>_<datetime>.tar.gz", which includes the following files and directories:

- "atlas_tool_i.zip" – All available results

  For each connected tool an individual files is created. The file format for tool log files is "tool-<tool type>-<tool serial number>.log"

- "ExportInfo.txt" - Text document containing information about the IAM, Controller and connected tools

## How to Export "Logs from Connected Tools"

1. On the Home view, select the Controller Tab. Then, on the left side, select the Export/Import Tab .

2. In the Export window, open the drop-down menu and select Logs from connected tools.

3. In the Export window, select Export.
   At the end of the exporting process, an exporting pop-up window confirms that the export is done.
   A PFExport_<IAM name>_<datetime>.tar.gz file is automatically downloaded.

# Exporting "Results"

It is possible to export only tightening results from the controller.

## How to Export "Results"

1. On the Home view, select the Controller Tab. Then, on the left side, select the Export/Import Tab .

2. In the Export window, open the drop-down menu and select Results.

3. In the Export window, select Export.
   At the end of the exporting process, an exporting pop-up window confirms that the export is done.
   In case of a multi-spindle systems (fixtured), the exported file automatically downloaded is in a .zip format, otherwise it is in a .csv format.

# Importing Controller Configurations and Settings

When users import controller configuration and settings, existing configurations and settings are replaced by the imported controller configuration and settings.

The following configurations are not imported or deselected:

- Controller Network settings are not imported

- Results and Events are not imported

- License Assignment is not imported

- Assigned task in Virtual Station/s is deselected

- "jsonConfigurations.zip" (Multistep Tightening and Loosening programs) is not imported

- "licenseInformation.zip" (License Information and System Capabilities) is not imported

## How to Import Controller Configurations and Settings

1. On the Home view, select the Controller Tab. Then, on the left side, select the Export/Import Tab .

2. In the Import window, select Import.

   An Information pop-up window confirms that all setting for tightening program, batch, accessories, and controller will be replaced with the settings of the imported file.
   However, settings for network, PIN, results, and events will not be imported.

   Select Continue.

3. In the Import pop-up window, select Choose File. Then, select the file to be imported on the controller.

   At the end of the importing process, the controller will restart automatically.

   If the importing process is interrupted before it has started, or the file disappears, the user is informed and the controller has to be restarted (to assure it is in a valid state).
   If the importing process is interrupted, but the file is not corrupt and exist, the import can be completed.

# Automated Backup

The Automated Backup window enables or disables sFTP export.

By default, Enable sFTP export switch is set to OFF.
When turning ON Enable sFTP export switch, an export file is created 10 minutes after the last configuration change.
If Enable sFTP export switch is set to ON on system startup, an export file is automatically created within 2-3 minutes. The export file is created within 2-3 minutes to reflect changes that might have been done before the system was shutdown.

The old Backup file is deleted before the new Backup file is available.

The data in the exported file include all configurations and settings of the controller.

The sFTP users can retrieve the exported file stored in the following directory of the system: /Export/<export file name>.

A system supporting sFTP is needed.

To retrieve the file sFTP users do not need to use any password.

The username for sFTP users is as follows:

Username | autoexport

# StepSync

Controller features, such as the Low Reaction Tightening Strategies and controller-wide functions among others, require licenses distributed through the Functionality Management System (FMS). Whereas configuration of features is possible without specific licenses, the assignment and use of those features will require the correct license to be installed on the controller. Please refer to Licenses (FMS) for more detailed information on licenses.

StepSync requires ToolsTalk 2 to configure.

With the StepSync function it is possible to connect several Power Focus 6000 controllers together and run synchronized tightenings. The first controller in the configuration is called the Sync Reference and handles all the tightening and data reporting. Up to 5 additional Power Focus 6000 controllers are then connected to the Sync Reference via a Power Focus 6000 daisy-chain cable (see Setting up StepSync (hardware) and are called Sync Members, their only function is to handle the tools.

## Sync Reference

The Sync Reference controller is the brain in the system. It handles the tightening settings and all data reporting. It also handles the configuration for the complete system and the connection to ToolsTalk and ToolsNet. All accessories or fieldbuses are connected directly to the Sync Reference

## Sync Member

The Sync Member controller works as a drive without extra functionality. The IT part is not running and it is not possible to connect any external accessories or protocols to a Sync Member. Each Sync Member has a channel number assigned to it. The channel number is used to identify the tool and drive within the Hardware Layout Configuration in ToolsTalk 2, as well as to select the ones that should be included in the tightening in Sync Mode, and also used for result reporting. It is also used for error events to make it possible to identify the faulty part.

## Tightenings

It is only possible to run Multistep tightening programs. To be able to synchronize tightenings between each tool, synchronization points are used. At these points, the tools will wait for each other before continuing with the next step in the tightening program. A tightening program can contain up to 10 steps (not counting the synchronization points). Note that the assignment of tightening programs can only take place through ToolsTalk 2. The controller does not provide possibilities to assign tightening programs.

## Licensing

The StepSync function is an FMS feature. It is only the Sync Reference that requires a license, making it possible to change any Power Focus 6000 controller into a Sync Member without any additional licenses. The Sync Reference license is an add-on FMS controller feature.

If the Sync Reference license is removed, no tightenings can be performed in StepSync mode. If connection to the license server is lost, the license will continue to operate for 48 hours. The controller will check for a valid Sync Reference license every hour.

Relevant Information

- Setting up StepSync (hardware)

In this Section

- StepSync User Interface
- Configuring StepSync
- Setting up StepSync (hardware)
- StepSync Tightenings
- StepSync Results
- StepSync Signals
- StepSync compatible tools
- StepSync CAN Accessories

# StepSync User Interface

The StepSync user interface is a simplified version of the regular POWER FOCUS 6000 interface. For detailed descriptions on the various interface elements, please refer to the dedicated chapters and sections in this manual describing those. Note that the user interface is only accessible on the Sync Reference.

Not all functions in the various menu items are available in the StepSync interface. The following functions are accessible and editable in the interface:

- Tool: all information available.

- Virtual Station: all functions accessible, except creation of new Virtual Stations, assignment of Tasks (tightening program), and assignment of tool among others.

- Configurations: all functions available.

- StepSync (Controller): all functions available. Note that there is an extra section here called Channels where information on the tools connected to the Sync Reference and Sync Members is given.

- Reports: Events (view all events).

- Settings: the following functions are not available:

  - Tightening

  - Wireless

  - Events

- Diagnostics: menu specific to StepSync/Flex.

- License assignment: all functions available.

# Configuring StepSync

The configuration of the Sync Reference and all Sync Members needs to be completed before performing the hardware set-up.

## Configuring the Sync Reference

1. Select the Controller menu, then select the StepSync tab.

2. In the StepSync section, select No Sync

   The Step Sync Mode window appears.

3. Select Sync Reference

   The Step Sync Mode window closes.

4. Select Apply.

   The controller will reboot and boot into the StepSync configuration, which is a simplified version of the regular Power Focus 6000 GUI.

## Enabling StepSync

In order for StepSync to work, it has to be enabled on the Sync Reference. There are two ways to enable StepSync:

1. Set the I/O signal Enable Operation (10055) to High, or

2. In the Sync reference, go to Configurations, then to the General Virtual Station tab, and click on Edit for the configuration in question. Then, in the Fixtured Stations field, set Auto Enable to Always.

If StepSync has not been enabled, at runtime the user will be presented with an error message saying "Unable to start, enable signal is low."

## Configuring the Sync Member

1. Select the Controller menu, then select the StepSync tab.

2. In the StepSync section, select No Sync

   The Step Sync Mode window appears.

3. Select Sync Member

   The Step Sync Mode window closes.

4. In the Channel field, set the channel number for the Sync Member by selecting the channel number. Then select the appropriate channel for the Sync Member.

   The channel numbers of the Sync Members in the same set-up must be unique.

5. Select Apply.

   The controller will reboot and boot into the Sync Member configuration, which will only display the Sync Member's channel number.

## Switching back to regular Power Focus 6000 mode (exiting StepSync)

1. Select the PF6 FlexSystem menu, then select the StepSync tab.

2. In the StepSync section, select Sync Reference

   The Step Sync Mode window appears.

3. Select No Sync

   The Step Sync Mode window closes.

4. Select Apply.

   The controller will reboot and boot into the regular configuration.

# Setting up StepSync (hardware)

Note that software configuration needs to be done before hardware set-up is completed in order to avoid possible set-up conflicts.

The StepSync function allows several POWER FOCUS 6000 to be connected in order to run synchronized tightenings.

1. Make sure each controller has been configured correctly (see StepSync Configuration for more information).

2. Using a Power Focus 6000 daisy-chain cable, connect the Sync Reference Com Port B to the first Sync Member's Com Port A.

3. Using another PF6000 daisy-chain cable, connect the first Sync Member's Com Port B to the second Sync Member's Com Port A. Do the same for all subsequent controllers.

   A StepSync system can be configured with a maximum of 5 Sync Members.

A | Sync Reference | D | Connected to Com Port A
B | Sync Member | E | Power Focus 6000 daisy-chain cable
C | Connected to Com Port B |  |

Relevant Information

- Configuring StepSync

# StepSync Tightenings

The only possible tightening programs to use in conjunction with StepSync are Multistep tightening programs. To synchronization between the tools in the set-up, Synchronization points are used. At these points, the tools will wait for each other before continuing with the next step in the Multistep tightening program. Note that assigning tightening programs to the different tools can only take place in ToolsTalk 2.

Example of a Multistep tighteningprogram for StepSync

A | Synchronization point

A tightening program can consist of a maximum of 10 steps (not counting the Synchronization points).

Available steps

- Tighten to Angle

- Tighten to Torque

- Tighten to Torque plus Angle

- Tighten to DynaTork

- Wait

- Socket Release

- Tighten to Torque or Angle

- Loosen to Angle

- Loosen to Torque

- Rundown

- Tighten to Yield M2

- Tighten to Yield

- Tighten to Torque and Angle

- Thread cutting to torque

- Engage

Available Monitors

- Angle

- Peak Torque

- Shut Off Torque

- Torque rate and deviation

- Torque in angle window

- Post view torque high

- Post view torque los

- Angle from Yield

- Prevailing Torque

- Shut Off Current

- Post Thread cut angle

- Post Thread cut peak torque

- Stick Slip Detection

- Time

Available Step Restrictions

- Maximum Torque

- Maximum Angle

- Cross Thread

- Rescinding Torque

- Torque Gradient

- Torque in Angle View

- Torque vs Current Deviation

Reject Management

Action if failure | Description
End all | All channels will end the tightening and report status NOK. The tightening that did not have an error itself will report additional info Terminated by other bolt.
Continue OK | The failing channels will end the tightening with status NOK. The remaining channels will continue with the rest of the tightening program.

# StepSync Results

The results for all the tools in the StepSync tightening will be shown on the controller GUI of the Sync Reference and in its corresponding Web GUI. The GIU on the Sync Members will not show any results.

There are three different Result views. The first shows an overview of the total status for the entire tightening (OK or NOK) and the total number of OK and NOK bolts. The second shows the status for each bolt separately, and the third also shows the torque and angle values for each bolt.

Example of Overall Status View
Example of Overall Status view with Bolt Status
Example of Detailed Status view

# StepSync Signals

The StepSync system supports the same I/O signals listed in the tables below. These can be mapped in fieldbus configuration and accessory configuration. Some are also available through Open Protocol.

In this Section

- Input Signals
- Output Signals
- Input/Output Signals
- Input Signals: Sub-signals
- Output Signals: Sub-signals

# Input Signals

Converter
Signal Type
Value Type
Size Min [bit]
Size Max [bit]
Devices
Search

# Abort Sequence - 10012

When a Batch sequence abort request is received, the Batch sequence functionality aborts the batch sequence only after getting the ongoing tightening result.

Name in SoftPLC: ABORT_BATCH_SEQUENCE

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Abort Sequence and Clear Result- 10127

When signal "Abort sequence and clear results" is set, the ongoing sequence is aborted and signals related to "Clear results" are cleared.

Name in SoftPLC:ABORT_SEQ_AND_CLEAR_RES

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Batch Decrement - 10002

Incrementally decreases the batch counter by one.

Name in SoftPLC: BATCH_DECREMENT

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Batch Increment - 10001

Incrementally increases the batch counter by one.

Name in SoftPLC: BATCH_INCREMENT

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Bypass Tightening Program - 10008

Skips the next tightening program in the running batch sequence.

Name in SoftPLC: BYPASS_PSET

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Channel Command - 10054

Channel Command is an input signal that inhibits individual tools and prevents that those tools are included in the next tightening. It is also possible to replace the tightening program or bolt number configured in the sync mode configuration. Up to 64 channels are supported.

Name in SoftPLC: CHANNEL_COMMAND

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | uint32 array | 1 | 64

The signal Channel Command -10054 contains sub-signals (for more information, see "Input Signals: Sub-signals").

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Continue Step - 10128

Continue Step is an input signal that stops the Wait tightening step.
When the tightening has reached a Wait tightening step with the condition Signal configured as Wait Type, a rising edge of the signal Continue Step causes the system (one or more spindles) to release.

For more information, see the sub-signal Channel Command - 10054: Continue Step.

Name in SoftPLC: CONTINUE_STEP

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Data Drop - 10125

When set DATADROP to true at the end of a tightening DATADROP signal will drop result from the tightening. The result will not be stored persistently or sent to any device or clients like ToolsNet or protocol adapters.

Name in SoftPLC: DATADROP

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Data Hold - 10124

When signal DATAHOLD is set to true at the end of a tightening, transmission of the result data will be stopped.

Name in SoftPLC: DATAHOLD

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Disable Fieldbus - 10049

Disables the fieldbus.

Name in SoftPLC: DISABLE_FIELDBUS

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Filedbus: FALSE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Disable Test Bolt - 10057

Name in SoftPLC: DISABLE_TESTBOLT

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Disable tool - 30000

If the signal is set to True, a tool is immediately stopped and locked.

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | Boolean | 1 | 1
Invert | State | Boolean | 1 | 1

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Dynamic Batch Size - 10074

Name in SoftPLC: DYNAMIC_BATCH_SIZE

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Integer | 1 | 16

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Enable Operation - 10055

Name in SoftPLC: ENABLE_OPERATION

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | Boolean | 1 | 1
Invert | State | Boolean | 1 | 1

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Fieldbus AsyncData To PF - 10077

Name in SoftPLC:

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | uint8 array | 16 | 2048

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Fieldbus Lock Loosening - 20021

A Virtual Station is locked when starting a loosening if the signal is set from a connected and supported accessory.
An ongoing loosening is aborted immediately when Fieldbus Lock Loosening is set to True, due to the Stop Drive setting.

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | Boolean | 1 | 1
Invert | State | Boolean | 1 | 1

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Fieldbus Lock Tightening - 20020

A Virtual Station is locked when starting a tightening if the signal is set from a connected and supported accessory.
An ongoing tightening is aborted immediately when Fieldbus Lock Tightening is set to True, due to the Stop Drive setting.

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | Boolean | 1 | 1
Invert | State | Boolean | 1 | 1

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Flush Read Result Queue - 30005

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# ID for Dynamic Batch Size - 10073

Name in SoftPLC: DYNAMIC_BATCH_SIZE_TPID

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | Integer | 1 | 16
TreatZeroAsOne | State | Integer | 1 | 16

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Lock Loosening - 20003

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Filedbus: FALSE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Lock Tightening - 20002

Tool locked for tightening by digital input.

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Filedbus: FALSE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Lock Tool Active High - 20004

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Filedbus: FALSE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Lock Tool Active Low - 20061

Locks the tool when this signal is low.

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Filedbus: FALSE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Master Unlock - 10005

Master Unlock is an input signal which unlocks the following functions and signals.

FUNCTIONS:

- Disable loosening at OK tightening

- Disable loosening at NOK tightening

- Disable tightening

- Max consecutive NOK

- Tool Lock on Sequence complete

SIGNALS:

- 20001 - Pending Event Acknowledge Lock

- 20002 - Lock Tightening

- 20003 - Lock Loosening

- 20004 - Lock Tool Active High

- 20013 - WorkTask Lock Tightening

- 20014 - WorkTask Lock Loosening

- 20015 - Batch Done lLock

- 20018 - Open Protocol Lock

- 20020 - Fieldbus Lock Tightening

- 20021 - Fieldbus Lock Loosening

- 20022 - Disable Loosening At OK Tight

- 20023 - Too Many NOK Tightenings Lock

- 20033 - Line Control Lock

- 20034 - Locked By Alternative Identifier

Name in SoftPLC: MASTER_UNLOCK

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Pulse Stop - 10030

If this signal is generated any ongoing tightening or loosening will be stopped. Used in combination with 10024 or 10072.

Name in SoftPLC: TIGHTENING_STOP_PULSE

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Read Result Handshake Ack - 30004

Enable the Read Result Handshake feature in the Fieldbus device for making the controller available for the signal Rear Result Handshake Ack.

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

Relevant Information

- Configuration of the Fieldbus

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Reset All Identifiers - 10115

In Source batch string used to reset all received string identifiers from string receiving sequence at once. In other worktasks clears VIN number.

Name in SoftPLC: RESET_ALL_IDENTIFIERS

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Reset Batch - 10003

Resets the batch counter to 0. No batch OK (nxOK). If batch OK is activated, it will be deactivated.

Name in SoftPLC: RESET_BATCH

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Reset Batch Sequence - 10053

Resets the Batch Sequence. Unlocks a tool that is locked by Tool Lock on Complete.

Name in SoftPLC: RESET_BATCH_SEQUENCE

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Reset Bistable Relay - 10022

Reset the bistable relay output.

Name in SoftPLC: RESET_BISTABLE_RELAY

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Reset Cycle Status - 10056

Name in SoftPLC: RESET_CYCLE_STATUS

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Reset Latest Identifier - 10114

In Source batch string used to reset latest received string from string receiving sequence. In other worktasks clears VIN number.

Name in SoftPLC: RESET_LATEST_IDENTIFIER

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Reset Sequence Status - 10118

Resets signals Batch Sequence Done/OK/NOK and Sequence Aborted.

Name in SoftPLC: RESET_SEQUENCE_STATUS

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Reset System Error - 10062

Name in SoftPLC: RESET_SYSTEM_ERROR

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Reset Too Many NOK - 10013

Reset the batch after receiving lock Too Many NOK

Name in SoftPLC: RESET_TOO_MANY_NOK

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Select Input - 10020

Selects Tightening Program withing Source Tightening/Batch within sequence.

Name in SoftPLC: SELECT_INPUT_VALUE

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | Integer | 1 | 16
TreatZeroAsOne | State | Integer | 1 | 1

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: TRUE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Select Input and Dynamic Batch Size - 30007

It is used to set the Batch Size for a specific "Identifier Number" in a Source Tightening Task, running "External batch control".

Batch size can be set to 1-250.

If Batch size is set to 0, it is treated as infinite batch. The user is not able to un-set a Batch back to a state where it has no size, once it has been set.

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | Integer | 16 | 16
TreatZeroAsOne | State | Integer | 16 | 16

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Select Input Bit 0 - 10016

Name in SoftPLC: SEL_INPUT_BIT_0

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Filedbus: FALSE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Select Input Bit 1 - 10017

Name in SoftPLC: SEL_INPUT_BIT_1

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Filedbus: FALSE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Select Input Bit 2 - 10018

Name in SoftPLC: SEL_INPUT_BIT_2

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Filedbus: FALSE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Select Input Bit 3 - 10019

Name in SoftPLC: SEL_INPUT_BIT_3

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Filedbus: FALSE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Select Input Bit 4 - 10066

Name in SoftPLC: SEL_INPUT_BIT_4

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Filedbus: FALSE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Select Input Bit 5 - 10067

Name in SoftPLC: SEL_INPUT_BIT_5

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Filedbus: FALSE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Select Input Bit 6 - 10068

Name in SoftPLC: SEL_INPUT_BIT_6

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Filedbus: FALSE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Select Input Bit 7 - 10069

Name in SoftPLC: SEL_INPUT_BIT_7

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Filedbus: FALSE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Select Input Bit 8 - 10070

Name in SoftPLC: SEL_INPUT_BIT_8

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Filedbus: FALSE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Select Input Bit 9 - 10071

Name in SoftPLC: SEL_INPUT_BIT_9

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Filedbus: FALSE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Select Loosening - 10029

Selects loosening as default operation mode and used in combination with Start Tools -10028 signal.

Name in SoftPLC: SELECT_LOOSENING

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

Relevant Information

- Start Tools - 10028

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Select Next Identifier Number - 10116

It is possible to use the signal Select Next Identifier Number when a task in the virtual station is configured as:

- Batch Sequence

- Source Tightening

- Source Batch

  - Number Identifier method

  - String Identifier method

ST Selector configurable functions Take Next and Take Previous enable the input signals Select Next Identifier Number and Select Previous Identifier Number.

## Batch Sequence selected as Virtual Station Task

If Free Order switch has been enabled, the signal Select Next Identifier Number can select different batches within the selected sequence.

Before selecting batches, it is mandatory that they have the identifier number assigned. If a batch does not have the identifier number assigned, the signal Select Next Identifier Number cannot select it, even if Free Order switch is enabled.

It enables looping through the batches that have a configured identifier number.
If identifier number is "None", it is possible to select it only after all Batches with configured identifier number are completed.

It is possible to do looping, but 0 is skipped. When a batch is finished, it is no longer selectable.

For example, in case of batches with assigned identifier numbers 1,2,4,5, the signal runs in loop: 1,2,4,5,1,2,4... as long as the batches are not finished.

## Source Tightening selected as Virtual Station Task

The signal selects the next identifier number from the list of tightening programs specified in the Source Tightening task.
The selection runs from the currently selected identifier number to the next larger one.

When the biggest identifier number is selected, this signal selects 0; after 0, the signal selects the next bigger identifier number.

If 0 is selected as identifier number, the tool is locked.

If the identifier number has been added to the Source Tightening list, but no tightening program has ever been assigned to it, it is skipped while looping through the Source Tightening list.

If the tightening program is assigned to an identifier number and then it is removed from the list of tightening programs, it is still possible to select this identifier number. In this case, the tool is locked because there is not a specific tightening program.

When Selector Mode switch is set to Confirm, the socket selector needs to be assigned and configured. All tightening programs can be selected, but before running them, appropriate socket must be lifted from the socket selector.

## Source Batch selected as Virtual Station Task

In Sources > Batch Sequence > Source Batch, when the identifier method is set to Number, the signal Select Next Identifier Number selects sequences from a list of sequences shown in Source Batch task.

It is possible to do looping through 0. The signal Select Next Identifier Number selects only the identifier numbers assigned to sequences.

For example, if there are 4 sequences available with identifier numbers 1,2,4, and 8, the signal Select Next Identifier Number iterates and selects 1,2,4,8,0,1,2...

The identifier numbers not defined are not selected.

In Sources > Batch Sequence > Source Batch, when the identifier method is set to String, it is necessary to select the sequence through external sources (like scanner or Open Protocol). The signal Select Next Identifier Number is able to select the batches within the selected sequence.

Name in SoftPLC: SELECT_NEXT_ID_NUMBER

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

Relevant Information

- ST Selector
- Working with the Batch Sequence Tab

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: TRUE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Select Previous Identifier Number - 10117

It is possible to use the signal Select Previous Identifier Number when a task in the virtual station is configured as:

- Batch Sequence

- Source Tightening

- Source Batch

  - Number Identifier method

  - String Identifier method

ST Selector configurable functions Take Next and Take Previous enable the input signals Select Next Identifier Number and Select Previous Identifier Number.

## Batch Sequence selected as Virtual Station Task

If Free Order switch has been enabled, the signal Select Previous Identifier Number can select different batches within the selected sequence.

Before selecting batches, it is mandatory that they have the identifier number assigned. If a batch does not have the identifier number assigned, the signal Select Previous Identifier Number cannot select it, even if Free Order switch is enabled.

It enables looping through the batches that have a configured identifier number.
If identifier number is "None", it is possible to select it only after all Batches with configured identifier number are completed.

It is possible to do looping, but 0 is skipped. When a batch is finished, it is no longer selectable.

For example, in case of batches with assigned identifier numbers 1,2,4,5, the signal runs in loop: 5,4,2,1,5,4,2... as long as the batches are not finished.

## Source Tightening selected as Virtual Station Task

The signal selects the previous identifier number from the list of tightening programs specified in the Source Tightening task.
The selection runs from the currently selected identifier number to the previous lower one.

When the smallest identifier number is selected, this signal selects 0; after 0, the signal selects the next smaller identifier number.

If 0 is selected as identifier number, the tool is locked.

If the tightening program is assigned to an identifier number and then it is removed from the list of tightening programs, it is still possible to select this identifier number. In this case, the tool is locked because there is not a specific tightening program.

When Selector Mode switch is set to Confirm, the socket selector needs to be assigned and configured. All tightening programs can be selected, but before running them, appropriate socket must be lifted from the socket selector.

## Source Batch selected as Virtual Station Task

In Sources > Batch Sequence > Source Batch, when the identifier method is set to Number, the signal Select Previous Identifier Number selects sequences from a list of sequences shown in Source Batch task.

It is possible to do looping through 0. The signal Select Previous Identifier Number selects only the identifier numbers assigned to sequences.

For example, if there are 4 sequences available with identifier numbers 1,2,4, and 8, the signal Select Previous Identifier Number iterates and selects 8,4,2,1,0,8,4...

The identifier numbers not defined are not selected.

In Sources > Batch Sequence > Source Batch, when the identifier method is set to String, it is necessary to select the sequence through external sources (like scanner or Open Protocol). The signal Select Previous Identifier Number is able to select the batches within the selected sequence.

Name in SoftPLC: SELECT_PREVIOUS_ID_NUMBER

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

Relevant Information

- ST Selector
- Working with the Batch Sequence Tab

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: TRUE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Set Bistable Relay - 10021

Set the bistable relay output.

Name in SoftPLC: SET_BISTABLE_RELAY

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Start Loosening - 10011

Active signal starts loosening. Once digital input goes inactive the loosening must be stopped.

Name in SoftPLC: START_LOOSENING

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Start Loosening, Pulse - 10072

Name in SoftPLC: SELECT_PREVIOUS_ID_NUMBER

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

Relevant Information

- ST Selector
- Working with the Batch Sequence Tab

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: TRUE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Start Tightening - 10010

Active signal starts tightening. Once input goes inactive the tightening must be stopped.

Name in SoftPLC: START_TIGHTENING

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Start Tightening Pulse - 10024

The tightening starts at signal. Runs until the tightening is finished, or until the 30 sec timeout in tightening program occurs.

Name in SoftPLC: TIGHTENING_START_PULSE

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Start Tools - 10028

Active signal which starts the tool (default operation mode is tightening). As soon as signal goes inactive the tool must be stopped. Used in combination with Select Loosening - 10029 signal.

Name in SoftPLC: START_DRIVE_CONTINIOUS

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

Relevant Information

- Select Loosening - 10029

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Start Tools, Pulse - 10113

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

Relevant Information

- ST Selector
- Working with the Batch Sequence Tab

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: TRUE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# To SoftPLC - 10065

Name in SoftPLC: TO_PLC

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | uint8 array | 1 | 1

## Devices

- Filedbus: FALSE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Unlock Tool on Complete - 10051

Unlocks a tool that is locked by "Tool Lock on Complete".

Name in SoftPLC: UNLOCK_TOOL_ON_COMPLETE

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Unlock Tool on Disable - 10059

Name in SoftPLC: UNLOCK_TOOL_ON_DISABLE

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Output Signals

Converter
Signal Type
Value Type
Size Min [bit]
Size Max [bit]
Devices
Search

# Active Identifier String - 186

Set when an identifier string has been received and accepted by the work-task; it is necessary that even sequence or tightening program are running.
If running Source batch-string, it is set when all scans have been received and a sequence had been selected. In that case it includes concatenated string consisted of saved positions.
For other work-tasks it includes the “VIN” number.

Name in SoftPLC: ACTIVE_IDENTIFIER_STRING

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | String | 8 | 800
IdentifierU32Hnw | State | String | 8 | 800
IdentifierU32 | State | String | 8 | 800

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Active Identifier String 1 - 188

Signal corresponding to the first configured string in Source batch-string.
Active Identifier String 1 signal is sent once a scanning sequence is done and a sequence has been selected, thus the identifier parts are active.
The strings is filtered with saved position.
Only sent when running Source batch string.

Name in SoftPLC: ACTIVE_ID_STRING_1

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | String | 8 | 800
IdentifierU32Hnw | State | String | 8 | 800
IdentifierU32 | State | String | 8 | 800

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Active Identifier String 2 - 189

Signal corresponding to the second configured string in Source batch-string.
Active Identifier String 2 signal is sent once a scanning sequence is done and a sequence has been selected, thus the identifier parts are active.
The strings is filtered with saved position.
Only sent when running Source batch string.

Name in SoftPLC: ACTIVE_ID_STRING_2

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | String | 8 | 800
IdentifierU32Hnw | State | String | 8 | 800
IdentifierU32 | State | String | 8 | 800

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Active Identifier String 3 - 190

Signal corresponding to the third configured string in Source batch-string.
Active Identifier String 3 signal is sent once a scanning sequence is done and a sequence has been selected, thus the identifier parts are active.
The strings is filtered with saved position.
Only sent when running Source batch string.

Name in SoftPLC: ACTIVE_ID_STRING_3

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | String | 8 | 800
IdentifierU32Hnw | State | String | 8 | 800
IdentifierU32 | State | String | 8 | 800

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Active Identifier String 4 - 191

Signal corresponding to the fourth configured string in Source batch-string.
Active Identifier String 4 signal is sent once a scanning sequence is done and a sequence has been selected, thus the identifier parts are active.
The strings is filtered with saved position.
Only sent when running Source batch string.

Name in SoftPLC: ACTIVE_ID_STRING_4

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | String | 8 | 800
IdentifierU32Hnw | State | String | 8 | 800
IdentifierU32 | State | String | 8 | 800

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Batch Completed - 30

Batch Completed is an output signal which is triggered when the batch is complete.
The batch result status (OK or NOK) has no effect on the Batch Completed signal.

Name in SoftPLC: BATCH_COMPLETED

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Batch Completed NOK - 37

Batch finished with status NOK.

Name in SoftPLC: BATCH_COMPLETED_NOK

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Batch Completed OK - 36

Batch finished with status OK.

Name in SoftPLC: BATCH_COMPLETED_OK

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Batch Count - 31

Batch Count is an output signal which shows the current number of tightening in the batch.

Name in SoftPLC: BATCH_COUNT

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Integer | 1 | 8

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: TRUE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Batch Running - 32

Indicates that a batch in a batch sequence is running.

Name in SoftPLC: BATCH_RUNNING

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Batch Sequence Completed NOK - 46

Batch sequence finished with status NOK.

Name in SoftPLC: BATCH_SEQUENCE_NOK

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Batch Sequence Completed OK - 45

Batch sequence finished with status OK.

Name in SoftPLC: BATCH_SEQUENCE_OK

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Batch Sequence Done - 48

Indicates when a sequence is completed, both in case Batch Sequence Completed OK and Batch Sequence Completed NOK.

Name in SoftPLC: BATCH_SEQUENCE_COMPLETED

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | Event | Boolean | 1 | 1
Invert | Event | Boolean | 1 | 1

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Batch Sequence Running - 47

Indicates if the Batch Sequence is running or not.

Name in SoftPLC: BATCHSEQUENCE_RUNNING

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | Boolean | 1 | 1
Invert | State | Boolean | 1 | 1

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Bistable Relay - 40

Bistable Relay is a signal controlled by the inputs "Set Bistable Relay" and "Reset Bistable Relay".
After receiving the input "Set Bistable Relay", Bistable Relay signal is set to True.
After receiving the input "Reset Bistable Relay", Bistable Relay signal is set to False.

If "Set Bistable Relay" or "Reset Bistable Relay" goes low, the Bistable relay keeps its state.
The state for the Bistable relay changes when "Set Bistable Relay" or "Reset Bistable Relay" goes high.

After restarting the controller, the Bistable relay is set to False as default.

Name in SoftPLC: BISTABLE_RELAY

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | Boolean | 1 | 1
Invert | State | Boolean | 1 | 1

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Bolt Tightening Status - 79

Bolt Tightening Status is an output signal that identifies the status for individual bolts in a synchronized tightening. 100 bolts are supported.
Bolt Tightening Status signal shows information related to the running tightening and the result of the last tightening.

Name in SoftPLC: BOLT_TIGHTENING_STATUS

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | uint32 array | 32 | 32
FordResultStatus | State |  | 4 | 4

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

The signal Bolt Tightening Status - 79 contains sub-signals (for more information, see "Output Signals: Sub-signals").

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Channel Hardware Status - 81

Channel Hardware Status is an output signal that identifies the hardware status for individual channels. 64 channels are supported.
Channel Hardware Status signal shows information about the hardware status and possible errors.

Name in SoftPLC: CHANNEL_HARDWARE_STATUS

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | uint32 array | 1 | 64

The signal Channel Hardware Status - 81 contains sub-signals (for more information, see "Output Signals: Sub-signals").

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Channel Tightening Status - 80

Channel Tightening Status is an output signal that identifies the status for individual channels in a synchronized tightening. 64 channels are supported.
Channel Tightening Status signal shows information related to the running tightening and the result of the last tightening.

Name in SoftPLC: CHANNEL_TIGHTENING_STATUS

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | uint32 array | 1 | 64
FordResultStatus | State |  | 4 | 4

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

The signal Channel Tightening Status - 80 contains sub-signals (for more information, see "Output Signals: Sub-signals").

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Configuration Version - 88

Name in SoftPLC: CONFIGURATION_VERSION

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Integer | 1 | 32

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Controller Switched On - 42

Set to true at start up of IO Exchange

Name in SoftPLC: IO_ON

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Current Running Batch - 180

Current Running Batch is an output signal which shows the index of the current running batch in a sequence.
If the user uses a socket selector, "Zero" appears if none, more than one, or wrong socket is selected.
If the user uses batch mode and a batch is running, "1" appears for Source Tightening configurations.

Name in SoftPLC: CURRENT_RUNNING_BATCH_IX

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Integer | 1 | 8

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: TRUE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Cycle Complete - 77

Name in SoftPLC: CYCLE_COMPLETE

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Cycle NOK - 76

Name in SoftPLC: CYCLE_NOK

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Cycle OK - 75

Name in SoftPLC: CYCLE_OK

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Cycle Ready To Start - 82

Name in SoftPLC: CYCLE_READY_TO_START

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Cycle Running - 78

Name in SoftPLC: CYCLE_RUNNING

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Data Drop Active - 199

This signal will be set high whenever DATADROP function is active. When DATADROP input signal is set and worktask supporting DATADROP is selected.

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Data Hold Active - 198

This signal will be set high whenever the DATAHOLD function is active. When DATAHOLD signal is set and a worktask supporting DATAHOLD is selected.

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Emergency Stop - 20036

Name in SoftPLC: EMERGENCY_STOP

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Event Code - 30001

Relay an event when it is triggered. Momentary, on for two cycle times.

Name in SoftPLC: EVENT_CODE

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Integer | 1 | 16

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Event Code Severity - 30003

Event Code Severity is an output signal which is activated when the triggered event has severity of error or warning.

Name in SoftPLC: EVENT_CODE_SEVERITY

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Event Present - 161

Indicates if event is triggered. It is only triggered on accessories if event requires an ACK.

Name in SoftPLC: EVENT_PRESENT

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Fieldbus AsyncData From PF - 107

Name in SoftPLC:

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | uint8 array | 48 | 2048

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Fieldbus Disconnected - 96

Name in SoftPLC: FIELDBUS_DISCONNECTED

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Filedbus: FALSE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# From SoftPLC - 10064

Allocated bytes for data transfer from PLC to accessories.

Name in SoftPLC: FROM_PLC

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | uint8 array | 8 | 8

## Devices

- Filedbus: FALSE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Identifier Received - 100

Name in SoftPLC: IDENTIFIER_RECEIVED

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Last Received Identifier String - 187

Set directly when an identifier has been received in the work-task.
For Source batch-string, it is set at every scanning in scan process, thus it is changed for every scanning and sent even if it does not match in length.
String set is in raw format and not only "saved positions" in the string.
For other work-tasks this signal is equal to Active Identifier String signal.

Name in SoftPLC: LAST_RECEIVED_ID_STRING

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | String | 8 | 800
IdentifierU32Hnw | State | String | 8 | 800
IdentifierU32 | State | String | 8 | 800

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

Relevant Information

- Active Identifier String - 186

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Loosening Disabled - 184

Loosening Disabled is an output signal which is activated when the loosening is externally locked by any of the following signals:

- 20003 - Lock Loosening

- 20004 - Lock Tool Active High

- 20033 - Line Control Lock

- 20018 - Open Protocol Lock

- 20021 - Fieldbus Lock Loosening

- 20041 - Soft PLC Lock Loosening

- 20061 - Lock Tool Active Low

Name in SoftPLC: LOOSENING_DISABLED

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Loosening Enabled - 185

Loosening Disabled is an output signal which is activated when the loosening is not externally locked by any of the following signals:

- 20003 - Lock Loosening

- 20004 - Lock Tool Active High

- 20033 - Line Control Lock

- 20018 - Open Protocol Lock

- 20021 - Fieldbus Lock Loosening

- 20041 - Soft PLC Lock Loosening

- 20061 - Lock Tool Active Low

Name in SoftPLC: LOOSENING_ENABLED

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Loosening is Locked - 28

The loosening is disabled.

Name in SoftPLC: LOOSENING_IS_LOCKED

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | Boolean | 1 | 1
Invert | State | Boolean | 1 | 1

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Loosening NOK - 74

NOK loosening took place.

Name in SoftPLC: LOOSENING_NOK

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Loosening OK - 70

OK loosening took place.

Name in SoftPLC: LOOSENING_OK

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Max Consecutive NOK Reached - 35

Indicates Max coherent NOK tightening counter is reachead.

Name in SoftPLC: MAX_COHERENT_NOK_REACHED

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# No System Error - 83

Name in SoftPLC: NO_SYSTEM_ERROR

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# No System Warning - 102

Name in SoftPLC: NO_SYSTEM_WARNING

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Open Protocol Disconnected - 95

If Open Protocol is set to off in the Virtual Station, "Open Protocol Disconnected" signal is set to False.
If Open Protocol is turned on in the Virtual Station the "Open Protocol Disconnected" signal is set to True.
When at least one client (several Open Protocol clients can connect to the same Virtual Station) is connected the "Open Protocol Disconnected" signal is set to False.

Name in SoftPLC: OPEN_PROTOCOL_DISCONNECTED

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | Boolean | 1 | 1
Invert | State | Boolean | 1 | 1

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Program Start - 132

Defines the starting level for a tightening cycle.

Name in SoftPLC: PROGRAM_START

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Read Result Queue Flushed - 30006

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Received Identifier 1 - 192

Signal corresponding to the first configured string in Source batch-string.
Active Identifier String 1 signal is sent in the order the strings/identifiers are received by the system as soon as a string has been received. If running in forced order scan, it is in the configured order, but if running free order scan, 1 might not correspond to the first configured string, but to the first received string.
The strings is the raw received string and not have the "saved position" applied.
Only sent when running Source batch string.

Name in SoftPLC: RECEIVED_IDENTIFIER_1

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | String | 8 | 800
IdentifierU32Hnw | State | String | 8 | 800
IdentifierU32 | State | String | 8 | 800

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Received Identifier 2 - 193

Signal corresponding to the second configured string in Source batch-string.
Active Identifier String 2 signal is sent in the order the strings/identifiers are received by the system as soon as a string has been received. If running in forced order scan, it is in the configured order, but if running free order scan, 2 might not correspond to the second configured string, but to the second received string.
The strings is the raw received string and not have the "saved position" applied.
Only sent when running Source batch string.

Name in SoftPLC: RECEIVED_IDENTIFIER_2

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | String | 8 | 800
IdentifierU32Hnw | State | String | 8 | 800
IdentifierU32 | State | String | 8 | 800

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Received Identifier 3 - 194

Signal corresponding to the third configured string in Source batch-string.
Active Identifier String 3 signal is sent in the order the strings/identifiers are received by the system as soon as a string has been received. If running in forced order scan, it is in the configured order, but if running free order scan, 3 might not correspond to the third configured string, but to the third received string.
The strings is the raw received string and not have the "saved position" applied.
Only sent when running Source batch string.

Name in SoftPLC: RECEIVED_IDENTIFIER_3

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | String | 8 | 800
IdentifierU32Hnw | State | String | 8 | 800
IdentifierU32 | State | String | 8 | 800

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Received Identifier 4 - 195

Signal corresponding to the fourth configured string in Source batch-string.
Active Identifier String 4 signal is sent in the order the strings/identifiers are received by the system as soon as a string has been received. If running in forced order scan, it is in the configured order, but if running free order scan, 4 might not correspond to the fourth configured string, but to the fourth received string.
The strings is the raw received string and not have the "saved position" applied.
Only sent when running Source batch string.

Name in SoftPLC: RECEIVED_IDENTIFIER_4

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | String | 8 | 800
IdentifierU32Hnw | State | String | 8 | 800
IdentifierU32 | State | String | 8 | 800

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Remaining Batch - 33

Remaining tightenings in a batch. Can only be viewed on a display.

Name in SoftPLC: REMAINING_BATCH

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Integer | 1 | 8

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: TRUE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Selected Mode Id - 72

Name in SoftPLC: SELECTED_MODE_ID

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | Integer | 1 | 32
TreatZeroAsOne | State | Integer | 1 | 32

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Selected Sequence Bit 0 - 139

Bit pattern showing selected sequence.

Name in SoftPLC: SELECTED_SEQUENCE_BIT_0

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Filedbus: FALSE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Selected Sequence Bit 1 - 140

Bit pattern showing selected sequence.

Name in SoftPLC: SELECTED_SEQUENCE_BIT_1

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Filedbus: FALSE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Selected Sequence Bit 2 - 141

Bit pattern showing selected sequence.

Name in SoftPLC: SELECTED_SEQUENCE_BIT_2

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Filedbus: FALSE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Selected Sequence Bit 3 - 142

Bit pattern showing selected sequence.

Name in SoftPLC: SELECTED_SEQUENCE_BIT_3

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Filedbus: FALSE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Selected Sequence Bit 4 - 143

Bit pattern showing selected sequence.

Name in SoftPLC: SELECTED_SEQUENCE_BIT_4

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Filedbus: FALSE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Selected Sequence Bit 5 - 144

Bit pattern showing selected sequence.

Name in SoftPLC: SELECTED_SEQUENCE_BIT_5

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Filedbus: FALSE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Selected Sequence Bit 6 - 145

Bit pattern showing selected sequence.

Name in SoftPLC: SELECTED_SEQUENCE_BIT_6

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Filedbus: FALSE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Selected Sequence Bit 7 - 146

Bit pattern showing selected sequence.

Name in SoftPLC: SELECTED_SEQUENCE_BIT_7

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Filedbus: FALSE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Selected Sequence Bit 8 - 147

Bit pattern showing selected sequence.

Name in SoftPLC: SELECTED_SEQUENCE_BIT_8

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Filedbus: FALSE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Selected Sequence Bit 9 - 163

Bit pattern showing selected sequence.

Name in SoftPLC: SELECTED_SEQUENCE_BIT_9

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Filedbus: FALSE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Selected Sequence Id - 84

Shows the index of the selected batch sequence.

Name in SoftPLC: SELECTED_BATCH_SEQUENCE_ID

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | Integer | 1 | 16
TreatZeroAsOne | State | Integer | 1 | 16

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: TRUE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Sequence Aborted - 160

Output signal indicating if sequence was aborted.

Name in SoftPLC: SEQUENCE_ABORTED

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Size of Sequence - 181

Shows the size of the currently running sequence. Only set when a sequence is loaded and not reset when sequence is done.

Name in SoftPLC: SIZE_OF_RUNNING_SEQUENCE

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Integer | 1 | 8

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: TRUE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Software Major Version - 86

Name in SoftPLC: SOFTWARE_MAJOR_VERSION

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Integer | 1 | 32

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Software Minor Version - 87

Name in SoftPLC: SOFTWARE_MINOR_VERSION

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Integer | 1 | 32

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Software Release Version - 85

Version of the software running.

Name in SoftPLC: SOFTWARE_RELEASE_VERSION

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Integer | 1 | 32

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Station Ready - 71

Indicates when the Virtual Station is ready.

Name in SoftPLC: STATION_READY

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | Boolean | 1 | 1
Invert | State | Boolean | 1 | 1

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Test Bolt Activated - 91

Name in SoftPLC: SELECTED_MODE_ID

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Tightening Disabled - 182

Tightening Disabled is an output signal which is activated when the tightening is externally disabled by any of the following signals:

- 20002 - Lock Tightening

- 20004 - Lock Tool Active High

- 20033 - Line Control Lock

- 20018 - Open Protocol Lock

- 20020 - Fieldbus Lock Tightening

- 20040 - Soft PLC Lock Tightening

- 20061 - Lock Tool Active Low

Name in SoftPLC: TIGHTENING_DISABLED

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Tightening Enabled - 183

Tightening Enabled is an output signal which is activated when the tightening is not externally disabled by any of the following signals:

- 20002 - Lock Tightening

- 20004 - Lock Tool Active High

- 20033 - Line Control Lock

- 20018 - Open Protocol Lock

- 20020 - Fieldbus Lock Tightening

- 20040 - Soft PLC Lock Tightening

- 20061 - Lock Tool Active Low

Name in SoftPLC: TIGHTENING_ENABLED

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Tightening is Locked - 27

The tightening is disabled; it is not possible to make any tightening.

Name in SoftPLC: TIGHTENING_IS_LOCKED

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | Boolean | 1 | 1
Invert | State | Boolean | 1 | 1

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Tightening NOK - 4

At least one result of the tightening is outside the specified limits.

Name in SoftPLC: TIGHTENING_NOK

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Tightening OK - 3

The result of the tightening is within the specified limits.

Name in SoftPLC: TIGHTENING_OK

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Tool Loosening - 22

Indicates that the tool is loosening.

Name in SoftPLC: TOOL_LOOSENING

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Tool Tightening - 21

Indicates that the tool is tightening.

Name in SoftPLC: TOOL_TIGHTENING

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Waiting To Continue - 201

Waiting To Continue is an output signal, which means that the tightening has reached a Wait tightening step with the condition Signal configured as Wait Type.
The system (one or more spindles) pauses the tightening waiting for the signal Continue Step - 10128 (for system release) or the sub-signal Channel Command - 10054: Continue Step (for individual spindle release).

For more information, see the sub-signals Bolt Tightening Status - 79: Waiting To Continue and Channel Tightening Status - 80: Waiting To Continue.

Name in SoftPLC: WAITING_FOR_CONTINUE

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Input/Output Signals

Converter
Signal Type
Value Type
Size Min [bit]
Size Max [bit]
Devices
Search

# Clear Results - 39

Clears status of other signals set to next tightening.

Name in SoftPLC: CLEAR_RESULTS

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Disable Open Protocol Commands - 10060

Disables the possibility to send commands over Open Protocol to the Virtual Station.

Name in SoftPLC: DISABLE_OPEN_PRTCOL_CMDS

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | Boolean | 1 | 1
Invert | State | Boolean | 1 | 1

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# External Identifier - 10045

The string sent in External identifier is included in the result as VIN number. It is possible to provide up to 2 identifiers to be passed from Fieldbus for task selection.

Name in SoftPLC: EXTERNAL_IDENTIFIER

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | String | 8 | 800
IdentifierU32Hnw | State | String | 8 | 800
IdentifierU32 | State | String | 8 | 800

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# External Monitored 1 - 10035

External Monitored 1 is an Input/Output signal that is not attached to any specific feature in the controller and can be used for customer specific needs.

Name in SoftPLC: EXTERNAL_MONITORED_1

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | Boolean | 1 | 1
Invert | State | Boolean | 1 | 1

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# External Monitored 2 - 10036

External Monitored 2 is an Input/Output signal that is not attached to any specific feature in the controller and can be used for customer specific needs.

Name in SoftPLC: EXTERNAL_MONITORED_2

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | Boolean | 1 | 1
Invert | State | Boolean | 1 | 1

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# External Monitored 3 - 10037

External Monitored 3 is an Input/Output signal that is not attached to any specific feature in the controller and can be used for customer specific needs.

Name in SoftPLC: EXTERNAL_MONITORED_3

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | Boolean | 1 | 1
Invert | State | Boolean | 1 | 1

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# External Monitored 4 - 10038

External Monitored 4 is an Input/Output signal that is not attached to any specific feature in the controller and can be used for customer specific needs.

Name in SoftPLC: EXTERNAL_MONITORED_4

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | Boolean | 1 | 1
Invert | State | Boolean | 1 | 1

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# External Monitored 5 - 10039

External Monitored 5 is an Input/Output signal that is not attached to any specific feature in the controller and can be used for customer specific needs.

Name in SoftPLC: EXTERNAL_MONITORED_5

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | Boolean | 1 | 1
Invert | State | Boolean | 1 | 1

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# External Monitored 6 - 10040

External Monitored 6 is an Input/Output signal that is not attached to any specific feature in the controller and can be used for customer specific needs.

Name in SoftPLC: EXTERNAL_MONITORED_6

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | Boolean | 1 | 1
Invert | State | Boolean | 1 | 1

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# External Monitored 7 - 10041

External Monitored 7 is an Input/Output signal that is not attached to any specific feature in the controller and can be used for customer specific needs.

Name in SoftPLC: EXTERNAL_MONITORED_7

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | Boolean | 1 | 1
Invert | State | Boolean | 1 | 1

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# External Monitored 8 - 10042

External Monitored 8 is an Input/Output signal that is not attached to any specific feature in the controller and can be used for customer specific needs.

Name in SoftPLC: EXTERNAL_MONITORED_8

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | Boolean | 1 | 1
Invert | State | Boolean | 1 | 1

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Fieldbus Keep Alive - 30002

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Integer | 1 | 8

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Flash Tool Green LED (external protocol) - 10058

Name in SoftPLC: FLASH_TOOL_GREEN_LED

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Generic I/O 1 - 50

Input/Output 1 used for Open Protocol.

Name in SoftPLC: GENERIC_IO_1

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Integer | 1 | 8

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: TRUE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Generic I/O 2 - 51

Input/Output 2 used for Open Protocol.

Name in SoftPLC: GENERIC_IO_2

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Integer | 1 | 8

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: TRUE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Generic I/O 3 - 52

Input/Output 3 used for Open Protocol.

Name in SoftPLC: GENERIC_IO_3

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Integer | 1 | 8

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: TRUE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Generic I/O 4 - 53

Input/Output 4 used for Open Protocol.

Name in SoftPLC: GENERIC_IO_4

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Integer | 1 | 8

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: TRUE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Generic I/O 5 - 54

Input/Output 5 used for Open Protocol.

Name in SoftPLC: GENERIC_IO_5

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Integer | 1 | 8

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: TRUE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Generic I/O 6 - 55

Input/Output 6 used for Open Protocol.

Name in SoftPLC: GENERIC_IO_6

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Integer | 1 | 8

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: TRUE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Generic I/O 7 - 56

Input/Output 7 used for Open Protocol.

Name in SoftPLC: GENERIC_IO_7

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Integer | 1 | 8

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: TRUE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Generic I/O 8 - 57

Input/Output 8 used for Open Protocol.

Name in SoftPLC: GENERIC_IO_8

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Integer | 1 | 8

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: TRUE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Generic I/O 9 - 58

Input/Output 9 used for Open Protocol.

Name in SoftPLC: GENERIC_IO_9

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Integer | 1 | 8

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: TRUE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Generic I/O 10 - 59

Input/Output 10 used for Open Protocol.

Name in SoftPLC: GENERIC_IO_10

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Integer | 1 | 8

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: TRUE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Generic Rising Edge 1 - 169

Generic Input/Output signal.

Name in SoftPLC: GENERIC_RISING_EDGE_1

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Generic Rising Edge 2 - 170

Generic Input/Output signal.

Name in SoftPLC: GENERIC_RISING_EDGE_2

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Generic Rising Edge 3 - 171

Generic Input/Output signal.

Name in SoftPLC: GENERIC_RISING_EDGE_3

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Generic Rising Edge 4 - 172

Generic Input/Output signal.

Name in SoftPLC: GENERIC_RISING_EDGE_4

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Generic Rising Edge 5 - 173

Generic Input/Output signal.

Name in SoftPLC: GENERIC_RISING_EDGE_5

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Generic Rising Edge 6 - 174

Generic Input/Output signal.

Name in SoftPLC: GENERIC_RISING_EDGE_6

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Generic Rising Edge 7 - 175

Generic Input/Output signal.

Name in SoftPLC: GENERIC_RISING_EDGE_7

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Generic Rising Edge 8 - 176

Generic Input/Output signal.

Name in SoftPLC: GENERIC_RISING_EDGE_8

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Generic Rising Edge 9 - 177

Generic Input/Output signal.

Name in SoftPLC: GENERIC_RISING_EDGE_9

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Generic Rising Edge 10 - 178

Generic Input/Output signal.

Name in SoftPLC: GENERIC_RISING_EDGE_10

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Input Signals: Sub-signals

Select the needed input signal to examine the related sub-signals:

- Channel Command -10054

In this Section

- Channel Command - 10054: Sub-signals

# Channel Command - 10054: Sub-signals

# Force Bolt ID

Name in SoftPLC: CHANNEL_COMMAND_FORCE_BOLT_ID

Value Type | Size Min [bit] | Size Max [bit]
--- | --- | ---
Integer | 1 | 8

# Force Pset

Name in SoftPLC: CHANNEL_COMMAND_FORCE_PSET

Value Type | Size Min [bit] | Size Max [bit]
--- | --- | ---
Integer | 1 | 8

# Inhibit No Result

Name in SoftPLC: CHANNEL_COMMAND_NO_RESULT

Value Type | Size Min [bit] | Size Max [bit]
--- | --- | ---
Boolean | 1 | 1

# Inhibit NOK Result

Name in SoftPLC: CHANNEL_COMMAND_NOK_RESULT

Value Type | Size Min [bit] | Size Max [bit]
--- | --- | ---
Boolean | 1 | 1

# Inhibit OK Result

Name in SoftPLC: CHANNEL_COMMAND_OK_RESULT

Value Type | Size Min [bit] | Size Max [bit]
--- | --- | ---
Boolean | 1 | 1

# Continue Step

If in a Wait tightening step with the condition Signal configured as Wait Type, through the sub-signal Continue Step, it is possible to control tools individually and let the tightening continue.

For more information, see the input signal Continue Step - 10128.

Name in SoftPLC: CHANNEL_COMMAND_CONTINUE_STEP

Value Type | Start bit | Length | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Boolean | 3 | 1 | 1 | 1

# Output Signals: Sub-signals

Select the needed output signal to examine the related sub-signals:

- Bolt Tightening Status - 79

- Channel Tightening Status - 80

- Channel Hardware Status - 81

In this Section

- Bolt Tightening Status - 79: Sub-signals
- Channel Tightening Status - 80: Sub-signals
- Channel Hardware Status - 81: Sub-signals

# Bolt Tightening Status - 79: Sub-signals

# All Signals

Name in SoftPLC: CYCLE_STATUS_ALL

Value Type | Size Min [bit] | Size Max [bit]
--- | --- | ---
Integer | 1 | 32

# Cycle Running

Name in SoftPLC: CYCLE_STATUS_RUNNING

Value Type | Size Min [bit] | Size Max [bit]
--- | --- | ---
Boolean | 1 | 1

# In Selected Mode

Name in SoftPLC: CYCLE_STATUS_IN_SELECTED_MODE

Value Type | Size Min [bit] | Size Max [bit]
--- | --- | ---
Boolean | 1 | 1

# Inhibited

Name in SoftPLC: CYCLE_STATUS_INHIBITED

Value Type | Size Min [bit] | Size Max [bit]
--- | --- | ---
Boolean | 1 | 1

# Last Cycle Angle High

Name in SoftPLC: CYCLE_STATUS_LAST_CYCLE_ANGLE_HIGH

Value Type | Size Min [bit] | Size Max [bit]
--- | --- | ---
Boolean | 1 | 1

# Last Cycle Angle Low

Name in SoftPLC: CYCLE_STATUS_LAST_CYCLE_ANGLE_LOW

Value Type | Size Min [bit] | Size Max [bit]
--- | --- | ---
Boolean | 1 | 1

# Last Cycle Hardware Error

Name in SoftPLC: CYCLE_STATUS_LAST_CYCLE_HW_ERROR

Value Type | Size Min [bit] | Size Max [bit]
--- | --- | ---
Boolean | 1 | 1

# Last Cycle Inhibited

Name in SoftPLC: CYCLE_STATUS_LAST_CYCLE_INHIBITED

Value Type | Size Min [bit] | Size Max [bit]
--- | --- | ---
Boolean | 1 | 1

# Last Cycle NOK

Name in SoftPLC: CYCLE_STATUS_LAST_CYCLE_NOK

Value Type | Size Min [bit] | Size Max [bit]
--- | --- | ---
Boolean | 1 | 1

# Last Cycle Not Included

Name in SoftPLC: CYCLE_STATUS_LAST_CYCLE_NOT_INCLUDED

Value Type | Size Min [bit] | Size Max [bit]
--- | --- | ---
Boolean | 1 | 1

# Last Cycle OK

Name in SoftPLC: CYCLE_STATUS_LAST_CYCLE_OK

Value Type | Size Min [bit] | Size Max [bit]
--- | --- | ---
Boolean | 1 | 1

# Last Cycle Terminated By Other

Name in SoftPLC: CYCLE_STATUS_LAST_CYCLE_TERMINATED_BY_OTHER

Value Type | Size Min [bit] | Size Max [bit]
--- | --- | ---
Boolean | 1 | 1

# Last Cycle Timeout

Name in SoftPLC: CYCLE_STATUS_LAST_CYCLE_TIMEOUT

Value Type | Size Min [bit] | Size Max [bit]
--- | --- | ---
Boolean | 1 | 1

# Last Cycle Torque High

Name in SoftPLC: CYCLE_STATUS_LAST_CYCLE_TORQUE_HIGH

Value Type | Size Min [bit] | Size Max [bit]
--- | --- | ---
Boolean | 1 | 1

# Last Cycle Torque Low

Name in SoftPLC: CYCLE_STATUS_LAST_CYCLE_TORQUE_LOW

Value Type | Size Min [bit] | Size Max [bit]
--- | --- | ---
Boolean | 1 | 1

# Last Loosening NOK

Name in SoftPLC: CYCLE_STATUS_LAST_LOOSENING_NOK

Value Type | Size Min [bit] | Size Max [bit]
--- | --- | ---
Boolean | 1 | 1

# Last Loosening OK

Name in SoftPLC: CYCLE_STATUS_LAST_LOOSENING_OK

Value Type | Size Min [bit] | Size Max [bit]
--- | --- | ---
Boolean | 1 | 1

# Last Tightening NOK

Name in SoftPLC: CYCLE_STATUS_LAST_TIGHTENING_NOK

Value Type | Size Min [bit] | Size Max [bit]
--- | --- | ---
Boolean | 1 | 1

# Last Tightening OK

Name in SoftPLC: CYCLE_STATUS_LAST_TIGHTENING_OK

Value Type | Size Min [bit] | Size Max [bit]
--- | --- | ---
Boolean | 1 | 1

# Loosening Running

Name in SoftPLC: CYCLE_STATUS_RUNNING_LOOSENING

Value Type | Size Min [bit] | Size Max [bit]
--- | --- | ---
Boolean | 1 | 1

# Running Repair

Name in SoftPLC: CYCLE_STATUS_REPAIR

Value Type | Size Min [bit] | Size Max [bit]
--- | --- | ---
Boolean | 1 | 1

# Running Termination

Name in SoftPLC: CYCLE_STATUS_TERMINATE

Value Type | Size Min [bit] | Size Max [bit]
--- | --- | ---
Boolean | 1 | 1

# Tightening Running

Name in SoftPLC: CYCLE_STATUS_RUNNING_TIGHTENING

Value Type | Size Min [bit] | Size Max [bit]
--- | --- | ---
Boolean | 1 | 1

# Tool Led Mirror Green

Name in SoftPLC: CYCLE_STATUS_TOOL_LED_MIRROR_GREEN

Value Type | Size Min [bit] | Size Max [bit]
--- | --- | ---
Boolean | 1 | 1

# Tool Led Mirror Red

Name in SoftPLC: CYCLE_STATUS_TOOL_LED_MIRROR_RED

Value Type | Size Min [bit] | Size Max [bit]
--- | --- | ---
Boolean | 1 | 1

# Tool Led Mirror Yellow

Name in SoftPLC: CYCLE_STATUS_TOOL_LED_MIRROR_YELLOW

Value Type | Size Min [bit] | Size Max [bit]
--- | --- | ---
Boolean | 1 | 1

# Waiting To Continue

If in a Wait tightening step with the condition Signal configured as Wait Type, through the sub-signal Waiting To Continue, each individual bolt shows if the related status is waiting for an input to continue.

For more information, see the output signal Waiting To Continue - 201.

Name in SoftPLC: CYCLE_STATUS_WAITING_FOR_CONTINUE

Value Type | Start bit | Length | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Boolean | 7 | 1 | 1 | 1

# Channel Tightening Status - 80: Sub-signals

# All Signals

Name in SoftPLC: CYCLE_STATUS_ALL

Value Type | Size Min [bit] | Size Max [bit]
--- | --- | ---
Integer | 1 | 32

# Cycle Running

Name in SoftPLC: CYCLE_STATUS_RUNNING

Value Type | Size Min [bit] | Size Max [bit]
--- | --- | ---
Boolean | 1 | 1

# In Selected Mode

Name in SoftPLC: CYCLE_STATUS_IN_SELECTED_MODE

Value Type | Size Min [bit] | Size Max [bit]
--- | --- | ---
Boolean | 1 | 1

# Inhibited

Name in SoftPLC: CYCLE_STATUS_INHIBITED

Value Type | Size Min [bit] | Size Max [bit]
--- | --- | ---
Boolean | 1 | 1

# Last Cycle Angle High

Name in SoftPLC: CYCLE_STATUS_LAST_CYCLE_ANGLE_HIGH

Value Type | Size Min [bit] | Size Max [bit]
--- | --- | ---
Boolean | 1 | 1

# Last Cycle Angle Low

Name in SoftPLC: CYCLE_STATUS_LAST_CYCLE_ANGLE_LOW

Value Type | Size Min [bit] | Size Max [bit]
--- | --- | ---
Boolean | 1 | 1

# Last Cycle Hardware Error

Name in SoftPLC: CYCLE_STATUS_LAST_CYCLE_HW_ERROR

Value Type | Size Min [bit] | Size Max [bit]
--- | --- | ---
Boolean | 1 | 1

# Last Cycle Inhibited

Name in SoftPLC: CYCLE_STATUS_LAST_CYCLE_INHIBITED

Value Type | Size Min [bit] | Size Max [bit]
--- | --- | ---
Boolean | 1 | 1

# Last Cycle NOK

Name in SoftPLC: CYCLE_STATUS_LAST_CYCLE_NOK

Value Type | Size Min [bit] | Size Max [bit]
--- | --- | ---
Boolean | 1 | 1

# Last Cycle Not Included

Name in SoftPLC: CYCLE_STATUS_LAST_CYCLE_NOT_INCLUDED

Value Type | Size Min [bit] | Size Max [bit]
--- | --- | ---
Boolean | 1 | 1

# Last Cycle OK

Name in SoftPLC: CYCLE_STATUS_LAST_CYCLE_OK

Value Type | Size Min [bit] | Size Max [bit]
--- | --- | ---
Boolean | 1 | 1

# Last Cycle Terminated By Other

Name in SoftPLC: CYCLE_STATUS_LAST_CYCLE_TERMINATED_BY_OTHER

Value Type | Size Min [bit] | Size Max [bit]
--- | --- | ---
Boolean | 1 | 1

# Last Cycle Timeout

Name in SoftPLC: CYCLE_STATUS_LAST_CYCLE_TIMEOUT

Value Type | Size Min [bit] | Size Max [bit]
--- | --- | ---
Boolean | 1 | 1

# Last Cycle Torque High

Name in SoftPLC: CYCLE_STATUS_LAST_CYCLE_TORQUE_HIGH

Value Type | Size Min [bit] | Size Max [bit]
--- | --- | ---
Boolean | 1 | 1

# Last Cycle Torque Low

Name in SoftPLC: CYCLE_STATUS_LAST_CYCLE_TORQUE_LOW

Value Type | Size Min [bit] | Size Max [bit]
--- | --- | ---
Boolean | 1 | 1

# Last Loosening NOK

Name in SoftPLC: CYCLE_STATUS_LAST_LOOSENING_NOK

Value Type | Size Min [bit] | Size Max [bit]
--- | --- | ---
Boolean | 1 | 1

# Last Loosening OK

Name in SoftPLC: CYCLE_STATUS_LAST_LOOSENING_OK

Value Type | Size Min [bit] | Size Max [bit]
--- | --- | ---
Boolean | 1 | 1

# Last Tightening NOK

Name in SoftPLC: CYCLE_STATUS_LAST_TIGHTENING_NOK

Value Type | Size Min [bit] | Size Max [bit]
--- | --- | ---
Boolean | 1 | 1

# Last Tightening OK

Name in SoftPLC: CYCLE_STATUS_LAST_TIGHTENING_OK

Value Type | Size Min [bit] | Size Max [bit]
--- | --- | ---
Boolean | 1 | 1

# Loosening Running

Name in SoftPLC: CYCLE_STATUS_RUNNING_LOOSENING

Value Type | Size Min [bit] | Size Max [bit]
--- | --- | ---
Boolean | 1 | 1

# Running Repair

Name in SoftPLC: CYCLE_STATUS_REPAIR

Value Type | Size Min [bit] | Size Max [bit]
--- | --- | ---
Boolean | 1 | 1

# Running Termination

Name in SoftPLC: CYCLE_STATUS_TERMINATE

Value Type | Size Min [bit] | Size Max [bit]
--- | --- | ---
Boolean | 1 | 1

# Tightening Running

Name in SoftPLC: CYCLE_STATUS_RUNNING_TIGHTENING

Value Type | Size Min [bit] | Size Max [bit]
--- | --- | ---
Boolean | 1 | 1

# Tool Led Mirror Green

Name in SoftPLC: CYCLE_STATUS_TOOL_LED_MIRROR_GREEN

Value Type | Size Min [bit] | Size Max [bit]
--- | --- | ---
Boolean | 1 | 1

# Tool Led Mirror Red

Name in SoftPLC: CYCLE_STATUS_TOOL_LED_MIRROR_RED

Value Type | Size Min [bit] | Size Max [bit]
--- | --- | ---
Boolean | 1 | 1

# Tool Led Mirror Yellow

Name in SoftPLC: CYCLE_STATUS_TOOL_LED_MIRROR_YELLOW

Value Type | Size Min [bit] | Size Max [bit]
--- | --- | ---
Boolean | 1 | 1

# Waiting To Continue

If in a Wait tightening step with the condition Signal configured as Wait Type, through the sub-signal Waiting To Continue, each individual channel shows if the related status is waiting for an input to continue.

For more information, see the output signal Waiting To Continue - 201.

Name in SoftPLC: CYCLE_STATUS_WAITING_FOR_CONTINUE

Value Type | Start bit | Length | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Boolean | 7 | 1 | 1 | 1

# Channel Hardware Status - 81: Sub-signals

# All Signals

Name in SoftPLC: CYCLE_STATUS_ALL

Value Type | Size Min [bit] | Size Max [bit]
--- | --- | ---
Integer | 1 | 32

# Drive Disconnected

Name in SoftPLC: CHANNEL_HW_STATUS_DRIVE_DISCONNECTED

Value Type | Size Min [bit] | Size Max [bit]
--- | --- | ---
Boolean | 1 | 1

# Drive Temp High

Name in SoftPLC: CHANNEL_HW_STATUS_DRIVE_TEMP_HIGH

Value Type | Size Min [bit] | Size Max [bit]
--- | --- | ---
Boolean | 1 | 1

# Drive Voltage Error

Name in SoftPLC: CHANNEL_HW_STATUS_DRIVE_VOLTAGE_ERROR

Value Type | Size Min [bit] | Size Max [bit]
--- | --- | ---
Boolean | 1 | 1

# Emergency Stop Active

Name in SoftPLC: CHANNEL_HW_STATUS_EMERGENCY_STOP_ACTIVE

Value Type | Size Min [bit] | Size Max [bit]
--- | --- | ---
Boolean | 1 | 1

# General Hardware Error

Name in SoftPLC: CHANNEL_HW_STATUS_GENERAL_ERROR

Value Type | Size Min [bit] | Size Max [bit]
--- | --- | ---
Boolean | 1 | 1

# Motortune Needed

Name in SoftPLC: CHANNEL_HW_STATUS_MOTORTUNE_NEEDED

Value Type | Size Min [bit] | Size Max [bit]
--- | --- | ---
Boolean | 1 | 1

# Tool Cable Invalid

Name in SoftPLC: CHANNEL_HW_STATUS_TOOL_CABLE_INVALID

Value Type | Size Min [bit] | Size Max [bit]
--- | --- | ---
Boolean | 1 | 1

# Tool Disconnected

Name in SoftPLC: CHANNEL_HW_STATUS_TOOL_DISCONNECTED

Value Type | Size Min [bit] | Size Max [bit]
--- | --- | ---
Boolean | 1 | 1

# Tool Temp High

Name in SoftPLC: CHANNEL_HW_STATUS_TOOL_TEMP_HIGH

Value Type | Size Min [bit] | Size Max [bit]
--- | --- | ---
Boolean | 1 | 1

# Torque Transducer Error

Name in SoftPLC: CHANNEL_HW_STATUS_TORQUE_TRANSDUCER_ERROR

Value Type | Size Min [bit] | Size Max [bit]
--- | --- | ---
Boolean | 1 | 1

# StepSync compatible tools

The following tools are supported by StepSync:

Tool Family | Supported Models
Tensor STR | ETV, ETD, ETP
Tensor ST | ETV, ETD, ETP
Tensor SL | ETV, ETD, ETP, ETF
Tensor SR | ETV, ETD, ETP
QST | All (Excluding Dual Transducer - CTT, CTA, CTTA)

# StepSync CAN Accessories

The following CAN accessories are supported by a Power Focus 6000 StepSync system:

- Internal I/O

- I/O Expander

- Operator Panel

- Stack light

- Indicator box

These accessories can only be connected to the Sync Reference. No accessories can be connected to Sync Members.

# Working with the Settings Tab

## Product Essentials Tutorials

https://www.youtube.com/watch?v=-nkc9mmzoBo

In this Section

- Configuration of the Network
- Configuration of the Protocol
- Configuration of the Preferences
- Configuration of the PIN Settings
- Configuration of the Tool Alarms
- Configuration of the Wireless Settings
- Configurations of the Events Settings
- Configuration of the Fieldbus
- Configuration of the Results
- Reset

# Configuration of the Network

The POWER FOCUS 6000 can be set up to be accessed from the Atlas Copco software ToolsTalk or from a web browser on a Local Area Network (LAN). It can also be accessed directly from a connected PC. It uses the IPv4 protocol.

To access and alter the Ethernet settings, select Edit.

Only the Factory Ethernet port can be configured. The Service Ethernet port has a designated IP address, 169.254.1.1, that must not be connected to the local network.

In this Section

- Accessing the Controller On Lan
- Accessing the Controller Through a Web GUI
- About the Firewall

# Accessing the Controller On Lan

Select the Settings menu, and click on Edit to access the Factory Ethernet port window. There you can alter the Ethernet settings.

Connect the network cable to the Factory Ethernet port and then either manually specify the required information or, if available, use the information provided by the DHCP server. Required information is:

- IP address

- Subnet mask

- Gateway

This information is provided by the local system administrator.

When using the manual option there are optional settings available for the use of DNS servers.

# Accessing the Controller Through a Web GUI

Connect the PC with a straight-through Ethernet cable (RJ45) to the Service Ethernet port. Access the controller with the IP address from a web browser.

# About the Firewall

The POWER FOCUS 6000 can be set up to use a firewall. The firewall is based on the trusted host principle, and only allows incoming connections via ports that are enabled, or addresses that are white-listed.

By default, the firewall is disabled.

The firewall applies only to incoming connections on the Factory Ethernet Port.

## Activating and configuring the firewall

To activate and configure the firewall, select Edit.

In the top container, activate the general firewall feature by setting it to On.
In the remaining containers, configure any of the following firewall layers:

- Port Filtering (layer 4 firewall). Opening a service on the controller - you can specify which services are reachable through the firewall.

- IP Filtering (layer 3 firewall). Specifying a trusted host by IP- you can specify an IP that is considered trusted on the network and can access all the services.

- MAC Filtering (layer 2 firewall). Specifying a trusted host by MAC.

When activating the general firewall feature, Port Filtering (layer 4 firewall) and all its predefined services are enabled by default.

A connection is allowed, when any of the firewall layers accepts it. When no firewall layer is enabled, all incoming connections are allowed through.

Further firewall configuring is done by enabling/disabling connections through the predefined services specified, by adding TCP or UDP ports manually and/or by white-listing IP/MAC addresses.

## Port Filtering (layer 4 firewall)

When Port Filtering (layer 4 firewall) sets Firewall rules, and TCP and UDP ports.

Port Filtering (layer 4 firewall) can be turned ON or OFF.
When Port Filtering (layer 4 firewall) is ON, the firewall is performing packet filtering based on destination port, and packets sent to an open port are immediately accepted. Non-matching packets are also processed by the other firewall types (IP Filtering and MAC Filtering) before being eventually rejected.
When Port Filtering (layer 4 firewall) is OFF, port filtering is disabled and all the other settings are hidden.

Predefined services have their own enable-switches:

- Open ports for web services (TCP 80, TCP 8080)

- Open ports for SSH and SFTP (TCP 22)

- Open ports for wireless tools (UDP 6677, TCP 6678)

- Open ports for accessories (TCP 25000)

- Additional TCP ports

- Additional UDP ports

Predefined service | Description
--- | ---
Open ports for web (TCP 80, TCP 8080) | Ports required for web services so the controller is accessible over the factory network. Setting Open ports for web (TCP 80, TCP 8080) to Off, triggers a warning that the connection with the Web HMI can be lost.
Open ports for SSH and SFTP (TCP 22) | Port required for SSH and SFTP functionality on the Factory Ethernet Port.
Open ports for wireless tools (UDP 6677, TCP 6678) | Ports required for wireless tools to connect to the controller over the factory network.
Open ports for accessories (TCP 25000) | Ports required for accessories to communicate with the controller over the factory network. This applies to Socket Selector 6.
Open additional TCP ports | Accepted are both comma-separated ports and port ranges using a dash (-). Example: when entering 1,2,3,4-10, all ports between 1 and 10 are opened. Invalid port entries trigger an immediate pop-up warning. Ports are automatically sorted after pressing the Apply button.
Open additional UDP ports

When using Open Protocol, the ports to be opened must be added manually in the Open additional TCP ports entry box. For example: 4545,4546,4547 (depending on the ports configured in Virtual Station > Virtual Station 1 > Protocols > Open Protocol > Server Port).

When using an NTP server, port 123 must be added manually in the Open additional UDP ports entry box.

Multiple ports can be added by using comma separation. Port ranges can be added by using a dash.

## IP Filtering (layer 3 firewall)

IP Filtering (layer 3 firewall) allows specifying trusted hosts or networks by entering their IP addresses in the IP White List entry box. To access the entry box, set the switch to On. Accepted entries are lists of IP addresses or network addresses in the form of IP tables, that is, host IP addresses or network IP addresses. The network mask can be entered as mask length (for example, /24) or as network IP address (for example, /255.255.255.0). Packets coming from a white-listed IP address are immediately allowed. Other packets are screened by the other firewall layers (Port Filtering and MAC Filtering).

IP address white-list example

Due to security issues, entering host names or network names is not accepted.

Note that processes like NATing (Network Address Translation) may change source IP addresses. Consult your local network administrator when white-listing a host based on source IP address is required.

## MAC Filtering (layer 2 firewall)

MAC Filtering (layer 2 firewall) allows specifying trusted hosts or networks by entering their MAC addresses in the MAC White List entry box. To access the entry box, set the switch to On. Accepted entries are comma-separated lists of MAC addresses. Packets coming from a whitelisted MAC address are immediately allowed. Other packets are screened by the other firewall layers (Port Filtering and IP Filtering).

MAC address white-list example

Invalid entries trigger an immediate pop-up warning.

Note that routing may change source MAC addresses. Consult your local network administrator when white-listing a host based on source MAC address is required.

## Packet counters

To display the Firewall statistics for each firewall layer, select Settings > Network > Firewall - Packet Counters.

The Update section includes the following buttons:

- Refresh – used to refresh the displayed packet counters.

- Reset – used to reset the packet counters to zero.

Both buttons are implemented with a switch that automatically resets itself to the original position after performing the action.

The Accepted Packet Counters section displays the counters for each of the firewall types and for rejected packets.

- Port Filtering – displays the packet counter for packets accepted by the Port Filtering firewall type.

- IP Filtering – displays the packet counter for packets accepted by the IP Filtering firewall type.

- MAC Filtering – displays the packet counter for packets accepted by the MAC Filtering firewall type.

- Rejected – displays the packet counter for packet that were rejected.

The packets accepted, and thus counted, by the Port, IP and MAC Filtering rules only include the initial packets that establish a connection.

The Rejected packets are all counted and displayed.

## Firewall status

The status of the general firewall feature and its firewall layers is shown in the Firewall main view directly under Settings > Network.

Status | Description
--- | ---
OK | The firewall is enabled and the firewall configuration is applied.
Disabled | The firewall is disabled and the firewall configuration is not applied.
Configuration Error | The firewall is enabled, but the firewall configuration is not applied due to an internal error. For safety reasons, the fail-open policy is applied, meaning all connections are allowed through.

When the general firewall status is OK, the status (Enabled / Disabled) for the respective firewall layers is also shown.

# Configuration of the Protocol

The POWER FOCUS 6000 can be set up to communicate with servers running an Atlas Copco license manager as well as the two Atlas Copco softwares ToolsTalk and ToolsNet. ToolsTalk is used to configure one or several controllers. ToolsNet is used to handle result reporting.

In this Section

- Configuring the ToolsTalk Connection
- Configuring the ToolsNet Connection
- Configuring a License Manager

# Configuring the ToolsTalk Connection

To connect a controller to ToolsTalk, configure and activate the ToolsTalk protocol settings on the controller.

1. On the Home view, select the Settings Tab. Then, on the left, select Server Connections.

2. In the ToolsTalk window, set the following parameters:

   Field | Description
   --- | ---
   On/Off | Enables/Disables communication with the ToolsTalk server
   Server port | ToolsTalk server port
   Server host | ToolsTalk server IP address

3. Select Apply.

To view the ToolsTalk connection status, select the Results icon and go to the Live Results view. Then, select the button. In the appearing dialog box, select the Server connections tab.

For information on how to configure ToolsTalk, refer to the ToolsTalk 2 User Guide.

## Product Essentials Tutorials

https://www.youtube.com/watch?v=bfznoHhYLvI

Relevant Information

- Viewing Protocol Status

# Configuring the ToolsNet Connection

To connect a controller to ToolsNet and collect tightening results, configure and activate the ToolsNet protocol settings on the controller.

1. On the Home view, select the Settings Tab. Then, on the left, select Server Connections.

2. In the ToolsNet window, set the following parameters:

   Field | Description
   --- | ---
   On/Off | Enables/Disables communication with the ToolsNet server
   Server port | ToolsNet server port
   Server host | ToolsNet server IP address

3. Select Apply.

To view the ToolsNet connection status, select the Results icon and go to the Live Results view. Then, select the button. In the appearing dialog box, select the Server connections tab.

For information on how to configure ToolsNet, refer to the ToolsNet 8 User Guide.

Relevant Information

- Viewing Protocol Status

# Configuring a License Manager

The Atlas Copco license manager is connected to a controller and the protocol settings are activated on the controller from the Server connections tab in the Settings menu.

Field | Description
--- | ---
On/Off | Enables/Disables communication with the Atlas Copco license manager.
Server host | Atlas Copco license manager server IP address
Server port | Atlas Copco license manager server port

# Configuration of the Preferences

Preferences contains general settings such as date and time, language, torque unit, and startup screen.

In this Section

- Configuring the Date and Time
- Configuring the Displayed Controller Language
- Configuring the Displayed Torque Unit
- Configuring the Startup Screen

# Configuring the Date and Time

Date and time must be set in order for events and results to get the correct time stamp for when they occurred.

9007201068760971

The time is retrieved from one of three available sources:

- Manual

- NTP

- ToolsNet

When the source is set to Manual the date, time, and time zone are set manually.

When the source is set to NTP, the date and time is retrieved from an NTP server defined in the GUI.

When the source is set to ToolsNet, the date and time is retrieved fron the ToolsNet server.

Parameters to set date and time
Field | Description
--- | ---
Source | Source to retrieve the time from.
Date | Date entered manually if the source is set to manual.
Time | Time entered manually if the source is set to manual.
Time zone | The time zone; either the location or a standard time zone such as UTC (coordinated universal time)
NTP Server | IP-address of an NTP server providing date and time for the controller.

# Configuring the Displayed Controller Language

The controller GUI is translated into twelve languages. To change the language of the GUI:

1. Tap or click on the arrow beside the name of the language currently in use.

2. Choose a language from the list.

The language change will take effect immediately.

Available GUI languages
Language | As displayed in controller
--- | ---
English | English
Czech | Čeština
German | Deutsch
Spanish | Español
French | Français
Korean | 한국어
Italian | Italiano
Japanese | 日本語
Portuguese | Português
Russian | Русский
Swedish | Svenska
Chinese | 中文

# Configuring the Displayed Torque Unit

Choose the unit to use for torque values and results. Torque results are displayed in the chosen unit both after a tightening is performed and when stored in the results list.

To change the torque unit used in the controller GUI:

1. Tap or click on the arrow beside the name of the unit currently in use.

2. Choose a unit from the list.

The torque unit change will take effect immediately.

Available torque units
Unit | Description
--- | ---
cNm | centinewton metre
dNm | decinewton metre
Nm | newton metre
kNm | kilonewton metre
in·lbf | inch-pound force
ft·lbf | foot-pound force
in·ozf | inch ounce-force
ft·ozf | foot ounce-force
gf·cm | gram-force centimetre
kgf·cm | kilogram-force centimetre
kgf·m | kilogram-force metre

# Configuring the Startup Screen

The default screen at startup of the controller is the Home screen. It is possible to change startup screen to the Result screen.

A change of startup screen in the settings requires a restart of the controller or a refresh of the web GUI.

# Configuration of the PIN Settings

The PIN code prevents unauthorized usage of the controller or accidental changes.

If enabled, a PIN code is required when accessing the controller either from the controller-GUI or Web-GUI.

In this Section

- Configuring the PIN

# Configuring the PIN

It is possible to have one or many different PIN configurations on the controller. Users can decide whether or not to activate one or several PIN configurations at the same time.

Each PIN configuration has a PIN code, a user name, a switch for enabling or disabling the user/PIN, and a list of available configurations that the user can access.

When PIN is enabled and the screen is locked, a locked padlock icon is shown at the upper-right corner of the GUI. The user can access and make changes only to the selected configuration(s) without entering any PIN code, and browse the unselected configurations with read-only access only. The unselected configurations are greyed out or disabled.

The screen lock goes automatically on after a certain time of inactivity, configurable by the user.
The minimum value of the inactivity time is 20 sec and the maximum value is 600 sec. The inactivity time is configurable and applies to all PIN configurations.

After a system startup, the controller is locked if the PIN is turned on, regardless of the current inactivity time.

The users and PIN configured apply also to the Service Port (169.254.1.1).
To enable PIN protection on the Service Port, in the PIN windows, set Use PIN for Service Port to On.

Each controller can configure up to 10 users.
The PIN of each configuration has to be unique. It is required to have at least one configuration to enable the PIN functionality on the controller.

The PIN can be configured from the Embedded controller-GUI, Web-based controller-GUI or Tools Talk 2.

## Adding New Users

1. On the Home view, select the Settings Tab. Then, on the left, select PIN.

2. In the PIN window, select Configure.

3. Select the Plus icon at the upper-right corner of the GUI.
   The PIN-Users window shows the new user. If there are not users stored in the controller, the new user is the first and only one in the list; if there are existing users stored in the controller, the new user is the last of the list.

4. Select the new user.
   The User window appears.
   Enter the Name and the PIN of the new user, and then confirm the PIN.

   The User Name must be unique.
   The Name text box can be 1 to 32 characters long.

   The PIN code must have 4 digits in length (numbers 1 through 9).
   Enter PIN box and Confirm PIN box need to match for the changes to be applied. By default, dots are indicated in both the text box, but these are just placeholders and need to be replaced with actual PIN codes.

5. Select Permissions. The list of the available configurations appears.
   Select the check box at the left of the necessary configuration(s) the user can access and make changes.
   After selecting the necessary configuration(s), select OK.
   The User window appears.

   Select all selects all the available configurations at the same time.
   Select Deselect all to clear the check boxes and undo the selection.

   The user can access and make changes only to the configuration(s) selected in the Permissions window, and browse the unselected configurations with read-only access. For the unselected configurations, no changes are allowed.

6. In the User window, select Apply.

## Enabling Users

1. On the Home view, select the Settings Tab. Then, on the left, select PIN.

2. In the PIN window, select Configure.

3. In the PIN-Users window, select the check box at the left of the user name to be enabled.

   PIN can also be enabled by clicking on the user name and setting - in the User window - the Enabled switch to On.

## Activating the PIN configuration

1. On the Home view, select the Settings Tab. Then, on the left, select PIN.

2. In the PIN window, select Configure.

3. In the PIN-activating window, set the PIN Code switch to On.

   The PIN can only be activated when at least one user/PIN is enabled. If no user/PIN is enabled, a Warning pop-up window appears.

4. Enter the Inactivity Timeout (in seconds), that defines the slot of time after which the screen is automatically locked up.

   Default value for Inactivity Timeout is 120 seconds: this is a global setting, and cannot be set on a per user basis.

## Unlocking the controller-GUI or Web-GUI

1. On the Home view, select the Padlock icon at the upper-right corner of the GUI. A pop-up window with a numeric keypad appears.

2. Enter the configured PIN code and select OK.

   When the PIN is enabled and the screen has been unlocked, an Open Padlock icon appears at the upper-right corner of the GUI. The controller-GUI or Web-GUI can be locked again manually, by selecting the Open Padlock icon.

## Disabling Users

1. On the Home view, select the Settings Tab. Then, on the left, select PIN.

2. In the PIN window, select Configure.

3. In the PIN-Users window, deselect the check box at the left of the user name to be disabled.

   PIN can also be disabled by clicking on the user name and setting - in the User window - the Enabled switch to Off.

## Deleting Users

1. On the Home view, select the Settings Tab. Then, on the left, select PIN.

2. In the PIN window, select Configure.

3. In the PIN-Users window, select the Delete icon at the right of the user name to be deleted.

   If the User is removed, also the PIN is deleted. It is not possible to access any configuration through the deleted PIN.

# Configuration of the Tool Alarms

Alarms are set to control when to perform maintenance or calibration on the tools connected to the controller.

The tool service interval and other information are found in the tool view on the Tool menu.

Different tool alarms
Field | Description
--- | ---
Service indicator alarm | Enables an alarm for when the service interval for the tool is reached.
Tool lock after alarm | Lock the tool when the service interval is reached.
Calibration alarm | Enables the tool calibration alarm for all tools connected to the controller.

# Configuration of the Wireless Settings

The Wireless settings in the controller activates the use of a WLAN and Bluetooth.

1. In the Settings menu, select the Wireless tab.

2. Depending on your tool (WLAN-equipped tools are marked IRC-W, while Bluetooth-equipped tools are marked IRC-B) set Enabled to On.

# Configurations of the Events Settings

It is possible to configure the events available in the controller as either or several of:

- Acknowledged

- Logged

- Displayed

# Configuration of the Fieldbus

The fieldbus section consists of information about the fieldbus type in use. This part is hardware dependent and read-only. The configuration section with general settings for the fieldbus in use is possible to edit.

The fieldbus mapping and the assigning of fieldbus maps to virtual stations are done with ToolsTalk. For more information refer to the ToolsTalk configurations manual.

In this Section

- Creating a General Fieldbus Configuration

# Creating a General Fieldbus Configuration

When a new fieldbus module is installed in the controller, General Fieldbus Configuration settings can be setup directly via the GUI, without the need of using ToolsTalk 2.

For configurations related to the fieldbus frame and connecting a fieldbus configuration to a Virtual Station, ToolsTalk 2 will still be needed.

1. Go to the Settings menu, and then select Fieldbus.

2. Select the Create Config button.

   If no Fieldbus module is installed this button will not be visible.

3. Configure the following parameters:

   - Set by network: OFF/ON

   - Read result handshake: OFF/ON

   - Lock tool when fieldbus offline: OFF/ON

   - Sync on task selected: OFF/ON

     - OFF - Task changes made in the Virtual Station are ignored.

     - YES - Task changes made in the Virtual Station are synced with the Fieldbus module.

4. Depending on the installed module type, enter the Fieldbus communication specific settings:

   - IP Address

   - Subnet mask

   - Gateway

5. A new Configuration is created.

If a Fieldbus configuration already exists on the controller, this will have to be removed before creating a new configuration. When the configuration has been removed, instead of a Remove button there will be a Create Config button.

# Configuration of the Results

The Results menu allows the user to configure the label names for results displayed in the Results list.

## Changing Result Status names

1. Go to Settings, then Results, and click on Customized detailed status.

2. Find the Status name you want to alter.

3. Write the new name in the corresponding field in the New status name on the right.

# Reset

# Factory Reset Controller

It is possible to undo the controller to the original factory settings.

All settings, events, configurations and historical data are deleted when the controller is reset. Do a factory reset only when you are completely sure that this is required.

## Performing a Controller Factory Reset

1. On the Home view, select the Settings Tab. Then, on the left, select Reset.

2. In the Factory Reset Controller window, select Reset.

   A pop-up window appears warning that all data will be deleted. Then, select Yes.

   The controller restarts to activate the new settings.

# Clear Results

It is possible to delete results and events stored on the controller.

## Deleting Results and Events

1. On the Home view, select the Settings Tab. Then, on the left, select Reset.

2. In the Clear Results window, select Clear.

   A pop-up window appears warning that all results and events will be deleted. Then, select Yes.

3. Turn off the controller and wait for 30 seconds before turning it on again.

# Operation

In this section, you can find step-by-step information about how to operate the product.

In this Section

- Remote Start and Emergency Stop
- DIG IN/OUT Connectors

# Remote Start and Emergency Stop

# Remote Start Configuration

A tightening can be started remotely from an accessory in both single and multiple controller configurations. The switch to activate remote start is found on the connector panel located behind the front access door of the controller.

Whenever using remote start you must enable an emergency stop solution for safety reasons. For more information about emergency stop, see Emergency stop (EM Stop) in the product instructions for POWER FOCUS 6000.

When using a tool with some type of safety handle (such as a trigger start button or a safety lever), remote start must be disabled by setting the switch to Off. This is done to ensure that it is not possible to override the safety function within the tool.

Relevant Information

- Single Controller without Emergency Stop Button

# Emergency Stop

The supply disconnecting device may serve as an emergency stop when it is readily accessible to the operator and it is of the type described in EN 60204-1:2006, 5.3.2 a), b), c) or d). When intended for such use, the supply disconnecting device shall be colored red and have a yellow background. (Ref. EN 60204-1:2006, 10.7.5).

The POWER FOCUS 6000 provides an infrastructure to build an Emergency Stop function with redundant breaking according to EN ISO 13849-1 category 3 PL d. The Emergency Stop function must be used when using remote start functionality.

The Emergency Stop functionality can be used with a supply-disconnecting device (such as an Emergency Stop button). When the Emergency Stop button is activated, it breaks the supply voltage to the controller.

A diagnose of the system is run automatically at the start of the controller. This is done both after an emergency stop and at a normal start.

The Emergency Stop function is used with either a single controller or up to 10 controllers in a single emergency stop chain. In a multiple controller configuration, the Emergency Stop signal is distributed from the first controller to all interconnected controllers using the I/O bus interface. The last controller in the chain returns a feedback signal to indicate that all controllers have received the Emergency Stop signal. The event Emergency Stop is displayed.

For the Emergency Stop there is a 24V DC output through the Emergency Stop interface on the connector panel.

In this Section

- Cabling
- Pin Configurations for Emergency Stop

# Cabling

# Emergency Stop Button Cables

Cable dimensions for the emergency stop button
Single/Multiple controllers | Dimension | Maximum length
--- | --- | ---
Single | 0.7 mm2 cable | 400 meters
Multiple | 1.5 mm2 cable | 50 meters

# I/O Cables

For connecting multiple controllers with I/O cables distributing the emergency stop signal, observe the maximum length according to the following table:

Cable dimensions for I/O cables
AWG 22 cable | Maximum total length
--- | ---
4 controllers | 200 meters
5 controllers | 140 meters
6 controllers | 100 meters
8 controllers | 70 meters
10 controller | 50 meters

# Pin Configurations for Emergency Stop

The Power Focus has an external EM Stop interface and I/O bus on the connector panel located behind the front access door.

The PIN configuration differs depending on whether it is a single or multiple controller solution. Furthermore, for the single controller, the PIN configuration differs depending on whether the controller is equipped with an EM Stop button or not.

The following sections describe the available PINs on the connecting panel, and the use of the different PINs to connect an EM Stop button.

In this Section

- Single Controller with Emergency Stop Button
- Single Controller without Emergency Stop Button
- Multiple Controllers with Emergency Stop Buttons

# Single Controller with Emergency Stop Button

Connector: Phoenix, 6-pin Headers 3.5mm pitch

Use the following pins to attach an EM Stop button:
Pin | Use |
--- | --- | ---
1 | Do not use | Connections for a single controller
2 | Do not use
3 | Attach an emergency button between pin 3 and pin 4
4 | See pin 3
5 | Attach an emergency button between pin 5 and pin 6
6 | See pin 5
7 | Connect a jumper between pin 7 and pin 8
8 | See pin 7
9 | Connect a jumper between pin 9 and pin 10
10 | See pin 9

# Single Controller without Emergency Stop Button

Connector: Phoenix, 6-pin Headers 3.5mm pitch

WARNING

Remote start switch must be set to OFF for this configuration

Use the following PIN configuration:
Pin | Use |
--- | --- | ---
1 | Do not use | Connections with no EM stop
2 | Do not use
3 | Connect a jumper between pin 3 and pin 4
4 | See pin 3
5 | Connect a jumper between pin 5 and pin 6
6 | See pin 5
7 | Connect a jumper between pin 7 and pin 8
8 | See pin 7
9 | Connect a jumper between pin 9 and pin 10
10 | See pin 9

# Multiple Controllers with Emergency Stop Buttons

The PIN configuration differs depending on the location of the controller in the EM Stop chain.

In this Section

- First Controller with an Emergency Stop Button Connected
- Controllers Between First and Last
- Last Controller

# First Controller with an Emergency Stop Button Connected

EM Stop button connector: Phoenix, 6-pin Headers 3.5mm pitch

EM Stop I/O cable connector: Molex Micro-Fit, 5-pin

Use the following pin configuration:
Pin | Use |
--- | --- | ---
1 | Do not use | Connections for the first controller
2 | Do not use
3 | Attach an emergency button between pin 3 and pin 4
4 | See pin 3
5 | Attach an emergency button between pin 5 and pin 6
6 | See pin 5
7 | Connect a jumper between pin 7 and pin 8
8 | See pin 7
9 | Do not use
10 | Do not use

# Controllers Between First and Last

EM Stop I/O cable connector: Molex Micro-Fit, 5-pin

Remove plug or use the following pin configuration:

Pin | Use |
--- | --- | ---
1 | Do not use | Connections for middle controllers
2 | Do not use
3 | Do not use
4 | Do not use
5 | Do not use
6 | Do not use
7 | Do not use
8 | Do not use
9 | Do not use
10 | Do not use

# Last Controller

EM Stop I/O cable connector: Molex Micro-Fit, 5-pin

Use the following pin configuration:
Pin | Use |
--- | --- | ---
1 | Do not use | Connections for last controller
2 | Do not use
3 | Do not use
4 | Do not use
5 | Do not use
6 | Do not use
7 | Do not use
8 | Do not use
9 | Connect a jumper between pin 9 and pin 10
10 | See pin 9

# DIG IN/OUT Connectors

The POWER FOCUS 6000 uses the same hardware accessories (Stacklight, Operator panel etc.) as the Power Focus 4000 system. However, the digital input and output connectors are configured differently and use a different plug. In order to rewire the plug from Power Focus 4000 to POWER FOCUS 6000 correctly, use the connector descriptions in the following sections.

In this Section

- Digital Output Connectors
- Digital Input Connectors

# Digital Output Connectors

The POWER FOCUS 6000 has a connector with four configurable internal digital outputs (DIG OUT) that are located behind the front access door.

In this Section

- Digital Output Connector
- Digital Output Connector for Power Focus 4000

# Digital Output Connector

For the POWER FOCUS 6000.

Pin | Relay | Function |
--- | --- | --- | ---
1 |  | Normally closed | Connectors for output
2 | Relay 1 | Common
3 |  | Normally open
4 |  | Normally closed
5 | Relay 2 | Common
6 |  | Normally open
7 |  | Normally closed
8 | Relay 3 | Common
9 |  | Normally open
10 |  | Normally closed
11 | Relay 4 | Common
12 |  | Normally open

# Digital Output Connector for Power Focus 4000

Pin | Relay | Function |
--- | --- | --- | ---
12 |  | Normally closed | Connectors for output
11 | Relay 4 | Common
10 |  | Normally open
9 |  | Normally closed
8 | Relay 3 | Common
7 |  | Normally open
6 |  | Normally closed
5 | Relay 2 | Common
4 |  | Normally open
3 |  | Normally closed
2 | Relay 1 | Common
1 |  | Normally open

# Digital Input Connectors

The POWER FOCUS 6000 has a connector with four configurable internal digital inputs (DIG IN) that are located behind the front access door.

In this Section

- Digital Input Connector
- Digital Input Connector for Power Focus 4000

# Digital Input Connector

For POWER FOCUS 6000.

Pin | Function |
--- | --- | ---
13 | 24V |
14 | 24V
15 | 0V
16 | 0V
17 | 0V
18 | Digital input -
19 | Digital input 1 +
20 | Digital input 2 +
21 | Digital input 3 +
22 | Digital input 4 +

# Digital Input Connector for Power Focus 4000

Pin | Function |
--- | --- | ---
22 | GND (+24VDC isolated) |
21 | +24VDC isolated
20 | Digital input 4 -
19 | Digital input 4 +
18 | Digital input 3 -
17 | Digital input 3 +
16 | Digital input 2 -
15 | Digital input 2 +
14 | Digital input 1 -
13 | Digital input 1 +

# Reports and Statistics

In this section, you can learn about available reports and statistics.

In this Section

- Working with the Reports Tab

# Working with the Reports Tab

# Results

This section describes how to access tightening results on the POWER FOCUS 6000 controller and how to read the information given in the different result views. It describes both the live results view available after each tightening and the historical results view available in Results on the Reports menu.

When a tightening is performed, the results are stored on the controller. Results can also be sent to an external system such as ToolsNet or exported for analysis using the export function.

Relevant Information

- Export/Import

In this Section

- Live Results
- Stored Results

# Live Results

The Live Results pop up window shows results from the different virtual stations on the controller in the upper four as well as the lower four panes. The reason for this is that you can choose two different result views for the same virtual station to be shown at the same time.

Select a result pane to open a window where you can step through the different result views by clicking the arrows at the side of the result window.

## Result View - Numbers

The first window will display the result in numbers.

Point and click at items on image to see if there is more information:

A | Virtual station name
B | Batch sequence name
C | Batches in sequence An OK batch is colored green. An ongoing batch is colored yellow. An NOK batch is colored red.
D | Tightenings in batch An OK tightening is colored green. An ongoing tightening is colored yellow. An NOK tightening is colored red.
E | Result status An NOK tightening will give a detailed status of the unsuccessful tightening.
F | Target torque/angle
G | Tightening program name
H | Number of completed batches in sequence
J | Number of completed tightenings in a batch
K | Tightening result

## Result View - High-Low Result

The graphic display shows whether the result is high, low or within the set limits.

Point and click at items on image to see if there is more information:

A | Graphic display showing if the tightening result is too high or too low with respect to the given limits for the tightening program. Torque value.
B | Result status
C | Angle value

If the tightening is NOK, a detailed reason will be given.

## Result View - Extensive Results

The extensive results views will display some additional tightening results.

The second view always shows the identifiers (VIN). If the first screen is already full with parameters, the rest of the parameters are shown on the second screen.

## Result View - Identifier Strings

This result view shows the identifier strings included in a multiple barcode scan.

## Result View - Trace

With the trace result view, one can learn better how the tightening behaves, in order to make adjustments to the tightening program. Depending on the tightening strategy, the trace will display different tightening parameters.

The trace result is available as two different graphs: torque/time and torque/angle.

## Result View - Result Reporter

The list shows the values from the result reporters. If there is a result reporter defined for a program monitor/restriction, the value from that monitor/restriction is reported. If there is no result reporter defined for a program monitor/restriction, the value from the latest executed result reporter in main path is reported.

Evaluation order if several reporters of the same type are defined in a program:

1. result reporter on program monitor/program restriction.

2. result reporter on monitor/restriction of the last executed step in main path.

Values on the highest level of the multistep result set by the corresponding result reporter:

- final angle set by result reporter final angle

- final torque set by result reporter final torque

- current set by result reporter current

In this Section

- Viewing Protocol Status

# Viewing Protocol Status

1. On the Home view, select the Results icon and go to the Live Results view.

2. At the upper-right corner, select the button. The Protocol Status dialog box appears.

3. The tabs in the dialog box show the following information:

   Tab | Description
   --- | ---
   Open Protocol | Shows the status of the open protocol connection: OK / NOK
   Server Connections | Shows the status of the connections to ToolsTalk and ToolsNet servers: OK / NOK To change the configuration setting Enabled / Disabled, go to Settings > Server Connections and select the server to configure.
   Launcher Status | Shows the launcher status of the different system adapters: OK / NOK

4. Select Close.

Relevant Information

- Configuring the ToolsNet Connection
- Configuring the ToolsTalk Connection

# Stored Results

The controller stores the result for every tightening or loosening performed.

## Showing Stored Results

1. On the Home view, select the Reports Tab. On the left side, Results is automatically selected.

2. In the Results window, select View all results.
   The results list shows with the following information:

   - Date: date and time of the tightening performed.

   - Virtual Station: Virtual Station which the tightening was performed with.

   - Tightening Program: Tightening Program column shows Multistep Tightening Program name, or Batch Sequence name followed by the Tightening Program name within the Batch Sequence.

   - Result: Torque / Angle result.

   - Limits: Limits column shows values only when the user sets Step Monitor or Step Restriction, or Program Monitor or Program Restrictions.

     Step Monitors, Step Restrictions, Program Monitors and Program Restrictions are applicable for Final Torque and Final Angle.

   - Details: Tightening / loosening result details.

   - Trace checkbox: By selecting a trace checkbox the corresponding result will be shown in the Sync trace result view.

In the Limits column, the minimum / maximum value can be red colored.
In this case, the red colored value means that any of the following has occurred:

- The measured value is lower than the minimum value set in the Multistep Program.

- The measured value is higher than the maximum value set in the Tightening Program.

## Showing and Reading Result Traces

1. On the Home view, select the Reports Tab. On the left side, Results is automatically selected.

2. In the Results window, select View all results.
   The results list shows in the Results window.

3. Select the necessary result.
   The tightening trace shows in the Trace Result View window.

Trace Result View window shows, step by step, the tightening life-cycle.
When the tightening is NOK, Trace Result View window shows which Step Monitor or Step Restriction caused it.
On the trace graph, the Step Monitor or Step Restriction that caused the NOK tightening in the Step level, is red colored.

On the upper-right corner of the trace graph, select the left-arrow / right-arrow to show the necessary trace graph.
The following trace graphs are available:

- Torque / Time

- Torque / Angle

- Angle / Time

- Speed / Time

- Speed / Angle

- Gradient / Time (when the tightening program is configured to make a gradient trace)

- Gradient / Angle (when the tightening program is configured to make a gradient trace)

- Current / Time

- Current / Angle

Step lines are upon the trace graph.

On the trace graph, it is possible to zoom in/out, move the trace, and read x-axis and y-axis values on a specific point.
On the lower-left corner of the trace graph, select "+" to zoom in , "-" to zoom out, or the "square icon" to reset the zoom level back to the default view.

On the lower part of the Trace Result View window, select the necessary step to open a pop up window with the detailed step information.

Relevant Information

- Step Monitors
- Step Restrictions
- Tightening Steps

In this Section

- Viewing Synchronized Traces

# Viewing Synchronized Traces

Synchronizing traces older than software version 3.5 is not supported.

Synchronize and compare traces

1. On the Home view, select the Reports Tab. On the left side, Results is automatically selected.

2. In the Results window, select View all results.

3. Select the traces to compare by marking the icon of the corresponding results. A selected trace icon turns blue.

   Up to 10 traces can be selected.

   Results without the icon do not support synchronization.

4. Select the icon in the upper right hand corner, to open the sync trace view. When selecting the icon all selected result traces will be unchecked.

5. In the Sync Trace Result View, select the preferred Sync method from the drop-down list.

   Select the trace types with the arrows in the upper right hand corner.

The Sync Trace Result View is shown below:

Point and click at items on image to see if there is more information:

Position | Description
--- | ---
1 | Select method to synchronize traces and display of current sync method.
2 | Switch between available trace types. The following trace graphs are available: Torque / Time Torque / Angle Angle / Time Speed / Time Speed / Angle Gradient / Time (when the tightening program is configured to make a gradient trace) Gradient / Angle (when the tightening program is configured to make a gradient trace) Current / Time Current / Angle
3 | Zoom methods to examine sections of the traces in more detail. Select "+" to zoom in , "-" to zoom out, or the "square icon" to reset the zoom level back to the default view. It is also possible to zoom to a specific section by holding down the right mouse button, moving the mouse over a section, and release the right mouse button. The area inside the drawn rectangle defines the area to show.
4 | Each result is represented by one tab, showing the time when the tightening was performed. An icon on the left of each tab reflects the outcome of the tightening: Blue: Tightening successful Red: Tightening failed Exclamation mark: The trace cannot be shown in the diagram Clicking on the icon toggles between the following display settings for its trace: Show trace only Show trace and step dividers with available limits or restrictions Hide trace
5 | Change primary result trace. The primary result trace is used as reference and will define the values for the x-axis. Only one trace can be set as primary result. The first selected trace (the left-most tab) is by default used as reference.
6 | Tightening details of currently selected result.

## Sync methods

Sync methods are different strategies to synchronize traces by a specific value.

Traces can be synchronized by, for example, peak torque (highest torque reached for each trace). This shifts all traces along the x-axis, until each curve has its peak torque value at the exact same position on the x-axis.

All subsequent results are given an offset on the x-axis according to one of the following methods:

Sync method | Description
--- | ---
None | Default value. Selected traces are not synced.
Peak / Torque Peak / Angle Peak / Speed Peak / Current Peak / Gradient | All traces are synchronized towards the peak value, that is, shifted along the x-axis so that the peak values are at the same position on the x-axis as the peak value of the primary result.
Custom / Torque Custom / Angle Custom / Speed Custom / Current Custom / Gradient | All traces are synchronized towards a set value, shifted along the x-axis so that the set value are the same at the same position The set value of the primary result is used as reference point on the x-axis. If sync method Custom is selected and none of the traces contains the configured value, an exclamation mark is shown in the custom value field.

If a result has no trace value that matches to the sync method it cannot be synchronized and its trace will not be shown. It will instead be shown with an exclamation mark.

If none of the traces are possible to synchronize, the error message “Unable to synchronize” is shown.

# Events

# Reading the Information Given in an Event

An event contains information that describes the occurred event as well as some system information to help describe what has happened, where and when.

51399307

1 | Heading - Describes what part of the system the event concerns.
2 | Event name - A short descriptive text of the event.
3 | Virtual station - If the event is related to a virtual station on the controller the virtual station name will be displayed.
4 | Code - A unique four-digit number that identifies the event.
5 | Module - Describes in what part of the system the event concerns.
6 | Type - Information, Warning or Error.
7 | Time - Date and time when the event occurred.

# Event Types

Events are divided into three types; Information, Warnings or Errors.

In this Section

- Event Information
- Event Warnings
- Event Errors

# Event Information

Information events signal a noteworthy event that has occurred from actions performed by the user or the system. Information events do not require any specific user actions.

# Event Warnings

Warning events signal a potentially serious condition that could affect the system performance or result in injury.

# Event Errors

Event Errors signal a serious condition, such as a failed service, that almost exclusively requires the user to make changes to the setup or the configuration in order to continue.

# Configuration of Events

Each event has a default setting for whether they should be acknowledged (Ack), logged (Log) or displayed (Disp). These settings can be configured in Events on the Settings menu.

Some options cannot be changed and they are greyed out.

# Event Codes

Different types of events are used to notify the user of certain state changes or occurrences in the system. Each event requires a different action.

Some of the procedures described can only be performed by Atlas Copco Service personnel.

For more information about a specific event code, use the below filters or enter the event code search criteria in the search box.

Event Code
Event Type
Event Name
Description
Procedure
Log / Display / Ack / Conf
Available for
Group
Search

Event Code | Event Type | Event Name | Description | Procedure | Log / Display / Ack / Conf | Available for | Group
--- | --- | --- | --- | --- | --- | --- | ---
none | item | none | none | none | column | list | list
1000 | Info | Controller Started | The controller is started. |  | Log Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Controller and Tool
1001 | Warning | Controller Serial Number Updated | Generated at start-up if IT-board box serial number (controller serial number) differs from AUX-board box serial number. AUX-board is considered to be non-replaceable in field. The controller will reboot when the serial number is updated. | Replace IT-board or box. | Log Display Ack Conf | Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Controller and Tool
1010 | Info | Tool Connected | A tool is connected. |  | Log Display Conf | Flex Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Controller and Tool
1011 | Info | Tool Disconnected | A tool is disconnected. |  | Log Display Conf | Flex Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Controller and Tool
1012 | Info | Tool Rejected Controller Connection | This event can occur if the tool is into a skip-zone. | Verify if another controller is connected to the tool. Make sure that the tool settings are correctly set up. | Log Display Conf | Power Focus 6000 Power Focus 8 Power Focus XC | Controller and Tool
2000 | Warning | Battery Low |  | Replace battery. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tool
2001 | Warning | Battery Empty |  | Replace battery. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tool
2002 | Warning | Tool Battery Health Low | Tool battery health problem is detected. Valid for SRB, TBP and IxB tools only. | Replace battery. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tool
2004 | Warning | Tool is not of the preferred type | Tool has been replaced by a tool with a different Tool Max Torque. | Change tool. | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tool
2006 | Warning | Tool Backup Battery Health low | The backup battery in the tool has too poor performance. | The backup battery should be replaced. | Log Display Ack Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tool
2007 | Warning | Tool Backup Battery Missing | Tool backup battery is missing. Valid for SRB, TBP and IxB tools only. | Insert battery | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tool
2008 | Warning | Tool Backup Battery Error | Tool backup battery error detected. Valid for SRB, TBP and IxB tools only. | Replace battery. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tool
2009 | Warning | Backup Battery Voltage Low | The controller's backup battery is almost empty | Replace battery. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tool
2010 | Error | Tool Software Version Mismatch | Tool and controller software versions not compatible. | Service tool - update tool software. | Log Display Ack Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tool
2012 | Warning | Tool Communication Disturbance | Communication between tool and controller interrupted. | Relocate antenna placement. | Conf | Flex Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tool
2013 | Warning | Illegal Ring Position | Tool direction switch in faulty position. | If occurring frequently - service the tool. | Log Display Conf | Flex Power Focus 6000 Power Focus 8 Power Focus XC | Tool
2014 | Warning | Tool Overheated | Tool overheated. Valid for SRB, TBP and IxB tools only. | Allow tool to cool down. | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tool
2015 | Error | Tool Temperature Sensor Error | SRB, TBP and IxB tools only. | Service the tool. | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tool
2016 | Warning | Tool Pulse Unit Overheated | Pulse unit overheated. Tool is not locked, but the warning is displayed whenever the tool is started as long as the pulse unit temperature is over threshold. Valid for SRB, TBP and IxB tools only. | Allow tool to cool down. | Log Display Conf | Power Focus 6000 Power Focus 8 Power Focus XC | Tool
2019 | Warning | Tool Could not Start Motor | Tool motor failure. Valid for SRB, TBP and IxB tools only. |  | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tool
2020 | Warning | Tool Requires Motor Tuning | Tool requires motor tuning. | Perform a motor tuning. | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tool
2021 | Warning | Motor Tuning Failed | Motor tuning failed. | Complete motor tuning or service the tool. | Log | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tool
2022 | Info | Motor Tuning Completed | Motor tuning completed. |  | Log Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tool
2023 | Warning | The Tool Requires Open End Tuning | The tool requires open end tuning. | Perform open end tuning. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tool
2024 | Warning | Open End Tuning Failed | Open end tuning failed. | Try to perform open end tuning one more time. If it fails again, service the tool. | Log Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tool
2025 | Info | Open End Tuning Successful | Open end tuning successful. |  | Log Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tool
2026 | Warning | Open End Position Failed | Open end position failed. | Press the tool trigger again and wait for the positioning to be completed. If it fails again, service the tool. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tool
2027 | Warning | Usage Limited Due To High Tool Temperature | Temperature limit value has been reached. Tightening has been inhibited to reduce risk for tool shutting down due to overheating. | Wait until tool temperature has been reduced. | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tool
2030 | Error | Tool Memory Failure: Change Tool | Tool memory corrupt. | Service the tool. | Log Display Ack Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tool
2031 | Error | Tool Accessory Memory Corrupt | Tool accessory memory corrupt. | Service the tool accessory. | Log Display Ack Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tool
2040 | Error | System Check Failure |  |  | Log Display Ack Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tool
2041 | Error | Torque Transducer Error | Will be generated either on calibration error or if tool reports transducer error. | Service the tool. | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tool
2042 | Error | Angle Transducer Error |  | Service the tool. | Log Display Ack Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tool
2043 | Error | Tool Ground Fault Error |  | Service the tool. | Log Display Ack Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tool
2044 | Info | Tool Service Interval Expired | Indicates that servicing of the tool is needed. Triggered when the number of set tightenings has been exceeded. | Perform service of tool. | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tool
2045 | Warning | Tool Calibration Data Invalid | If validation of calibration data fails. | Service the tool. | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tool
2046 | Info | Tool: Next Calibration Date Has Passed | Indicates that calibration of tool is needed. Triggered when calibration alarm is enabled in settings and the current time is greater than next calibration date. | Service the tool. | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tool
2048 | Info | Tool Calibration Value Updated By QA Device | Tool calibration was updated when a calibration with a QA device was performed. |  | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tool
2050 | Error | Tool Parameter File Not Supported | Required tool parameters are missing. | Update tool parameters. | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tool
2060 | Info | Unexpected Trigger Behavior | Used to prevent start of tool if accessory is connected. |  | Log Display Conf | IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tool
2071 | Error | Tool Memory Corrupt | Tool descriptor is corrupt. | Service the tool. | Log Display Conf | Flex Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tool
2072 | Info | Unknown Device Connected |  |  | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tool
2073 | Warning | Tool Trigger Supervision Failure | HW channel failure. Mismatch between hardware and software of tool trigger. |  | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tool
2074 | Warning | Tool Indicator Board Failure | Tool indicator board failure. | Service the tool. | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tool
2075 | Warning | Tool Fan Voltage Failure | Tool fan voltage failure. | Service the tool. | Log Display Conf | Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tool
2076 | Warning | Tool Accessory Bus Voltage Failure | Tool accessory bus voltage failure. | Service the tool. | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tool
2077 | Warning | Tool Trigger Sensor Error | Tool trigger sensor error. | Service the tool. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tool
2078 | Info | Tool Tightening Program Updated | Tool locked due to tightening program update. |  | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tool
2079 | Error | Tool Cable Not Supported | Tool cable is corrupt. The chip in the cable is not responding or is damaged. | Switch cable. | Log Display Conf | Flex Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tool
2080 | Error | Tool Battery Failure | DC voltage too high or too low. Battery failure. | Contact the Atlas Copco service representative and send back battery to Atlas Copco (do not reuse it!). | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tool
2081 | Error | Tool Current Limit Reached | The current limit value has been reached and the drive is disabled. | Service the tool. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tool
2082 | Error | Tool Current Measurement Error | Current measurement error. Current cannot be measured with a reliable result. | Service the tool. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tool
2083 | Error | Tool Internal Error | Various internal hardware errors. Valid for STB and IxB tools only. | Service the tool. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tool
2084 | Error | Tool Internal Software Error | Various internal software errors. Valid for STB and IxB tools only. | Service the tool. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tool
2085 | Error | Tool RBU Error | An RBU error was detected by the tool software. | Check that the RBU is correctly installed. If error is still present then service the tool. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tool
2086 | Error | Tool Stall | Tool motor is stalling. | Service the tool. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tool
2087 | Warning | Tool Motor Current High | Tool motor current limit value is exceeded, and the tool is locked. Tool will enter failsafe mode. Valid for SRB, TBP and IxB tools only. |  | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tool
2088 | Warning | Tool Battery Current High | Tool battery current is too high. Valid for SRB, TBP and IxB tools only. |  | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tool
2089 | Warning | Tool Drive Voltage Low | Tool drive voltage is below the monitored lower voltage limit value. Valid for SRB, TBP and IxB tools only. |  | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tool
2090 | Warning | Tool Drive Voltage High | Tool drive voltage is above monitored higher voltage limit value. Valid for SRB, TBP and IxB tools only. |  | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tool
2091 | Warning | Tool Main Board Error | Tool main board internal error. Valid for SRB, TBP and IxB tools only. |  | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tool
2092 | Warning | Tool Power Module Error | Tool power module internal error. Valid for SRB, TBP and IxB tools only. |  | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tool
2093 | Warning | Pulse Unit Oil Level Low | The oil level of the connected pulse tool is low. | Service the tool. | Log Display Conf | Power Focus 6000 Power Focus 8 Power Focus XC | Tool
2094 | Warning | Pulse Unit Oil Level Empty | The oil level of the connected pulse tool is below required operational level. | Service the tool. | Log Display Ack Conf | Power Focus 6000 Power Focus 8 Power Focus XC | Tool
2095 | Warning | Tool Battery Communication Lost | Tool lost communication with battery. Valid for SRB, TBP and IxB tools only. | Make sure battery is snugged correctly. Otherwise change battery. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tool
2096 | Error | Tool Battery Software Version Mismatch | Tool battery software incompatible with tool software. Valid for SRB, TBP and IxB tools only. | Update software. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tool
2100 | Info | STwrench smartHEAD Removed | STwrench smartHEAD has been removed. | Reconnect smartHEAD and restart the wrench. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tool
2101 | Warning | Wrench Tightening When Locked | A wrench tightening was performed when the tool status was locked in the controller. | Wait until the tool status in controller is unlocked. | Log Display Conf | Power Focus 6000 Power Focus 8 | Tool
2120 | Warning | Unable To Start: Tool Has No Active Torque Transducer |  |  | Log Display | Flex | Tool
2121 | Warning | Transducers Are Disabled For Connected Tool |  |  | Log Display | Flex | Tool
2122 | Warning | Unable To Start: Tool Is Missing Required Torque Transducer |  |  | Log Display | Flex IxB | Tool
2123 | Warning | Unable To Start: Tool Is Missing Required Angle Transducer |  |  | Log Display | Flex | Tool
2124 | Error | Torque Transducer Error On Main Transducer | Shows that there is an error on the Main torque transducer of a Tool with dual transducers. |  | Log Display | Flex | Tool
2125 | Error | Torque Transducer Error On Secondary Transducer | Shows that there is an error on the Secondary torque transducer of a Tool with dual transducers. |  | Log Display | Flex | Tool
2126 | Error | Tool Torque Transducer Calibration Error On Main Transducer |  |  | Log Display | Flex | Tool
2127 | Error | Tool Torque Transducer Calibration Error |  |  | Log Display | Flex StepSync | Tool
2128 | Error | Tool Torque Transducer: Shunt Test Failed On Main Transducer |  |  | Log Display | Flex | Tool
2129 | Error | Tool Torque Transducer: Shunt Test Failed |  |  | Log Display | Flex StepSync | Tool
2130 | Error | Tool Torque Transducer: Zero Offset Compensation Failed On Main Transducer |  |  | Log Display | Flex | Tool
2131 | Error | Tool Torque Transducer: Zero Offset Compensation Failed |  |  | Log Display | Flex StepSync | Tool
2132 | Error | Tool Torque Transducer Hardware Error On Main Transducer |  |  | Log Display | Flex | Tool
2133 | Error | Tool Torque Transducer Hardware Error |  |  | Log Display | Flex StepSync | Tool
2134 | Error | Tool Torque Transducer Error: Overflow In A/D Converter On Main Transducer |  |  | Log Display | Flex | Tool
2135 | Error | Tool Torque Transducer Error: Overflow In A/D Converter |  |  | Log Display | Flex StepSync | Tool
2136 | Error | Tool Torque Transducer Calibration Error On Secondary Transducer |  |  | Log Display | Flex | Tool
2137 | Error | Tool Torque Transducer Error: Shunt Test Failed On Secondary Transducer |  |  | Log Display | Flex | Tool
2138 | Error | Tool Torque Transducer Error: Zero Offset Compensation Failed On Secondary Transducer |  |  | Log Display | Flex | Tool
2139 | Error | Tool Torque Transducer Hardware Error On Secondary Transducer |  |  | Log Display | Flex | Tool
2140 | Error | Tool Torque Transducer Error: Overflow In A/D Converter On Secondary Transducer |  |  | Log Display | Flex | Tool
3000 | Error | Controller Internal Software Error | Software error in the controller. | Contact service. | Log Display Ack Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Controller, Drive and StepSync
3001 | Error | Controller Clock Battery Empty | Internal battery is getting close to end of life. | Replace battery. | Log Display Ack Conf | Flex Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Controller, Drive and StepSync
3010 | Warning | System Overheated | The controller is overheated. | Cool down. | Log Display Conf | Power Focus 6000 Power Focus 8 Power Focus XC | Controller, Drive and StepSync
3011 | Warning | Drive Overheated Controller Hardware |  | Cool down. | Log Display Conf | Flex | Controller, Drive and StepSync
3013 | Warning | Usage Limited Due To High Controller Temperature | Temperature limit value has been reached. Tightening has been inhibited to reduce risk for controller shutting down due to overheating. | Wait until controller temperature has been reduced. | Log Display Conf | Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Controller, Drive and StepSync
3020 | Warning | Controller Hardware Failure |  |  | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Controller, Drive and StepSync
3021 | Warning | System Voltage Problem | DC voltage too high or too low. |  | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Controller, Drive and StepSync
3022 | Warning | Controller Voltage Problem: AC Input Voltage Too High | DC voltage too high or too low. | Fix the input voltage. | Log Display | Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Controller, Drive and StepSync
3023 | Warning | Controller Voltage Problem: AC Input Voltage Too Low | DC voltage too high or too low. | Fix the input voltage. | Log Display | Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Controller, Drive and StepSync
3024 | Warning | Drive Voltage Problem: AC Input Voltage Too High | DC voltage too high or too low. | Fix the input voltage. | Log Display | Flex | Controller, Drive and StepSync
3025 | Warning | Drive Voltage Problem: AC Input Voltage Too Low | DC voltage too high or too low. | Fix the input voltage. | Log Display | Flex | Controller, Drive and StepSync
3030 | Error | IP Address Conflicting With Another Node On The Network | The set IP address is in use by another device on the same network. | Change IP address on one of the devices. | Log Display Conf | Flex Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Controller, Drive and StepSync
3031 | Info | Network Cable Unplugged | The carrier of the factory port is lost (cable disconnected). | Check the cable connection. | Log Display Conf | Flex Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Controller, Drive and StepSync
3032 | Info | Pairing Started | Tool pairing started. |  | Log Display Conf | Power Focus 6000 Power Focus 8 Power Focus XC | Controller, Drive and StepSync
3033 | Info | Pairing Successful | Tool pairing successful. |  | Log Display Conf | Power Focus 6000 Power Focus 8 Power Focus XC | Controller, Drive and StepSync
3034 | Error | Pairing Unsuccessful: No Tool Found | The controller found no tool to pair with when scanning for radio peers. | Set the tool in pairing mode and try again. | Log Display Conf | Power Focus 6000 Power Focus 8 Power Focus XC | Controller, Drive and StepSync
3035 | Error | Pairing Unsuccessful: More Than One Tool Found | The controller found more than one tool when scanning for radio peers. | Ensure that only one tool is in pairing mode when starting the pairing mode on the controller. | Log Display Conf | Power Focus 6000 Power Focus 8 Power Focus XC | Controller, Drive and StepSync
3036 | Error | Pairing Unsuccessful: Communication Error | The controller experienced a loss of connection, an unexpected answer or timeout during the pairing process. | Try to perform pairing one more time. If it fails again, service the tool. | Log Display Conf | Power Focus 6000 Power Focus 8 Power Focus XC | Controller, Drive and StepSync
3037 | Info | Pairing Unsuccessful: Tool Slot Is Full |  | Clear one tool slot. | Log Display Conf | Power Focus 6000 Power Focus 8 Power Focus XC | Controller, Drive and StepSync
3040 | Warning | Emergency Stop | Drive disabled due to emergency stop. | Reset emergency stop. | Log Display Conf | Flex Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Controller, Drive and StepSync
3050 | Info | System Clock Updated | System clock has been updated. |  | Log Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Controller, Drive and StepSync
3051 | Error | System Clock Error | Wrong time read from hardware Real Time Clock (RTC). | Change RTC battery. | Log Display Ack Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Controller, Drive and StepSync
3052 | Warning | Remote Start Configuration Error | Mismatch between HW and SW remote start configuration. | Verify that HW dip switch matches the selected start source. | Log Display Conf | Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Controller, Drive and StepSync
3053 | Info | Drive Connected | StepSync drive has been connected. |  | Log Display | Flex Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Controller, Drive and StepSync
3054 | Info | Drive Disconnected | StepSync drive disconnected. |  | Log Display | Flex Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Controller, Drive and StepSync
3055 | Warning | Mode Configuration Error | Generated when selected mode is configured wrongly. E.g. configuring two bolts with the same bolt number or the same channel, incomplete mode configuration. | Check ToolsTalk 2 for mode configuration error. | Log Display | Flex StepSync | Controller, Drive and StepSync
3056 | Warning | Unable to Start: Tool Or Drive Is Missing | Generated when a used channel is missing a drive or tool. | Verify Channel Menu on the HMI. Connect missing drive or tool. | Log Display | Flex StepSync | Controller, Drive and StepSync
3057 | Info | Unable to Start: Channel Is Already In Use | Generated when a needed channel has been allocated to another virtual station. |  | Log Display | Flex | Controller, Drive and StepSync
3058 | Info | No Mode Selected |  | Select mode. | Log Display | Flex StepSync | Controller, Drive and StepSync
3059 | Warning | Failed To Connect To Atlas Copco License Manager | Indicates that the controller failed to connect to the local license manager to get licenses. | Verify the local network. If it fails again, service the controller. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Controller, Drive and StepSync
3061 | Warning | Unable To Start: Enable Signal Is Low |  |  | Log Display | Flex StepSync | Controller, Drive and StepSync
3062 | Warning | Unable To Start: Stop Signal Is High |  |  | Log Display | Flex StepSync | Controller, Drive and StepSync
3063 | Warning | Unable To Start: All Channels Inhibited | All channels have been set inhibited, so no tightening can be started. | Set at least one channel to not be inhibited. | Log Display | Flex StepSync | Controller, Drive and StepSync
3064 | Warning | Carrier Number Faulty | A FlexCarrier hex switch is set to zero. | Turn the switch to a non-zero value. | Log Display | Flex | Controller, Drive and StepSync
3065 | Warning | Carrier E-Stop Configuration Plug Wrong Type Or Missing | A Carrier is missing its E-stop configuration plug, or the plug type is wrong. | Insert correct plug type. | Log Display | Flex | Controller, Drive and StepSync
3066 | Warning | Carrier Voltage Inlet: No 3-Phase AC |  |  | Log Display | Flex | Controller, Drive and StepSync
3067 | Warning | Carrier Voltage Inlet: One AC Phase Missing |  |  | Log Display | Flex | Controller, Drive and StepSync
3068 | Warning | Carrier: Internal 24 VDC Power Supply Unit Broken |  |  | Log Display | Flex | Controller, Drive and StepSync
3069 | Warning | Carrier 24 Voltage OUT-Port Disabled Due To Over-Current |  | Reset the system. | Log Display | Flex | Controller, Drive and StepSync
3070 | Warning | Carrier, Hardware Error In PF6 FlexControl Cable OUT |  | Reset the system. | Log Display | Flex | Controller, Drive and StepSync
3071 | Warning | Carrier, Hardware Error In PF6 FlexControl Cable IN |  | Reset the system. | Log Display | Flex | Controller, Drive and StepSync
3072 | Warning | Emergency Stop 24 VDC Power Failure Due To Short-Circuit |  |  | Log Display | Flex | Controller, Drive and StepSync
3073 | Warning | Unable To Start: System Is Emergency Stopped | When allocating multiple spindles, this event is invoked by "preStartCheckFailed" due to emergency stop. | Reset the emergency stop. | Log Display | Flex StepSync | Controller, Drive and StepSync
3074 | Warning | Carrier Overheated |  |  | Log Display | Flex | Controller, Drive and StepSync
3075 | Warning | Carrier Temperature OK |  |  | Log Display | Flex | Controller, Drive and StepSync
3076 | Warning | Carrier: Internal 24 VDC Power Supply Overload | Current output from internal PSU is too high. | Disconnect other carriers that are powered from the PSU. Disconnect any external equipment using 24 VDC. | Log Display | Flex | Controller, Drive and StepSync
3077 | Warning | Carrier: Internal 24 VDC Power Supply Over Voltage | Voltage output from internal PSU is too high. | Replace the carrier. | Log Display | Flex | Controller, Drive and StepSync
3078 | Warning | Carrier: Internal 24 VDC Power Supply Under Voltage | Voltage output from internal PSU is too low. | Replace the carrier. | Log Display | Flex | Controller, Drive and StepSync
3079 | Warning | External Supply To Carrier: 24 VDC Over Voltage | Backup input voltage is more than 27 VDC. | Adjust the backup input voltage. | Log Display | Flex | Controller, Drive and StepSync
3080 | Warning | External Supply To Carrier: 24 VDC Under Voltage | Backup input voltage is less than 19 VDC. | Adjust the backup input voltage. | Log Display | Flex | Controller, Drive and StepSync
3081 | Warning | Carrier Voltage Inlet: 3-Phase AC Over Voltage | Input voltage is too high. | Lower input voltage: must be 400 VAC or 480 VAC. | Log Display | Flex | Controller, Drive and StepSync
3082 | Warning | Carrier Voltage Inlet: 3-Phase AC Under Voltage | Input voltage is too low. | Higher input voltage: must be 400 VAC or 480 VAC. | Log Display | Flex | Controller, Drive and StepSync
3083 | Error | Wrong Anybus/Profisafe Module Firmware |  |  | Log Display | Flex Power Focus 6000 Power Focus 8 StepSync | Controller, Drive and StepSync
3084 | Error | Soft PLC Runtime Error | eCLR has terminated in an uncontrolled way. |  | Log Display Conf | Flex Power Focus 6000 Power Focus 8 StepSync | Controller, Drive and StepSync
3085 | Warning | Carrier: Fan Module Out Of Order |  |  | Log Display | Flex | Controller, Drive and StepSync
3086 | Warning | Carrier: Fan Module Partly Out Of Order |  |  | Log Display | Flex | Controller, Drive and StepSync
3087 | Warning | Carrier: Left Fan Module Out Of Order |  |  | Log Display | Flex | Controller, Drive and StepSync
3088 | Warning | Carrier: Left Fan Module Partly Out Of Order |  |  | Log Display | Flex | Controller, Drive and StepSync
3089 | Warning | Carrier: Right Fan Module Out Of Order |  |  | Log Display | Flex | Controller, Drive and StepSync
3090 | Warning | Carrier: Right Fan Module Partly Out Of Order |  |  | Log Display | Flex | Controller, Drive and StepSync
3100 | Warning | Mode Configuration Does Not Exist |  |  | Log Display | Flex StepSync | Controller, Drive and StepSync
3150 | Error | Software IAM Incompatibility | IAM is incompatible with the software that is installed on the controller. | Replace IAM. | Log Display Ack | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Controller, Drive and StepSync
3160 | Error | Failed To Activate Newly Installed Software | Something went wrong during the activation. When the newly installed software starts, a fallback to the previous working software happens. This error happens when the new software fails to start for three times and only during software installation. | Take an export and contact Atlas Copco for further assistance. Note down the software version you are trying to install as well as the software version that is working. | Log Display Ack | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Controller, Drive and StepSync
3161 | Error | Started On Unexpected Software Partition | The controller has started on the inactive software side and not on the expected software side. | Note down the software information (on the Home screen of the controller, select Controller > Software). Try to restart the controller and make sure its running on correct software when started again. If error persists, do an export and contact Atlas Copco. | Log Display Ack | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Controller, Drive and StepSync
3500 | Error | Generic License Manager Error | Inconsistency detected in the feature management system used. | Contact Atlas Copco representative. | Log Display Ack | IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Controller, Drive and StepSync
3501 | Error | License Manager Synchronization Error |  |  | Log Display Ack | IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Controller, Drive and StepSync
3502 | Info | License Manager Synchronization Done |  |  |  | IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Controller, Drive and StepSync
3503 | Warning | License Manager: Another Source in Use | License is used by another source. | Verify license assignment. | Log Display | IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Controller, Drive and StepSync
3504 | Warning | License Manager Restart Needed |  | Restart license manager. | Log Display | IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Controller, Drive and StepSync
3505 | Info | USB License Synchronization Started |  |  | Log | Power Focus 6000 Power Focus 8 Power Focus XC | Controller, Drive and StepSync
3506 | Error | USB License Synchronization Error |  |  | Log | Power Focus 6000 Power Focus 8 Power Focus XC | Controller, Drive and StepSync
3507 | Info | USB License Synchronization Done |  |  | Log | Power Focus 6000 Power Focus 8 | Controller, Drive and StepSync
3508 | Info | One or more of your licenses are about to expire. Please make sure you have a license server configured |  | Update licenses. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Controller, Drive and StepSync
3511 | Warning | One of your licenses has a different license definition | Inconsistency detected in a license to be used. | Contact Atlas Copco representative. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Controller, Drive and StepSync
3550 | Warning | License Is Missing |  | Install the correct license. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Controller, Drive and StepSync
3551 | Warning | Wireless Communication Disabled By Licensing |  | Unassign Standalone license from the Virtual Station. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Controller, Drive and StepSync
4010 | Info | Tool Locked By Digital Input | The tool is locked by a digital input signal. |  | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tightening Process
4011 | Info | Tool Locked By Open Protocol | The tool is locked by Open Protocol. |  | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tightening Process
4012 | Info | Tool Locked By Fieldbus | The tool is locked by the Fieldbus. |  | Log Display Conf | Flex Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tightening Process
4013 | Info | Tool Locked By Socket Selector | Tool is locked when the socket selector is disconnected from the Virtual Station. | Unlock by Master Unlock. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4014 | Info | Tool Locked By Soft PLC | Soft PLC signal locked the tool. | Unlock by Master Unlock. | Log Display Conf | Flex Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tightening Process
4015 | Info | Loosening Disabled | Loosening is disabled in the tightening program. |  | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tightening Process
4016 | Info | Tightening Disabled |  |  | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tightening Process
4017 | Info | Loosening Not Configured | Loosening is not configured in the selected tightening program | Select different tightening program. | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tightening Process
4020 | Info | Too Many NOK Tightenings | Maximum consecutive NOK tightenings in batch is exceeded |  | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tightening Process
4025 | Info | No Tightening Program Selected | No tightening program selected. | Select tightening program or batch sequence. | Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4030 | Info | Batch Sequence Aborted | The batch sequence has been aborted. |  | Log Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tightening Process
4031 | Info | Max Time To Complete Batch Sequence Reached |  |  | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tightening Process
4032 | Info | Max Time To Complete First Tightening Reached |  |  | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tightening Process
4035 | Info | Locked By Line Control |  |  | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4040 | Info | Locked By Alternative Identifier | Tool locked by alternative identifier. |  | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4050 |  | Invalid Socket Configuration | Tightening program assigned to multiple sockets. | Tightening program assigned to multiple sockets. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4060 | Info | Tool Locked On Batch Complete | When running a batch with flag Tool lock on batch sequence complete this event is generated when the user press the trigger. | Unlock with signal Unlock Tool on complete. | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tightening Process
4070 | Info | Process Enter Manual Mode | Indicates that manual mode has been activated for a virtual station. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4071 | Info | Process Enter Automatic Mode | Indicates that automatic mode has been entered for a virtual station. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4072 | Info | Test Bolt |  |  | Conf | Flex StepSync | Tightening Process
4100 | Warning | Identifier Not Accepted: Invalid String Length |  |  | Display Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tightening Process
4101 | Warning | String Selection Unsuccessful: Multiple Matches |  |  | Display Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tightening Process
4102 | Warning | String Selection Unsuccessful: No Match Found |  |  | Display Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tightening Process
4103 | Warning | Identifier Not Accepted: Identical String Already Received |  |  | Display Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tightening Process
4104 | Warning | Identifier Not Accepted: No Match Found |  |  | Display Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tightening Process
4500 | Info | Result DriveError | Internal driver error or driver loss detected. |  | Conf | Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4501 | Info | Result Rehit | Attempt to tighten an already tightened bolt when Rehit detection is on. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4502 | Info | Result Soft Start Torque Low | Soft start torque below minimum level. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4503 | Info | Result Soft Start Torque High | Soft start torque exceeded maximum level. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4504 | Info | Result Self Tap Torque High | Self-tap torque exceeded maximum level. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4505 | Info | Result Self Tap Torque Low | Self-tap torque below minimum limit. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4506 | Info | Result Safety Torque Low | Automatically calculated torque value to ensure torque sensor is mounted correctly. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4507 | Info | Result Rundown Torque High | Rundown torque exceeded maximum level. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4508 | Info | Result Rundown Angle High | Rundown angle exceeded maximum level. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4509 | Info | Result Rundown Time High | Rundown time exceeded maximum limit. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4510 | Info | Result Rundown Time Low | Rundown time below minimum limit. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4511 | Info | Result Rundown Torque Low | Rundown torque below minimum level. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4512 | Info | Result Rundown Angle Low | Rundown angle below minimum level. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4513 | Info | Result Final Torque High | Final step torque exceeded maximum level. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4514 | Info | Result Final Angle High | Final step angle exceeded maximum level. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4515 | Info | Result Final Torque Low | Final step torque below minimum level. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4516 | Info | Result Final Angle Low | Final step angle below minimum level. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4517 | Info | Result Tightening Timeout | Tightening time limit exceeded. For General Tightening Strategies max tightening time is 30 seconds. For Multistep max tightening time depends on step restriction Maximum Time Limit. Error code is dependent on tightening stage. | Redo tightening. | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4518 | Info | Result Trigger Lost | Tool trigger was released before target was reached. For General Tightening Strategies it is not allowed to release the trigger before the tightening stage has finished. For Multistep, the error is displayed when trigger is lost before the target in a specific step is reached. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4519 | Info | Premature Torque Loss | Socket has slipped off the nut. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4520 | Info | Result Target Reached Before Final Step | Target torque reached before final step in tightening program. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4521 | Info | Result Post View Torque Low | Post view torque below minimum level. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4522 | Info | Result Post View Torque High | Post view torque exceeded maximum level. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4523 | Info | Result Post View Torque Interval Not Reached | Post view torque interval not reached. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4524 | Info | Result Torque Compensation Interval Not Reached | Torque compensation interval angle before rundown end not reached. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4525 | Info | Result Tool Movement Exceeded | From a NOK tightening detailed status. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4526 | Info | Result SafetyCurrMon Sensor Mismatch | Current monitoring error. |  |  | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4527 | Info | Result Tool Movement Exceeded |  |  |  | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4538 | Info | Result Final Supervision Torque Low | Final Supervision Torque was not reached. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4543 | Info | Result Snug Monitor High | Wrench only. Monitor detected snug value exceeded. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4545 | Info | Result No Residual Torque | Wrench only. Residual torque was under threshold. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4546 | Info | Result Overspeed | Wrench only. Wrench gyro failed to measure angle due to high speed. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4547 | Info | Result Effective Loosening | Wrench only. Wrench detected unexpected loosening. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4548 | Info | Result Final Less Than Target | Final torque is below target torque set in tightening program. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4549 | Info | TurboTight Time Limit Exceeded |  |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4550 | Info | Result Rundown Pulses High | Maximum number of rundown pulses is exceeded. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4551 | Info | Result Rundown Pulses Low | Rundown is completed before the minimum number of rundown pulses is reached. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4552 | Info | Result Final Pulses High | Maximum number of pulses is exceeded. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4553 | Info | Result Final Pulses Low | Tightening is completed before the minimum number of pulses is reached. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4554 | Info | Current At Shutoff High | Current at shut off exceeded Current Limit High. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4555 | Info | Current At Shutoff Low | Shut off current measured was below Current Limit Low. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4556 | Info | Uncategorized Multistep Error | An error in the multistep configuration, often with tool validation. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4557 | Info | Result Overload |  |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4600 | Warning | Data Drop or Data Hold used in combination with Batch Tightening. The signals have no effect |  | Data Drop and Data Hold are only supported for worktasks, without batch control. Select another worktask if the signals must be used. |  | Flex StepSync | Tightening Process
4601 | Info | Data Hold Active: tightening result is sent once signal is low |  |  |  | Flex StepSync | Tightening Process
4602 | Info | Data Drop active: tightening result discarded |  |  |  | Flex StepSync | Tightening Process
5010 | Warning | Invalid Tightening Program Parameter Value | The parameter in the selected tightening program are invalid. | Check the configuration of the selected tightening program to find and to change the value of the parameter. | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Program Configuration
5020 | Info | Main Trigger Is Not The Active Start Source | Generated when configured for push start only and user presses main trigger. Will be generated until user presses the push start. | Press push start to start the tool. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Program Configuration
5030 | Info | Tightening Program Complexity Exceeds Tool Capacity | The selected tightening program is too complex for the STB tool that is used. Tool will be locked. | Reduce complexity of the tightening program, or choose different program. | Log Display Conf | Power Focus 6000 Power Focus 8 Power Focus XC | Program Configuration
6010 | Info | Accessory Connected | Accessory is connected to the controller. |  | Log Display Ack Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Accessory
6020 | Info | Accessory Disconnected | Accessory is disconnected from the controller. |  | Log Display Ack Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Accessory
6021 | Warning | Fieldbus Offline | No communication with Fieldbus. |  | Log Display Ack Conf | Flex Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Accessory
6030 | Warning | Accessory Address Collision | Two or more accessories with the same address are connected. | Change address on accessory. | Log Display Ack Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Accessory
6040 | Warning | Accessory Communication Error | Intermittent communication error with accessory. | Check cables and connectors. | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Accessory
6041 | Warning | Fieldbus Error | Communication error with Fieldbus. |  | Log Display Ack Conf | Flex Power Focus 6000 Power Focus 8 StepSync | Accessory
6042 | Warning | Fieldbus Module Mismatch | The installed Fieldbus module does not match with the configured module. | Change the configuration to match with the installed module, or replace the installed module with the correct one. | Log Display Ack Conf | Flex Power Focus 6000 Power Focus 8 StepSync | Accessory
6043 | Warning | Fieldbus Output Buffer Overflow | The output buffer used for the Fieldbus communication is exhausted and an overflow of the buffer has occurred. One or more signal updates have been discarded. | Stop Fieldbus communication and Fieldbus diagnostics (if used) to recover the buffer. If this event occurs frequently, check your Fieldbus communication setup, including the PLC program: too frequent updates compared to your update interval can lead to this scenario. | Log Display Ack Conf | Flex Power Focus 6000 Power Focus 8 StepSync | Accessory
6044 | Warning | Fieldbus Provider ID mismatch | The installed fieldbus module is not supported. | Connect a supported Atlas Copco fieldbus module. | Log Display Ack | Power Focus 8 | Accessory
6050 | Info | Wrong Socket Selected | Generated when no or incorrect socket is selected. |  | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Accessory
6090 | Warning | Barcode Scanner Could Not Be Identified | When no unique serial number is found. | Configure the barcode reader device. | Log Display Ack Conf | Flex Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Accessory
7010 | Info | Message Text To Display | General event for displaying of messages. |  | Display Ack Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Message
8200 | Info | Failed To Open Serial Port | Serial port to be used could not be opened. | Check serial port connections. | Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Miscellaneous
8214 | Error | EHMI Software Version Mismatch | EHMI software version does not match in compatibility with the controller. | Update the software version of the EHMI. | Log Display Ack Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Miscellaneous

## Glossary

Conf - Event Codes list

Tells the user whether it is possible to configure the event through the "Configure Event" page.

Available for - Event Codes list

List of products for which the event code is available.

Groups - Event Codes list

Group which the event codes belong to.

Event Description

A short description of the event and why it occurs.

Procedure - Event Codes list

If applicable, the procedure contains an instruction on how to clear the event.

Log - Event Codes list

Tells the user whether the event is to be saved in the event log or not. The value in this list is the default value.

display - Event Codes list

Tells the user whether the event is to be displayed on the screen or not. The value in this list is the default value.

Ack - Event Codes list

Tells the user whether the event must be acknowledged or not before you can proceed. The value in this list is the default value.

Event code

The unique event number.

Type of events - Event Codes list

Type of event: Info, Warning, and Error.

Event name

A descriptive name of the event.

# NOK Results List

Error message | Description | GUI location
--- | --- | ---
Drive error | Internal driver error or driver loss detected. | N/A
Rehit | Attempt to tighten an already tightened bolt. | Tightening parameters (Edit) > Rehit detection
Soft start torque above max | Soft start torque exceeded maximum level. | Tightening parameters (Edit) > (Step 1) Soft Start > Torque max
Selftap torque above max | Selftap torque exceeded maximum level. | Tightening parameters (Edit) > (Step 2) Selftap > Torque max
Selftap torque below min | Selftap torque below minimum limit. | Tightening parameters (Edit) > (Step 2) Selftap > Torque min
Safety torque limit low | Automatically calculated torque value to ensure torque sensor is mounted correctly. | N/A
Rundown torque above max | Rundown torque exceeded maximum level. | Tightening parameters (Edit) > (Step 2) Rundown torque limits > Torque max
Rundown angle above max | Rundown angle exceeded maximum level. | Tightening parameters (Edit) > (Step 2) Rundown angle limits > Angle max
Rundown exceeded max time limit | Rundown time exceeded maximum limit. | Tightening parameters (Edit) > (Step 2) Rundown angle limits > Time max
Rundown below min time limit | Rundown time below minimum limit. | Tightening parameters (Edit) > (Step 2) Rundown angle limits > Time min
Rundown torque below min | Rundown torque below minimum level. | Tightening parameters (Edit) > (Step 2) Rundown torque limits > Torque min
Rundown angle below min | Rundown angle below minimum level. | Tightening parameters (Edit) > (Step 2) Rundown angle limits > Angle min
Final step torque above max | Final step torque exceeded maximum level. | Tightening parameters (Edit) > (Step 3) Final step > Torque limits Manual > Torque max
Final step angle above max | Final step angle exceeded maximum level. | Tightening parameters (Edit) > (Step 3) Final step > Angle max
Final step torque below min | Final step torque below minimum level. | Tightening parameters (Edit) > (Step 3) Final step > Torque limits Manual > Torque min
Final step angle below min | Final step angle below minimum level. | Tightening parameters (Edit) > (Step 3) Final step > Angle max
Tightening timeout | Tightening time limit exceeded. | [Multistep] Tightening parameters (Edit) > Step dependent [Other tightening programs]: fixed parameter set to 30 seconds
Trigger lost | Tool trigger was released before target was reached. | [Multistep]: trigger release before tightening step target has been reached [Other tightening programs]: trigger release before tightening stage has finished
Slip off | Socket has slipped off the nut. | Tightening parameters (Edit) > (Step 3) Tightening parameters > Slipoff detection time
Target reached before final step | Target torque reached before final step in tightening program. | Target torque
Post view torque below min | Post view torque below minimum level. | Tightening parameters (Edit) > (Step 2) Post view torque > Torque min
Post view torque above max | Post view torque exceeded maximum level. | Tightening parameters (Edit) > (Step 2) Post view torque > Torque max
Post view torque interval not reached | Post view torque interval not reached. | Tightening parameters (Edit) > (Step 2) Post view torque > Torque min length
Torque compensation interval not reached | Torque compensation interval angle before rundown end not reached. | Tightening parameters (Edit) > (Step 3) Torque compensation > Torque compensation point
Tool movement exceeded | Tool was moved beyond set angle limits. | Tightening parameters (Edit) > (Step 1) TrueAngle compensation (On); Tool movement limits > Positive/Negative
Current monitoring error | Current monitoring error. | Tightening parameters (Edit) > (Step 1) Current monitoring (On)
Final step exceeded max time limit |  | [TurboTight] Tightening parameters (Edit) > (Step 3) Final step > Time max
Final step below min time limit |  | [TurboTight] Tightening parameters (Edit) > (Step 3) Final step > Time min
TurboTight time limit exceeded | TurboTight time limit exceeded. | [TurboTight] Tightening parameters (Edit) > (Step 3) Final step > Time max
Snug monitor high | Wrench only. Monitor detected snug value exceeded. | Tightening parameters (Edit) > Rundown stage (Step 2) Rundown complete > Rundown complete torque
No residual torque | Wrench only. Residual torque was under threshold. | [TurboTight] + [TensorPulse] Tightening parameters (Edit) > (Step 3) > Tightening parameters > Residual torque correlation factor
Overspeed | Wrench only. Wrench gyro failed to measure angle due to high speed. | N/A

# SPC - Statistical Process Control

The purpose of the built-in SPC function is to give the operator or quality control staff data that let them judge the stability and capability of the assembly process according to standard SPC rules.
By configuring the SPC function within the controller, it is possible to simplify and do the work directly on the controller without the need of external software. The charts are generated on the controller.
Since it is possible to use program monitors within the controller as a SPC variable, it is necessary to specify that only variables controlled by the controller show the performance of the controller system. Other variables show mainly results from other processes. For example, if a torque value is applied to a joint, then SPC of the final torque value and the related results - such as Cp and Cpk - show the performance of the tool and the controller on that joint.

Statistical calculations are based on old data stored in the controller.

Statistical calculations are done on a Virtual Station level, depending on the tightening program selected and used for that specific Virtual Station.

In this Section

- Configuring SPC Parameters
- Configuring SPC Variables
- Calculating Statistics
- Viewing Statistical Results

# Configuring SPC Parameters

1. On the Home view, select the Reports Tab. Then, on the left, select Statistics.

2. In the SPC Configuration window, enter the following parameters to collect results stored in the controller:

   - Number of Subgroups: enter the number of subgroups the statistics calculation is based upon.
     The number of results (Number of Subgroups × Frequency) can range from 2 through 500.

   - Subgroup Size: enter the number of tests (samples) necessary to define each point (the average value of the tests in the subgroup) on the SPC charts.
     The subgroup size can range from 2 through 25.

   - Frequency: enter how often to start collecting a new subgroup.
     Frequency must be equal or higher than Subgroup size.

     For instance, if Frequency is 8 and Subgroup Size is 5, the first 5 data (results) is used for the subgroup. Because of the Frequency =8, the next subgroup starts considering data (results) from the 8th one on, and so on in a loop.

# Configuring SPC Variables

1. On the Home view, select the Reports Tab. Then, on the left, select Statistics.

2. Select the Plus icon at the upper-right corner of the GUI.
   The SPC Variable window shows the new variable.

3. In the Name box, enter the name of the variable.
   The name of the variable is the heading of the SPC Variable window.

4. Select Tightening Program.
   The Tightening Program window appears and lists all the multistep tightening programs stored in the controller and available for statistical calculations.
   Select the multistep tightening program of the new variable.

   The Tightening Program must be a Multistep Program.

5. Select Virtual Station.
   The Virtual Station window appears.
   Select the Virtual Station which the results are made from.

   Statistics are based on results made by a Virtual Station that has the following license type assigned:

   - Process Control

6. Select Monitor.
   The Monitor window appears.
   Select one of the following program monitors which the SPC calculation is based on:

   - Step monitor peak torque

   - Step monitor angle

   - Final torque

   - Final angle

   - Program monitor torque

   - Program monitor angle

   If the user selects Step monitor peak torque or Step monitor angle, in the Step number box enter the number of the necessary step of the tightening program which read the value from.

   If the user uses the result reporters, it is possible to have an effect on the following monitor values: Final torque and Final angle.

7. Select Edit limits.
   The Variable configuration window appears.
   For calculations and analysis of the results, set the following limits for each value of interest.

In the Tolerance limits window, set the following limits (used for calculation of the process capabilities Cp and Cpk):

- Upper Tolerance Limit (UTL): a user-defined quantity that identifies the highest acceptable value of a product attribute.

- Lower Tolerance Limit (LTL): a user-defined quantity that identifies the lowest acceptable value of a product attribute.

In the Control limits window, enable or disable the Auto calculate switch.
If the Auto calculate switch is set to Yes, the control limits are automatically calculated.
If the Auto calculate switch is set to No, set the following limits:

- Mean - Upper control limit: a statistically determined measurement that appears as a horizontal dashed line above the process average.

- Mean - Lower control limit: a statistically determined value that appears as a horizontal dashed line below the process average.

- Range - Upper control limit: a statistically determined measurement that appears as a horizontal dashed line above the process average.

- Range - Lower control limit: a statistically determined value that appears as a horizontal dashed line below the process average.

- Sigma - Upper control limit: a statistically determined measurement that appears as a horizontal dashed line above the process average.

- Sigma - Lower control limit: a statistically determined value that appears as a horizontal dashed line below the process average.

In the Capabilities window, set the following limits:

- Cp: the Cp index gives the process capability: it is the number of times the spread of the process is into the tolerance width (Upper tolerance limit - Lower tolerance limit). The higher the value of Cp, the better the process.

- Cpk: the Cpk index gives the process capability corrected for the position. It is not useful having a high Cp index if the process setting is way off center in relation to the middle of the tolerance range. A high Cpk index means, then, that you have a good process with a small spread in relation to the tolerance width, and also that it is well centered within that width (Upper tolerance limit - Lower tolerance limit). If Cpk is equal to Cp, the process is set to produce exactly in the middle of the tolerance range.

Relevant Information

- Multistep Programs
- Step Monitors
- Working with the Virtual Station Tab

# Calculating Statistics

1. On the Home view, select the Reports Tab. Then, on the left, select Statistics.

2. In the SPC Configuration window, enter the parameters to collect results stored in the controller (Number of Subgroups, Subgroup Size, and Frequency).

3. Select the Plus icon at the upper-right corner of the GUI.
   The SPC Variable window shows the new variable.
   Configure the new SPC Variable.

4. In the SPC Variable window, select Calculate.
   Data is collected from the historical results stored in the controller that are aligned with the criteria set in the SPC Configuration window and SPC Variable window. The values of interest are collected into subgroups of the size set in the SPC Configuration window. The collected tightening results on the controller are used for statistics calculations.

It is not possible to calculate statistics for results from deleted tightening programs or Virtual Stations, unless the results are still stored on the controller.

Only 1 user at a time can calculate statistics.

## Statistics Formulas

Data in a subgroup is calculated as:

- Average:

- Range = R = max (Xi) - min (Xi), where i=1...n

- Standard deviation for a subgroup:

- Total overall of the standard deviation:

  Where N = total number of observations.

When specified number of subgroups to use for calculations has been collected, the SPC function starts calculations to determine the statistical stability.
Calculations are performed through the following steps: (m = number of subgroups)

- Calculation of Average of Average values:

- Calculation of Average of Range:

- Calculation of Average of Standard deviation:

- Calculation of the process capabilities Cp and Cpk with respect to Sigma:

  Where:

  - is the overall arithmetic average of the observed characteristic values.

  - UTL is the Upper Tolerance Limit.

  - LTL is the Lower Tolerance Limit.

  - The sigma estimation is the mean square standard deviation within the subgroups:

- Calculation of the process capabilities Cp and Cpk with respect to Range:

  Where for a normal distribution su = sl = 3.

Calculations for control limits if, in the SPC Configuration window, the Auto calculate switch is set to Yes:

- X-bar R (Mean)

- X-bar R (Range)

- X-bar S (Mean)

- X-bar S (Sigma)

A2, A3, D3, D4, B3, and B4 are constants (for more information, see the "SPC Calculation Constants" paragraph).

## SPC Calculations Constants

Subgroup Size | Divisors for estimate of standard dev. | Factors for Control Limits
--- | --- | ---
|  | Xbar R | Xbar S
A2 | D3 | D4 | A3 | B3 | B4
n | d2
2 | 1.128 | 1.880 | - | 3.267 | 2.659 | - | 3.267
3 | 1.693 | 1.023 | - | 2.574 | 1.954 | - | 2.568
4 | 2.059 | 0.729 | - | 2.282 | 1.628 | - | 2.266
5 | 2.326 | 0.577 | - | 2.114 | 1.427 | - | 2.089
6 | 2.534 | 0.483 | - | 2.004 | 1.287 | 0.030 | 1.970
7 | 2.704 | 0.419 | 0.076 | 1.924 | 1.182 | 0.118 | 1.882
8 | 2.847 | 0.373 | 0.136 | 1.864 | 1.099 | 0.185 | 1.815
9 | 2.970 | 0.337 | 0.184 | 1.816 | 1.032 | 0.239 | 1.761
10 | 3.078 | 0.308 | 0.223 | 1.777 | 0.975 | 0.284 | 1.716
11 | 3.173 | 0.285 | 0.256 | 1.744 | 0.927 | 0.321 | 1.679
12 | 3.258 | 0.266 | 0.283 | 1.717 | 0.886 | 0.354 | 1.646
13 | 3.336 | 0.249 | 0.307 | 1.693 | 0.850 | 0.382 | 1.618
14 | 3.407 | 0.235 | 0.328 | 1.672 | 0.817 | 0.406 | 1.594
15 | 3.472 | 0.223 | 0.347 | 1.653 | 0.789 | 0.428 | 1.572
16 | 3.532 | 0.212 | 0.363 | 1.637 | 0.763 | 0.448 | 1.552
17 | 3.588 | 0.203 | 0.378 | 1.622 | 0.739 | 0.466 | 1.534
18 | 3.640 | 0.194 | 0.391 | 1.608 | 0.718 | 0.482 | 1.518
19 | 3.689 | 0.187 | 0.403 | 1.597 | 0.698 | 0.497 | 1.503
20 | 3.735 | 0.180 | 0.415 | 1.585 | 0.680 | 0.510 | 1.490
21 | 3.778 | 0.173 | 0.425 | 1.575 | 0.663 | 0.523 | 1.477
22 | 3.819 | 0.167 | 0.434 | 1.566 | 0.647 | 0.534 | 1.466
23 | 3.858 | 0.162 | 0.443 | 1.557 | 0.633 | 0.545 | 1.455
24 | 3.895 | 0.157 | 0.451 | 1.548 | 0.619 | 0.555 | 1.445
25 | 3.931 | 0.153 | 0.459 | 1.541 | 0.606 | 0.565 | 1.435

Relevant Information

- Configuring SPC Parameters
- Configuring SPC Variables

# Viewing Statistical Results

1. On the Home view, select the Reports Tab. Then, on the left, select Statistics.

2. In the SPC Configuration window, enter the following parameters: Number of Subgroups, Subgroup Size, and Frequency.

3. Select the Plus icon at the upper-right corner of the GUI.
   The SPC Variable window shows the new variable.
   Configure the new SPC Variable.

4. In the SPC Variable window, select Calculate.

5. To show the statistical results, in the SPC Variable window, select View box.
   View box shows the date and time which the statistics results have been done.
   The statistical results are displayed through a histogram, the XBar-R chart, and the XBar-S chart.

   When all calculations on the filtered results are done, they are sent to the Web HMI and ToolsTalk 2.
   The statistics results are locally saved on a Temporary Internet Files folder (not saved on the controller).

   Statistical results can be displayed only on the Web HMI.

## Histogram

A histogram is a series of rectangles, each proportional in width to the range of values within a class and proportional in height to the number of samples falling in the class. A Gaussian curve follows the trend of the rectangles. A histogram reveals the amount of variation that any process has within it.
The histogram is useful because it emphasizes and clarifies trends that are not readily discernible in tables.

## XBar-R Chart

The XBar-R control chart shows both the mean value (XBar) and the range (R) of a subgroup. This is the most common type of control chart using indiscrete or continuous values. The XBar part of the chart shows any changes in the mean value of the process while the R part shows any changes in the dispersion of the process.
This chart is particularly useful because it shows changes in mean value and dispersion of the process at the same time, making it a very effective method for checking abnormalities in the process.

## XBar-S Chart

The XBar-S control chart shows both the mean value (XBar) Chart and the standard deviation (S) for each subgroup.
The XBar-S chart is identical to the XBar-R chart except that the R (range) is replaced by an S (standard deviation).

## Calculated Statistical Values

In the Web HMI the calculated statistical values are displayed in information boxes below the histogram, the XBar-R chart, and the XBar-S chart.

The calculated values depend on the chart which they are read on.

The calculated statistical values are:

- Min = minimum value for all collected sample values

- Max = maximum value for all collected sample values

- Mean =

- Mean+3Sigma = + 3*stdDev

- Mean-3Sigma = - 3*stdDev

- Cp (in XBar-R chart the value is based on range, and in XBar-S chart the value is based on sigma)

- Cpk (in XBar-R chart the value is based on range, and in XBar-S chart the value is based on sigma)

- Center line = in Range part , and in Sigma part

- Target (if available the target value for the monitor)

- Standard deviation = Total overall standard deviation = stdDev

Relevant Information

- Calculating Statistics
- Configuring SPC Parameters
- Configuring SPC Variables

# Troubleshooting and Service

This section provides assistance in troubleshooting problems, should they arise, and contains information to help you maintain and service the product.

In this Section

- Troubleshooting: WLAN and Bluetooth

# Troubleshooting: WLAN and Bluetooth

Problem | Possible cause | Solution
--- | --- | ---
Failed pairing (WLAN) | Tool has been restarted and lost connection to the controller | Pair tool with the controller
Failed pairing (WLAN) | Other tools are being paired at the same time | Make sure all other tools have exited pairing mode
Failed pairing (WLAN) | Tool is out of range | Move the tool closer to the controller and make sure you have a clear line of sight to the controller
Failed pairing (Bluetooth) | Other tools are being paired at the same time | Make sure all other tools have exited pairing mode
Failed pairing (Bluetooth) | Tool is out of range | Move the tool closer to the controller and make sure you have a clear line of sight to the controller
Failed pairing (Bluetooth) | Interference from other tools | The Bluetooth module can be sensitive; make sure to move other Bluetooth devices further away from the controller, or switch them off if possible
Failed pairing (Bluetooth) | All six slots have been filled and all six tools have been assigned to a Virtual Station | Remove one of the existing paired tools from the Virtual Station (in the Virtual Station menu, in the Tool field)
Tool disappeared from the Tool list (Bluetooth) | When pairing additional tools, existing tools will disappear from the connected tools list (in the Tools menu) | Press the tool trigger to make it appear in the list again
Tool disappeared from the Tool list (Bluetooth) | Tools may disappear from the list when the tool has been outside radio coverage | Make sure to be inside the radio coverage area and press the tool trigger to make it appear in the list again

# Reference

In this section, you can find miscellaneous useful information.

In this Section

- Terms and Definitions
- Input Signals
- Output Signals
- Input/Output Signals
- Third Party Licenses

# Terms and Definitions

Term | Synonym | Definition | Note
--- | --- | --- | ---
batch |  | multiple tightening using the same tightening program and socket |
batch sequence | sequence | multiple tightening using a combination of different tightening programs and sockets |
controller GUI |  | user interface at controller buttons or touch screen |
event |  | controller and tool status signals |
final angle |  | actual measured angle value at the end of the tightening cycle |
final torque |  | actual measured torque value at the end of the tightening cycle |
GUI |  | user interface made up of interactive graphical elements such as windows, icons and symbols on a display |
HMI | Human Machine Interface | user interface to tool or controller | The HMI can be a computer web-based interface or controller touch screen.
IAM | Intelligent Application Module | removable module in controller containing program, configuration parameters and tightening results |
line structure |  | sorting and grouping controllers in structures, folders or sub-folders in ToolsTalk | The line structure is a method for improving the visibility of a large group of controllers in a structured manner.
post view torque |  | function for monitoring and detecting torque maximum and minimum values before rundown is complete | One purpose of post view torque is the use of a self-locking nut.
Tightening program | Parameter set | configuration of parameters and values to control and monitor a single tightening action, and to store the tightening result |
push |  | transfer of data saved in ToolsTalk to the controller memory |
QIF | Quality Integrated Fastening | fully integrated line of nutrunners, controllers, accessories and process monitoring tools to guarantee high quality and traceability of tightening in industrial assembly systems | QIF was developed at Atlas Copco and is preferably used in motor vehicle industry and other assembly situations where many joints are critical. The QIF concept also includes process monitoring and documentation.
QIF accessory |  | accessory for operator communication and guidance used in QIF | Accessory products used for communication between system and operator. For example: scanner, operator panel, stacklight and socket selector. The communication provides improved quality and traceability in the assembly process.
quick step |  | tightening strategy | A tightening strategy to reduce the joint’s preload scatter by combining an initial step with a given speed and torque and then reducing the speed in the final step.
Re-hit detection |  | detection of re-tightening of an already tightened joint |
rotate |  | tightening strategy which rotates the tool head. | Rotate is mainly used for test or demonstration purposes.
rundown complete |  | end of the rundown step, when the screw head is in contact with the surface and the tightening step begins |
rundown step |  | step when a bolt enters the thread until the bolt head touches the surface |
snug |  | screw or bolt is approximately finger-tight to the surface |
socket selector |  | QIF accessory, consisting of a socket tray with lamps, that can be used to guide an operator to the correct socket |
soft start |  | start tightening at slow speed during a specified rotation angle | The function helps the bolt to enter the thread in a well controlled way and may prevent unwanted ergonomic tool movement when the trigger is pressed.
stacklight |  | QIF accessory, which handles the communication between operator and controller through digital signals like lamps, buttons, switches and buzzer |
target |  | desired result of a tightening | The target is expressed in torque or angle.
target angle |  | desired angle value at the end of the tightening cycle, measured from a reference point |
target torque |  | desired torque value at the end of the tightening cycle |
three step |  | tightening strategy | A tightening strategy to reduce the joint’s preload scatter and relaxation effects with an initial step with a given speed and torque followed by a short loosening step before the final tightening at reduced speed.
tightening step |  | step from when a bolt head has reached the surface until the tightening has reached the desired target torque or target angle |
tightening strategy |  | algorithm which continuously controls and monitors the tightening process | The user can select a strategy optimized for the joint and program certain parameters.
TurboTight |  | tightening strategy | A tightening strategy based on the tool’s maximum speed to perform fast and ergonomic tightening. The strategy requires only a target torque value to be set.
two step |  | tightening strategy | A tightening strategy to reduce the joint’s preload scatter and relaxation effects with an initial step with a given speed and torque, followed by a short-term stop, before the final tightening at reduced speed.
web GUI |  | user interface to controller through web browser window from a remote computer |
virtual station | virtual controller | software abstraction of a physical controller to behave like multiple controllers | A controller can have only one cable tool connected to it, but several wireless tools. Each tool is connected to its own virtual station.
Virtual station type |  | License containing a bundle of controller features. | This license is required for running a virtual station.
Virtual station feature |  | License for individual features. | Can be used to complement Virtual station type licenses.
Controller feature |  | License for controller-wide features, such as Soft PLC and StepSync. | Are assigned to an entire controller and can be used by all virtual stations.

# Input Signals

Converter
Signal Type
Value Type
Size Min [bit]
Size Max [bit]
Devices
Search

# Abort Sequence - 10012

When a Batch sequence abort request is received, the Batch sequence functionality aborts the batch sequence only after getting the ongoing tightening result.

Name in SoftPLC: ABORT_BATCH_SEQUENCE

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Abort Sequence and Clear Result- 10127

When signal "Abort sequence and clear results" is set, the ongoing sequence is aborted and signals related to "Clear results" are cleared.

Name in SoftPLC:ABORT_SEQ_AND_CLEAR_RES

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Acknowledge Events - 10004

Acknowledge of an event.

Name in SoftPLC: ACKNOWLEDGE_EVENT

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Activate Tool Scanner - 10075

Activates the tool scanner through an external source.

Name in SoftPLC: ACTIVATE_TOOL_SCANNER

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Batch Decrement - 10002

Incrementally decreases the batch counter by one.

Name in SoftPLC: BATCH_DECREMENT

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Batch Increment - 10001

Incrementally increases the batch counter by one.

Name in SoftPLC: BATCH_INCREMENT

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Bypass Identifier - 10123

In source batch string used to bypass an identifier string in string receiving sequence.

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Bypass Tightening Program - 10008

Skips the next tightening program in the running batch sequence.

Name in SoftPLC: BYPASS_PSET

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Disable Fieldbus - 10049

Disables the fieldbus.

Name in SoftPLC: DISABLE_FIELDBUS

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Filedbus: FALSE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Disable tool - 30000

If the signal is set to True, a tool is immediately stopped and locked.

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | Boolean | 1 | 1
Invert | State | Boolean | 1 | 1

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Disable Tool Scanner - 10119

Disables tool scanner when scanning by tool trigger when signal is set. It is still possible to scan by using the scan button but the scan string is ignored.

Name in SoftPLC: DISABLE_TOOL_SCANNER

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Dynamic Batch Size - 10074

Name in SoftPLC: DYNAMIC_BATCH_SIZE

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Integer | 1 | 16

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# External OK - 10063

Name in SoftPLC: EXTERNAL_OK

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Fieldbus Lock Loosening - 20021

A Virtual Station is locked when starting a loosening if the signal is set from a connected and supported accessory.
An ongoing loosening is aborted immediately when Fieldbus Lock Loosening is set to True, due to the Stop Drive setting.

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | Boolean | 1 | 1
Invert | State | Boolean | 1 | 1

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Fieldbus Lock Tightening - 20020

A Virtual Station is locked when starting a tightening if the signal is set from a connected and supported accessory.
An ongoing tightening is aborted immediately when Fieldbus Lock Tightening is set to True, due to the Stop Drive setting.

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | Boolean | 1 | 1
Invert | State | Boolean | 1 | 1

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Flush Read Result Queue - 30005

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# ID for Dynamic Batch Size - 10073

Name in SoftPLC: DYNAMIC_BATCH_SIZE_TPID

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | Integer | 1 | 16
TreatZeroAsOne | State | Integer | 1 | 16

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Lock Loosening - 20003

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Filedbus: FALSE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Lock Tightening - 20002

Tool locked for tightening by digital input.

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Filedbus: FALSE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Lock Tool Active High - 20004

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Filedbus: FALSE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Lock Tool Active Low - 20061

Locks the tool when this signal is low.

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Filedbus: FALSE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Manual Mode - 10061

Used to set the Virtual Station in manual mode.

If the signal is True (high) the signal 101 - Manual mode is high.
If the signal is False (low) the signal 101 - Manual mode is low.

Name in SoftPLC: SET_MANUAL_MODE

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | Boolean | 1 | 1
Invert | State | Boolean | 1 | 1

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

Relevant Information

- Manual Mode - 101

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Master Unlock - 10005

Master Unlock is an input signal which unlocks the following functions and signals.

FUNCTIONS:

- Disable loosening at OK tightening

- Disable loosening at NOK tightening

- Disable tightening

- Max consecutive NOK

- Tool Lock on Sequence complete

SIGNALS:

- 20001 - Pending Event Acknowledge Lock

- 20002 - Lock Tightening

- 20003 - Lock Loosening

- 20004 - Lock Tool Active High

- 20013 - WorkTask Lock Tightening

- 20014 - WorkTask Lock Loosening

- 20015 - Batch Done lLock

- 20018 - Open Protocol Lock

- 20020 - Fieldbus Lock Tightening

- 20021 - Fieldbus Lock Loosening

- 20022 - Disable Loosening At OK Tight

- 20023 - Too Many NOK Tightenings Lock

- 20033 - Line Control Lock

- 20034 - Locked By Alternative Identifier

Name in SoftPLC: MASTER_UNLOCK

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Pulse Stop - 10030

If this signal is generated any ongoing tightening or loosening will be stopped. Used in combination with 10024 or 10072.

Name in SoftPLC: TIGHTENING_STOP_PULSE

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Read Result Handshake Ack - 30004

Enable the Read Result Handshake feature in the Fieldbus device for making the controller available for the signal Rear Result Handshake Ack.

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

Relevant Information

- Configuration of the Fieldbus

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Reset All Identifiers - 10115

In Source batch string used to reset all received string identifiers from string receiving sequence at once. In other worktasks clears VIN number.

Name in SoftPLC: RESET_ALL_IDENTIFIERS

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Reset Batch - 10003

Resets the batch counter to 0. No batch OK (nxOK). If batch OK is activated, it will be deactivated.

Name in SoftPLC: RESET_BATCH

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Reset Batch Sequence - 10053

Resets the Batch Sequence. Unlocks a tool that is locked by Tool Lock on Complete.

Name in SoftPLC: RESET_BATCH_SEQUENCE

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Reset Bistable Relay - 10022

Reset the bistable relay output.

Name in SoftPLC: RESET_BISTABLE_RELAY

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Reset Latest Identifier - 10114

In Source batch string used to reset latest received string from string receiving sequence. In other worktasks clears VIN number.

Name in SoftPLC: RESET_LATEST_IDENTIFIER

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Reset Relays - 10120

Resets all signals.

Name in SoftPLC: RESET_RELAYS

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Reset Sequence Status - 10118

Resets signals Batch Sequence Done/OK/NOK and Sequence Aborted.

Name in SoftPLC: RESET_SEQUENCE_STATUS

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Reset Too Many NOK - 10013

Reset the batch after receiving lock Too Many NOK

Name in SoftPLC: RESET_TOO_MANY_NOK

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Select Input - 10020

Selects Tightening Program withing Source Tightening/Batch within sequence.

Name in SoftPLC: SELECT_INPUT_VALUE

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | Integer | 1 | 16
TreatZeroAsOne | State | Integer | 1 | 1

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: TRUE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Select Input and Dynamic Batch Size - 30007

It is used to set the Batch Size for a specific "Identifier Number" in a Source Tightening Task, running "External batch control".

Batch size can be set to 1-250.

If Batch size is set to 0, it is treated as infinite batch. The user is not able to un-set a Batch back to a state where it has no size, once it has been set.

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | Integer | 16 | 16
TreatZeroAsOne | State | Integer | 16 | 16

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Select Input Bit 0 - 10016

Name in SoftPLC: SEL_INPUT_BIT_0

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Filedbus: FALSE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Select Input Bit 1 - 10017

Name in SoftPLC: SEL_INPUT_BIT_1

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Filedbus: FALSE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Select Input Bit 2 - 10018

Name in SoftPLC: SEL_INPUT_BIT_2

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Filedbus: FALSE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Select Input Bit 3 - 10019

Name in SoftPLC: SEL_INPUT_BIT_3

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Filedbus: FALSE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Select Input Bit 4 - 10066

Name in SoftPLC: SEL_INPUT_BIT_4

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Filedbus: FALSE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Select Input Bit 5 - 10067

Name in SoftPLC: SEL_INPUT_BIT_5

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Filedbus: FALSE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Select Input Bit 6 - 10068

Name in SoftPLC: SEL_INPUT_BIT_6

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Filedbus: FALSE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Select Input Bit 7 - 10069

Name in SoftPLC: SEL_INPUT_BIT_7

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Filedbus: FALSE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Select Input Bit 8 - 10070

Name in SoftPLC: SEL_INPUT_BIT_8

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Filedbus: FALSE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Select Input Bit 9 - 10071

Name in SoftPLC: SEL_INPUT_BIT_9

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Filedbus: FALSE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Select Loosening - 10029

Selects loosening as default operation mode and used in combination with Start Tools -10028 signal.

Name in SoftPLC: SELECT_LOOSENING

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

Relevant Information

- Start Tools - 10028

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Select Next Identifier Number - 10116

It is possible to use the signal Select Next Identifier Number when a task in the virtual station is configured as:

- Batch Sequence

- Source Tightening

- Source Batch

  - Number Identifier method

  - String Identifier method

ST Selector configurable functions Take Next and Take Previous enable the input signals Select Next Identifier Number and Select Previous Identifier Number.

## Batch Sequence selected as Virtual Station Task

If Free Order switch has been enabled, the signal Select Next Identifier Number can select different batches within the selected sequence.

Before selecting batches, it is mandatory that they have the identifier number assigned. If a batch does not have the identifier number assigned, the signal Select Next Identifier Number cannot select it, even if Free Order switch is enabled.

It enables looping through the batches that have a configured identifier number.
If identifier number is "None", it is possible to select it only after all Batches with configured identifier number are completed.

It is possible to do looping, but 0 is skipped. When a batch is finished, it is no longer selectable.

For example, in case of batches with assigned identifier numbers 1,2,4,5, the signal runs in loop: 1,2,4,5,1,2,4... as long as the batches are not finished.

## Source Tightening selected as Virtual Station Task

The signal selects the next identifier number from the list of tightening programs specified in the Source Tightening task.
The selection runs from the currently selected identifier number to the next larger one.

When the biggest identifier number is selected, this signal selects 0; after 0, the signal selects the next bigger identifier number.

If 0 is selected as identifier number, the tool is locked.

If the identifier number has been added to the Source Tightening list, but no tightening program has ever been assigned to it, it is skipped while looping through the Source Tightening list.

If the tightening program is assigned to an identifier number and then it is removed from the list of tightening programs, it is still possible to select this identifier number. In this case, the tool is locked because there is not a specific tightening program.

When Selector Mode switch is set to Confirm, the socket selector needs to be assigned and configured. All tightening programs can be selected, but before running them, appropriate socket must be lifted from the socket selector.

## Source Batch selected as Virtual Station Task

In Sources > Batch Sequence > Source Batch, when the identifier method is set to Number, the signal Select Next Identifier Number selects sequences from a list of sequences shown in Source Batch task.

It is possible to do looping through 0. The signal Select Next Identifier Number selects only the identifier numbers assigned to sequences.

For example, if there are 4 sequences available with identifier numbers 1,2,4, and 8, the signal Select Next Identifier Number iterates and selects 1,2,4,8,0,1,2...

The identifier numbers not defined are not selected.

In Sources > Batch Sequence > Source Batch, when the identifier method is set to String, it is necessary to select the sequence through external sources (like scanner or Open Protocol). The signal Select Next Identifier Number is able to select the batches within the selected sequence.

Name in SoftPLC: SELECT_NEXT_ID_NUMBER

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

Relevant Information

- ST Selector
- Working with the Batch Sequence Tab

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: TRUE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Select Previous Identifier Number - 10117

It is possible to use the signal Select Previous Identifier Number when a task in the virtual station is configured as:

- Batch Sequence

- Source Tightening

- Source Batch

  - Number Identifier method

  - String Identifier method

ST Selector configurable functions Take Next and Take Previous enable the input signals Select Next Identifier Number and Select Previous Identifier Number.

## Batch Sequence selected as Virtual Station Task

If Free Order switch has been enabled, the signal Select Previous Identifier Number can select different batches within the selected sequence.

Before selecting batches, it is mandatory that they have the identifier number assigned. If a batch does not have the identifier number assigned, the signal Select Previous Identifier Number cannot select it, even if Free Order switch is enabled.

It enables looping through the batches that have a configured identifier number.
If identifier number is "None", it is possible to select it only after all Batches with configured identifier number are completed.

It is possible to do looping, but 0 is skipped. When a batch is finished, it is no longer selectable.

For example, in case of batches with assigned identifier numbers 1,2,4,5, the signal runs in loop: 5,4,2,1,5,4,2... as long as the batches are not finished.

## Source Tightening selected as Virtual Station Task

The signal selects the previous identifier number from the list of tightening programs specified in the Source Tightening task.
The selection runs from the currently selected identifier number to the previous lower one.

When the smallest identifier number is selected, this signal selects 0; after 0, the signal selects the next smaller identifier number.

If 0 is selected as identifier number, the tool is locked.

If the tightening program is assigned to an identifier number and then it is removed from the list of tightening programs, it is still possible to select this identifier number. In this case, the tool is locked because there is not a specific tightening program.

When Selector Mode switch is set to Confirm, the socket selector needs to be assigned and configured. All tightening programs can be selected, but before running them, appropriate socket must be lifted from the socket selector.

## Source Batch selected as Virtual Station Task

In Sources > Batch Sequence > Source Batch, when the identifier method is set to Number, the signal Select Previous Identifier Number selects sequences from a list of sequences shown in Source Batch task.

It is possible to do looping through 0. The signal Select Previous Identifier Number selects only the identifier numbers assigned to sequences.

For example, if there are 4 sequences available with identifier numbers 1,2,4, and 8, the signal Select Previous Identifier Number iterates and selects 8,4,2,1,0,8,4...

The identifier numbers not defined are not selected.

In Sources > Batch Sequence > Source Batch, when the identifier method is set to String, it is necessary to select the sequence through external sources (like scanner or Open Protocol). The signal Select Previous Identifier Number is able to select the batches within the selected sequence.

Name in SoftPLC: SELECT_PREVIOUS_ID_NUMBER

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

Relevant Information

- ST Selector
- Working with the Batch Sequence Tab

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: TRUE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Set Bistable Relay - 10021

Set the bistable relay output.

Name in SoftPLC: SET_BISTABLE_RELAY

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Socket Selector External Green Light - 10046

Controls green lights when socket selector is in external mode (how multiple physical devices are mapped to logical sockets are defined by the socket selector resource configuration).

- Byte0 - logical sockets 1-4

- Byte1 - logical sockets 5-8

- Byte2 - logical sockets 9-12

- Byte3 - logical sockets 13-16

- Byte4 - logical sockets 17-20

- Byte5 - logical sockets 21-24

- Byte6 - logical sockets 25-28

- Byte7 - logical sockets 29-32

2 bits per socket, 00=off, 01=flash, 10=solid

Name in SoftPLC: SOCKET_SEL_EXT_GREEN_LIGHT

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | uint64 | 1 | 64
SocketLedControlTwoDevices | State | uint64 | 1 | 64

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Socket Selector External Red Light - 10047

Controls red lights when socket selector is in external mode (how multiple physical devices are mapped to logical sockets are defined by the socket selector resource configuration).

- Byte0 - logical sockets 1-4

- Byte1 - logical sockets 5-8

- Byte2 - logical sockets 9-12

- Byte3 - logical sockets 13-16

- Byte4 - logical sockets 17-20

- Byte5 - logical sockets 21-24

- Byte6 - logical sockets 25-28

- Byte7 - logical sockets 29-32

2 bits per socket, 00=off, 01=flash, 10=solid

Name in SoftPLC: SOCKET_SEL_EXT_RED_LIGHT

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | uint64 | 1 | 64
SocketLedControlTwoDevices | State | uint64 | 1 | 64

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Soft PLC Lock Loosening - 20041

This signal is used to lock loosening from the SoftPLC.

Name in SoftPLC: LOCK_LOOSENING

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Filedbus: FALSE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Soft PLC Lock Tightening - 20040

This signal is used to lock tightening from the SoftPLC.

Name in SoftPLC: LOCK_TIGHTENING

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Filedbus: FALSE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Start Loosening - 10011

Active signal starts loosening. Once digital input goes inactive the loosening must be stopped.

Name in SoftPLC: START_LOOSENING

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Start Tightening - 10010

Active signal starts tightening. Once input goes inactive the tightening must be stopped.

Name in SoftPLC: START_TIGHTENING

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Start Tightening Pulse - 10024

The tightening starts at signal. Runs until the tightening is finished, or until the 30 sec timeout in tightening program occurs.

Name in SoftPLC: TIGHTENING_START_PULSE

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Start Tools - 10028

Active signal which starts the tool (default operation mode is tightening). As soon as signal goes inactive the tool must be stopped. Used in combination with Select Loosening - 10029 signal.

Name in SoftPLC: START_DRIVE_CONTINIOUS

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

Relevant Information

- Select Loosening - 10029

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# To SoftPLC - 10065

Name in SoftPLC: TO_PLC

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | uint8 array | 1 | 1

## Devices

- Filedbus: FALSE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Unlock Tool on Complete - 10051

Unlocks a tool that is locked by "Tool Lock on Complete".

Name in SoftPLC: UNLOCK_TOOL_ON_COMPLETE

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Unlock Tool on Disable - 10059

Name in SoftPLC: UNLOCK_TOOL_ON_DISABLE

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Output Signals

Converter
Signal Type
Value Type
Size Min [bit]
Size Max [bit]
Devices
Search

# Active Identifier String - 186

Set when an identifier string has been received and accepted by the work-task; it is necessary that even sequence or tightening program are running.
If running Source batch-string, it is set when all scans have been received and a sequence had been selected. In that case it includes concatenated string consisted of saved positions.
For other work-tasks it includes the “VIN” number.

Name in SoftPLC: ACTIVE_IDENTIFIER_STRING

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | String | 8 | 800
IdentifierU32Hnw | State | String | 8 | 800
IdentifierU32 | State | String | 8 | 800

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Active Identifier String 1 - 188

Signal corresponding to the first configured string in Source batch-string.
Active Identifier String 1 signal is sent once a scanning sequence is done and a sequence has been selected, thus the identifier parts are active.
The strings is filtered with saved position.
Only sent when running Source batch string.

Name in SoftPLC: ACTIVE_ID_STRING_1

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | String | 8 | 800
IdentifierU32Hnw | State | String | 8 | 800
IdentifierU32 | State | String | 8 | 800

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Active Identifier String 2 - 189

Signal corresponding to the second configured string in Source batch-string.
Active Identifier String 2 signal is sent once a scanning sequence is done and a sequence has been selected, thus the identifier parts are active.
The strings is filtered with saved position.
Only sent when running Source batch string.

Name in SoftPLC: ACTIVE_ID_STRING_2

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | String | 8 | 800
IdentifierU32Hnw | State | String | 8 | 800
IdentifierU32 | State | String | 8 | 800

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Active Identifier String 3 - 190

Signal corresponding to the third configured string in Source batch-string.
Active Identifier String 3 signal is sent once a scanning sequence is done and a sequence has been selected, thus the identifier parts are active.
The strings is filtered with saved position.
Only sent when running Source batch string.

Name in SoftPLC: ACTIVE_ID_STRING_3

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | String | 8 | 800
IdentifierU32Hnw | State | String | 8 | 800
IdentifierU32 | State | String | 8 | 800

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Active Identifier String 4 - 191

Signal corresponding to the fourth configured string in Source batch-string.
Active Identifier String 4 signal is sent once a scanning sequence is done and a sequence has been selected, thus the identifier parts are active.
The strings is filtered with saved position.
Only sent when running Source batch string.

Name in SoftPLC: ACTIVE_ID_STRING_4

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | String | 8 | 800
IdentifierU32Hnw | State | String | 8 | 800
IdentifierU32 | State | String | 8 | 800

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Batch Completed - 30

Batch Completed is an output signal which is triggered when the batch is complete.
The batch result status (OK or NOK) has no effect on the Batch Completed signal.

Name in SoftPLC: BATCH_COMPLETED

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Batch Completed NOK - 37

Batch finished with status NOK.

Name in SoftPLC: BATCH_COMPLETED_NOK

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Batch Completed OK - 36

Batch finished with status OK.

Name in SoftPLC: BATCH_COMPLETED_OK

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Batch Count - 31

Batch Count is an output signal which shows the current number of tightening in the batch.

Name in SoftPLC: BATCH_COUNT

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Integer | 1 | 8

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: TRUE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Batch Running - 32

Indicates that a batch in a batch sequence is running.

Name in SoftPLC: BATCH_RUNNING

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Batch Sequence Completed NOK - 46

Batch sequence finished with status NOK.

Name in SoftPLC: BATCH_SEQUENCE_NOK

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Batch Sequence Completed OK - 45

Batch sequence finished with status OK.

Name in SoftPLC: BATCH_SEQUENCE_OK

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Batch Sequence Done - 48

Indicates when a sequence is completed, both in case Batch Sequence Completed OK and Batch Sequence Completed NOK.

Name in SoftPLC: BATCH_SEQUENCE_COMPLETED

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | Event | Boolean | 1 | 1
Invert | Event | Boolean | 1 | 1

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Batch Sequence Running - 47

Indicates if the Batch Sequence is running or not.

Name in SoftPLC: BATCHSEQUENCE_RUNNING

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | Boolean | 1 | 1
Invert | State | Boolean | 1 | 1

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Bistable Relay - 40

Bistable Relay is a signal controlled by the inputs "Set Bistable Relay" and "Reset Bistable Relay".
After receiving the input "Set Bistable Relay", Bistable Relay signal is set to True.
After receiving the input "Reset Bistable Relay", Bistable Relay signal is set to False.

If "Set Bistable Relay" or "Reset Bistable Relay" goes low, the Bistable relay keeps its state.
The state for the Bistable relay changes when "Set Bistable Relay" or "Reset Bistable Relay" goes high.

After restarting the controller, the Bistable relay is set to False as default.

Name in SoftPLC: BISTABLE_RELAY

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | Boolean | 1 | 1
Invert | State | Boolean | 1 | 1

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Calibration Alarm - 138

The Calibration alarm from the Tool maintenance configuration. Provides a reminder for when it is time to calibrate the tool.

Name in SoftPLC: CALIBRATION_ALARM

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Configuration Version - 88

Name in SoftPLC: CONFIGURATION_VERSION

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Integer | 1 | 32

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Controller Switched On - 42

Set to true at start up of IO Exchange

Name in SoftPLC: IO_ON

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Current Running Batch - 180

Current Running Batch is an output signal which shows the index of the current running batch in a sequence.
If the user uses a socket selector, "Zero" appears if none, more than one, or wrong socket is selected.
If the user uses batch mode and a batch is running, "1" appears for Source Tightening configurations.

Name in SoftPLC: CURRENT_RUNNING_BATCH_IX

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Integer | 1 | 8

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: TRUE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Direction Switch CCW - 13

The direction switch on the tool is turned in counter clockwise direction.

Name in SoftPLC: DIRECTION_SWITCH_CCW

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Direction Switch CW - 12

The direction switch on the tool is turned in clockwise direction.

Name in SoftPLC: DIRECTION_SWITCH_CW

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Emergency Stop - 20036

Name in SoftPLC: EMERGENCY_STOP

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Event Code - 30001

Relay an event when it is triggered. Momentary, on for two cycle times.

Name in SoftPLC: EVENT_CODE

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Integer | 1 | 16

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Event Code Severity - 30003

Event Code Severity is an output signal which is activated when the triggered event has severity of error or warning.

Name in SoftPLC: EVENT_CODE_SEVERITY

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Event Present - 161

Indicates if event is triggered. It is only triggered on accessories if event requires an ACK.

Name in SoftPLC: EVENT_PRESENT

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Fieldbus Disconnected - 96

Name in SoftPLC: FIELDBUS_DISCONNECTED

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Filedbus: FALSE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Final Angle - 31003

Actual measured Angle value at the end of the tightening cycle.

Name in SoftPLC: FINAL_ANGLE

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Integer | 16 | 16

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Final Angle - 8

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Float | 0 | 0

## Devices

- Filedbus: FALSE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: TRUE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Final Angle Status - 31006

This signal shows the status of the final angle, which can be:

- OK - if the measured angle is within the limits configured in the tightening program.

- HIGH - if the measured angle is more than the high limit configured in the tightening program.

- LOW - if the measured angle is less than the low limit configured in the tightening program.

The value of the Final Angle Status signal shows differently, depending on the configuration of the fieldbus signal.
If the user selects the signal converter, the signal shows one of the following values:

- O - Final Angle Status OK.

- H - Final Angle Status High.

- L - Final Angle Status Low.

If there is no filter applied, the signal shows one of the following values:

- 1 - Final Angle Status OK.

- 2 - Final Angle Status High.

- 3 - Final Angle Status Low.

Name in SoftPLC: FINAL_ANGLE_STATUS

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | Integer | 2 | 8
StatusAsChar | State | Integer | 2 | 8

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Final Measured Current - 31017

Current at the measurement step of final angle and final torque. It is sent when a result is available.

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | Event | Integer | 32 | 32
FixedPointToDecimal | Event | Integer | 32 | 32

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Final Target Speed - 31020

The target speed of the last step of the tightening program.

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Integer | 16 | 16

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Final Target Torque - 31015

Gets the target torque of the tightening program for a performed tightening. The value is copied from the program of the tightening result and is published after the tightening.

The Multistep programs retrieve the Target Torque from the last tightening step in the tightening program defined as Step Category "Final".

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | Event | Integer | 32 | 32
FixedPointToDecimal | Event | Integer | 32 | 32

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Final Torque - 31002

Actual measured torque value at the end of the tightening cycle.

Name in SoftPLC: FINAL_TORQUE

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | Integer | 32 | 32
FixedPointToDecimal | State | Integer | 32 | 32

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Final Torque - 5

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Float | 1 | 1

## Devices

- Filedbus: FALSE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: TRUE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Final Torque Status - 31009

This signal shows the status of the final torque, which can be:

- OK - if the measured torque is within the limits configured in the tightening program.

- HIGH - if the measured torque is more than the high limit configured in the tightening program.

- LOW - if the measured torque is less than the low limit configured in the tightening program.

The value of the Final Torque Status signal shows differently, depending on the configuration of the fieldbus signal.
If the user selects the signal converter, the signal shows one of the following values:

- O - Final Torque Status OK.

- H - Final Torque Status High.

- L - Final Torque Status Low.

If there is no filter applied, the signal shows one of the following values:

- 1 - Final Torque Status OK.

- 2 - Final Torque Status High.

- 3 - Final Torque Status Low.

Name in SoftPLC: FINAL_TORQUE_STATUS

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | Integer | 2 | 8
StatusAsChar | State | Integer | 2 | 8

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# First Target Torque - 31019

Retrieves the first target torque after a completed tightening.

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | Event | Integer | 32 | 32
FixedPointToDecimal | Event | Integer | 32 | 32

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# From SoftPLC - 10064

Allocated bytes for data transfer from PLC to accessories.

Name in SoftPLC: FROM_PLC

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | uint8 array | 8 | 8

## Devices

- Filedbus: FALSE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# High Angle - 10

Angle result is too high.

Name in SoftPLC: HIGH_ANGLE

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# High Torque - 7

Torque result is higher than maximum torque limit.

Name in SoftPLC: HIGH_TORQUE

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Identifier Received - 100

Name in SoftPLC: IDENTIFIER_RECEIVED

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Last Received Identifier String - 187

Set directly when an identifier has been received in the work-task.
For Source batch-string, it is set at every scanning in scan process, thus it is changed for every scanning and sent even if it does not match in length.
String set is in raw format and not only "saved positions" in the string.
For other work-tasks this signal is equal to Active Identifier String signal.

Name in SoftPLC: LAST_RECEIVED_ID_STRING

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | String | 8 | 800
IdentifierU32Hnw | State | String | 8 | 800
IdentifierU32 | State | String | 8 | 800

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

Relevant Information

- Active Identifier String - 186

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# License Server Connection Lost - 134

Indicates that the connection to the Atlas Copco license server has been lost or the synchronization has failed. The signal is cleared when the License manager synchronization has been done successfully

Name in SoftPLC: LICENSE_SERVER_CONN_LOST

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Loosening Disabled - 184

Loosening Disabled is an output signal which is activated when the loosening is externally locked by any of the following signals:

- 20003 - Lock Loosening

- 20004 - Lock Tool Active High

- 20033 - Line Control Lock

- 20018 - Open Protocol Lock

- 20021 - Fieldbus Lock Loosening

- 20041 - Soft PLC Lock Loosening

- 20061 - Lock Tool Active Low

Name in SoftPLC: LOOSENING_DISABLED

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Loosening Enabled - 185

Loosening Disabled is an output signal which is activated when the loosening is not externally locked by any of the following signals:

- 20003 - Lock Loosening

- 20004 - Lock Tool Active High

- 20033 - Line Control Lock

- 20018 - Open Protocol Lock

- 20021 - Fieldbus Lock Loosening

- 20041 - Soft PLC Lock Loosening

- 20061 - Lock Tool Active Low

Name in SoftPLC: LOOSENING_ENABLED

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Loosening is Locked - 28

The loosening is disabled.

Name in SoftPLC: LOOSENING_IS_LOCKED

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | Boolean | 1 | 1
Invert | State | Boolean | 1 | 1

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Loosening NOK - 74

NOK loosening took place.

Name in SoftPLC: LOOSENING_NOK

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Loosening OK - 70

OK loosening took place.

Name in SoftPLC: LOOSENING_OK

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Low Angle - 9

Angle result is lower than minimum angle limit.

Name in SoftPLC: LOW_ANGLE

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Low Torque - 6

Torque result is lower than minimum torque limit.

Name in SoftPLC: LOW_TORQUE

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Manual Mode - 101

Indicates on any supported and configured accessory the Virtual Station status for manual mode

Name in SoftPLC: MANUAL_MODE

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | Boolean | 1 | 1
Invert | State | Boolean | 1 | 1

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Max Consecutive NOK Reached - 35

Indicates Max coherent NOK tightening counter is reachead.

Name in SoftPLC: MAX_COHERENT_NOK_REACHED

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Open End in Open Position - 89

Open End tool in open position.

Name in SoftPLC: OPEN_END_IN_OPEN_POSITION

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Filedbus: FALSE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Open Protocol Disconnected - 95

If Open Protocol is set to off in the Virtual Station, "Open Protocol Disconnected" signal is set to False.
If Open Protocol is turned on in the Virtual Station the "Open Protocol Disconnected" signal is set to True.
When at least one client (several Open Protocol clients can connect to the same Virtual Station) is connected the "Open Protocol Disconnected" signal is set to False.

Name in SoftPLC: OPEN_PROTOCOL_DISCONNECTED

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | Boolean | 1 | 1
Invert | State | Boolean | 1 | 1

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Pass-Through Identifier - 104

Output signal for sending a scanned string from a scanner to an external device.

Name in SoftPLC: BARCODE_ID_PASSTHROUGH

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | String | 8 | 800

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Program End - 168

This signal indicates the torque level when the tightening cycle is complete. A timer - Program end timeout - starts when the torque falls below this level. Tightening is complete when the torque has fallen below the level for Program end torque and stayed there until Program end timeout has been reached.

Name in SoftPLC: PROGRAM_END

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Program Start - 132

Defines the starting level for a tightening cycle.

Name in SoftPLC: PROGRAM_START

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Pulse Tool Alarm Oil Level Empty - 167

Oil level supervision configured in the Tool maintenance, provides a mechanism to remind the users when it is time to fill up oil on a pulse tool. The signal does not notify the user when the trigger gets pressed.
The signal is cleared when tool is disconnected; then, it is sent again from the tool if the condition prevails next time the tool is connected.

Name in SoftPLC: TOOL_OIL_LEVEL_EMPTY

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# PVT Compensate Value - 31029

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | Event | Integer | 32 | 32
FixedPointToDecimal | Event | Integer | 32 | 32

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Read Result Queue Flushed - 30006

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Ready to Start - 29

If a tool is connected to the virtual station, there is not any active tightening locks, emergency stop is not activated, and a valid Tightening Program is selected, this signal indicates that it is possible to start a tightening.

Name in SoftPLC: READY_TO_START

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | Boolean | 1 | 1
Invert | State | Boolean | 1 | 1

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Received Identifier 1 - 192

Signal corresponding to the first configured string in Source batch-string.
Active Identifier String 1 signal is sent in the order the strings/identifiers are received by the system as soon as a string has been received. If running in forced order scan, it is in the configured order, but if running free order scan, 1 might not correspond to the first configured string, but to the first received string.
The strings is the raw received string and not have the "saved position" applied.
Only sent when running Source batch string.

Name in SoftPLC: RECEIVED_IDENTIFIER_1

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | String | 8 | 800
IdentifierU32Hnw | State | String | 8 | 800
IdentifierU32 | State | String | 8 | 800

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Received Identifier 2 - 193

Signal corresponding to the second configured string in Source batch-string.
Active Identifier String 2 signal is sent in the order the strings/identifiers are received by the system as soon as a string has been received. If running in forced order scan, it is in the configured order, but if running free order scan, 2 might not correspond to the second configured string, but to the second received string.
The strings is the raw received string and not have the "saved position" applied.
Only sent when running Source batch string.

Name in SoftPLC: RECEIVED_IDENTIFIER_2

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | String | 8 | 800
IdentifierU32Hnw | State | String | 8 | 800
IdentifierU32 | State | String | 8 | 800

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Received Identifier 3 - 194

Signal corresponding to the third configured string in Source batch-string.
Active Identifier String 3 signal is sent in the order the strings/identifiers are received by the system as soon as a string has been received. If running in forced order scan, it is in the configured order, but if running free order scan, 3 might not correspond to the third configured string, but to the third received string.
The strings is the raw received string and not have the "saved position" applied.
Only sent when running Source batch string.

Name in SoftPLC: RECEIVED_IDENTIFIER_3

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | String | 8 | 800
IdentifierU32Hnw | State | String | 8 | 800
IdentifierU32 | State | String | 8 | 800

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Received Identifier 4 - 195

Signal corresponding to the fourth configured string in Source batch-string.
Active Identifier String 4 signal is sent in the order the strings/identifiers are received by the system as soon as a string has been received. If running in forced order scan, it is in the configured order, but if running free order scan, 4 might not correspond to the fourth configured string, but to the fourth received string.
The strings is the raw received string and not have the "saved position" applied.
Only sent when running Source batch string.

Name in SoftPLC: RECEIVED_IDENTIFIER_4

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | String | 8 | 800
IdentifierU32Hnw | State | String | 8 | 800
IdentifierU32 | State | String | 8 | 800

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Rehit - 31014

Name in SoftPLC: FIELDBUS_TIGHTENING_REHIT

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Remaining Batch - 33

Remaining tightenings in a batch. Can only be viewed on a display.

Name in SoftPLC: REMAINING_BATCH

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Integer | 1 | 8

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: TRUE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Rundown Angle - 31038

Value of the rundown angle.

Name in SoftPLC: RUNDOWN_ANGLE

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Integer | 16 | 16

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Rundown Angle High - 165

This signal is active if the rundown angle on the program level is higher than the set one.

Name in SoftPLC: RUNDOWN_ANGLE_HIGH

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Rundown Angle Low - 166

This signal is active if the rundown angle on the program level is lower than the set one.

Name in SoftPLC: RUNDOWN_ANGLE_LOW

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Selected Sequence Bit 0 - 139

Bit pattern showing selected sequence.

Name in SoftPLC: SELECTED_SEQUENCE_BIT_0

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Filedbus: FALSE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Selected Sequence Bit 1 - 140

Bit pattern showing selected sequence.

Name in SoftPLC: SELECTED_SEQUENCE_BIT_1

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Filedbus: FALSE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Selected Sequence Bit 2 - 141

Bit pattern showing selected sequence.

Name in SoftPLC: SELECTED_SEQUENCE_BIT_2

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Filedbus: FALSE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Selected Sequence Bit 3 - 142

Bit pattern showing selected sequence.

Name in SoftPLC: SELECTED_SEQUENCE_BIT_3

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Filedbus: FALSE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Selected Sequence Bit 4 - 143

Bit pattern showing selected sequence.

Name in SoftPLC: SELECTED_SEQUENCE_BIT_4

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Filedbus: FALSE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Selected Sequence Bit 5 - 144

Bit pattern showing selected sequence.

Name in SoftPLC: SELECTED_SEQUENCE_BIT_5

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Filedbus: FALSE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Selected Sequence Bit 6 - 145

Bit pattern showing selected sequence.

Name in SoftPLC: SELECTED_SEQUENCE_BIT_6

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Filedbus: FALSE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Selected Sequence Bit 7 - 146

Bit pattern showing selected sequence.

Name in SoftPLC: SELECTED_SEQUENCE_BIT_7

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Filedbus: FALSE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Selected Sequence Bit 8 - 147

Bit pattern showing selected sequence.

Name in SoftPLC: SELECTED_SEQUENCE_BIT_8

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Filedbus: FALSE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Selected Sequence Bit 9 - 163

Bit pattern showing selected sequence.

Name in SoftPLC: SELECTED_SEQUENCE_BIT_9

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Filedbus: FALSE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Selected Sequence Id - 84

Shows the index of the selected batch sequence.

Name in SoftPLC: SELECTED_BATCH_SEQUENCE_ID

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | Integer | 1 | 16
TreatZeroAsOne | State | Integer | 1 | 16

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: TRUE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Selected Tightening Program - 69

The actual id of a selected tightening program; 0 if no tightening program selected.

Name in SoftPLC: SELECTED_PSET_ID

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | Integer | 1 | 16
TreatZeroAsOne | State | Integer | 1 | 16

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: TRUE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Selected Tightening Program Bit 0 - 148

Bit pattern showing selected tightening program.

Name in SoftPLC: SELECTED_PROGRAM_BIT_0

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Filedbus: FALSE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Selected Tightening Program Bit 1 - 149

Bit pattern showing selected tightening program.

Name in SoftPLC: SELECTED_PROGRAM_BIT_1

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Filedbus: FALSE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Selected Tightening Program Bit 2 - 150

Bit pattern showing selected tightening program.

Name in SoftPLC: SELECTED_PROGRAM_BIT_2

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Filedbus: FALSE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Selected Tightening Program Bit 3 - 151

Bit pattern showing selected tightening program.

Name in SoftPLC: SELECTED_PROGRAM_BIT_3

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Filedbus: FALSE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Selected Tightening Program Bit 4 - 152

Bit pattern showing selected tightening program.

Name in SoftPLC: SELECTED_PROGRAM_BIT_4

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Filedbus: FALSE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Selected Tightening Program Bit 5 - 153

Bit pattern showing selected tightening program.

Name in SoftPLC: SELECTED_PROGRAM_BIT_5

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Filedbus: FALSE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Selected Tightening Program Bit 6 - 154

Bit pattern showing selected tightening program.

Name in SoftPLC: SELECTED_PROGRAM_BIT_6

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Filedbus: FALSE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Selected Tightening Program Bit 7 - 155

Bit pattern showing selected tightening program.

Name in SoftPLC: SELECTED_PROGRAM_BIT_7

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Filedbus: FALSE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Selected Tightening Program Bit 8 - 156

Bit pattern showing selected tightening program.

Name in SoftPLC: SELECTED_PROGRAM_BIT_8

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Filedbus: FALSE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Selected Tightening Program Bit 9 - 157

Bit pattern showing selected tightening program.

Name in SoftPLC: SELECTED_PROGRAM_BIT_9

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Filedbus: FALSE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Sequence Aborted - 160

Output signal indicating if sequence was aborted.

Name in SoftPLC: SEQUENCE_ABORTED

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Service Indicator Alarm - 137

Service alarm configured in the Tool maintenance, provides a mechanism to remind the users when it is time to service the tool.

Name in SoftPLC: SERVICE_INDICATOR_ALARM

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Size of Sequence - 181

Shows the size of the currently running sequence. Only set when a sequence is loaded and not reset when sequence is done.

Name in SoftPLC: SIZE_OF_RUNNING_SEQUENCE

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Integer | 1 | 8

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: TRUE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Socket Selector Disconnected Lock - 20039

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Software Major Version - 86

Name in SoftPLC: SOFTWARE_MAJOR_VERSION

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Integer | 1 | 32

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Software Minor Version - 87

Name in SoftPLC: SOFTWARE_MINOR_VERSION

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Integer | 1 | 32

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Software Release Version - 85

Version of the software running.

Name in SoftPLC: SOFTWARE_RELEASE_VERSION

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Integer | 1 | 32

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Start Final Angle - 31016

The Start Final Angle torque value is shown if available. It is sent when a result is available.

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | Integer | 32 | 32
FixedPointToDecimal | State | Integer | 32 | 32

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Station Ready - 71

Indicates when the Virtual Station is ready.

Name in SoftPLC: STATION_READY

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | Boolean | 1 | 1
Invert | State | Boolean | 1 | 1

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Target Torque - 30100

Signal displaying the target torque of a performed tightening.

Set Step Category of the last step to Final. The ST Selector displays Target Torque only if the last step has a torque target.

Name in SoftPLC: STSELECTOR_TARGET_TORQUE

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Integer | 1 | 1

## Devices

- Filedbus: FALSE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: TRUE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Target/Final Torque - 30101

Signal displaying the target/final torque alternatively.

Target/Final torque is between the target torque and the final torque if a selected tightening program is updated or a new tightening program is selected.

Set Step Category of the last step to Final. The ST Selector displays Target Torque only if the last step has a torque target.

Name in SoftPLC: STSELECTOR_TARGET_FINAL_TORQUE

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Integer | 1 | 1

## Devices

- Filedbus: FALSE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: TRUE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Thread Direction CCW - 26

Selected tightening program has counterclockwise chosen as thread direction.

Name in SoftPLC: THREAD_DIRECTION_CCW

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Tightening Date - 31030

Tightening date in the format YYYY:MM:DD.

Name in SoftPLC: TIGHTENING_DATE

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | String | 80 | 80

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Tightening Date Day - 31032

Day of month when the tightening was performed.

Name in SoftPLC: TIGHTENING_DATE_DAY

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Integer | 8 | 16

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Tightening Date Month - 31033

Month when the tightening was performed.

Name in SoftPLC: TIGHTENING_DATE_MONTH

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Integer | 8 | 16

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Tightening Date Year - 31034

Year when the tightening was performed.

Name in SoftPLC: TIGHTENING_DATE_YEAR

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Integer | 16 | 16

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Tightening Disabled - 182

Tightening Disabled is an output signal which is activated when the tightening is externally disabled by any of the following signals:

- 20002 - Lock Tightening

- 20004 - Lock Tool Active High

- 20033 - Line Control Lock

- 20018 - Open Protocol Lock

- 20020 - Fieldbus Lock Tightening

- 20040 - Soft PLC Lock Tightening

- 20061 - Lock Tool Active Low

Name in SoftPLC: TIGHTENING_DISABLED

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Tightening Done - 31010

Name in SoftPLC: TIGHTENING_DONE

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Tightening Enabled - 183

Tightening Enabled is an output signal which is activated when the tightening is not externally disabled by any of the following signals:

- 20002 - Lock Tightening

- 20004 - Lock Tool Active High

- 20033 - Line Control Lock

- 20018 - Open Protocol Lock

- 20020 - Fieldbus Lock Tightening

- 20040 - Soft PLC Lock Tightening

- 20061 - Lock Tool Active Low

Name in SoftPLC: TIGHTENING_ENABLED

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Tightening is Locked - 27

The tightening is disabled; it is not possible to make any tightening.

Name in SoftPLC: TIGHTENING_IS_LOCKED

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | Boolean | 1 | 1
Invert | State | Boolean | 1 | 1

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Tightening NOK - 4

At least one result of the tightening is outside the specified limits.

Name in SoftPLC: TIGHTENING_NOK

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Tightening OK - 3

The result of the tightening is within the specified limits.

Name in SoftPLC: TIGHTENING_OK

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Tightening Program Max Angle - 31004

Name in SoftPLC: MAX_ANGLE

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Integer | 16 | 16

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Tightening Program Max Torque - 31007

Name in SoftPLC: MAX_TORQUE

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | Integer | 32 | 32
FixedPointToDecimal | State | Integer | 32 | 32

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Tightening Program Min Angle - 31005

Name in SoftPLC: MIN_ANGLE

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Integer | 16 | 16

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Tightening Program Min Torque - 31008

Name in SoftPLC: MIN_TORQUE

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | Integer | 32 | 32
FixedPointToDecimal | State | Integer | 32 | 32

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Tightening Time - 31031

Tightening time in the format hh:mm:ss.

Name in SoftPLC: TIGHTENING_TIME

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | String | 64 | 64

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Tightening Time High - 135

Indicates if NOK tightenings occurred due to execution time exceeding the maximum allowed.

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- I/O Expander: TRUE

- TLS Tag: FALSE

# Tightening Time Hour - 31035

Hour when the tightening was performed.

Name in SoftPLC: TIGHTENING_TIME_HOUR

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Integer | 8 | 16

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Tightening Time Low - 136

Indicates if NOK tightenings occurred due to execution time lowering the minimum allowed.

Tightening Time Low signal works only for Tightening Programs.

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

Relevant Information

- Tightening Programs

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Tightening Time Minute - 31037

Minute when the tightening was performed.

Name in SoftPLC: TIGHTENING_TIME_MINUTES

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Integer | 8 | 16

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Tightening Time Second - 31036

Second when the tightening was performed.

Name in SoftPLC: TIGHTENING_TIME_SEC

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Integer | 8 | 16

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Tool Battery Low - 90

Name in SoftPLC: TOOL_BATTERY_LOW

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Tool Connected - 73

Indicates if a tool is connected or not to a Virtual Station.

Name in SoftPLC: TOOL_CONNECTED

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | Boolean | 1 | 1
Invert | State | Boolean | 1 | 1

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Tool Disabled - 158

Tool Disabled is an output signal which is activated when the tool is externally disabled by any of the following signals:

- 20002 - Lock Tightening

- 20003 - Lock Loosening

- 20004 - Lock Tool Active High

- 20033 - Line Control Lock

- 20018 - Open Protocol Lock

- 20020 - Fieldbus Lock Tightening

- 20021 - Fieldbus Lock Loosening

- 20040 - Soft PLC Lock Tightening

- 20041 - Soft PLC Lock Loosening

- 20061 - Lock Tool Active Low

Name in SoftPLC: TOOL_DISABLED

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Tool Enabled - 159

Tool Enabled is an output signal which is activated when the tool is not externally disabled by any of the following signals:

- 20002 - Lock Tightening

- 20003 - Lock Loosening

- 20004 - Lock Tool Active High

- 20033 - Line Control Lock

- 20018 - Open Protocol Lock

- 20020 - Fieldbus Lock Tightening

- 20021 - Fieldbus Lock Loosening

- 20040 - Soft PLC Lock Tightening

- 20041 - Soft PLC Lock Loosening

- 20061 - Lock Tool Active Low

Name in SoftPLC: TOOL_ENABLED

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Tool Function Button Pressed - 179

Output signal tracking the Function button state. The signal is set when the Function button is pressed and cleared when the Function button is released. Not for critical use in case of battery tools.

Name in SoftPLC: FUNCTION_BUTTON_PRESSED

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Tool Health OK - 103

Tool Health OK is High when there is no tool error present, while Tool Health OK is Low when any of the following tool errors are set:

- Tool Overheated

- Tool Requires motor tuning

- Open End not tuned

- Tool parameter file not supported

- Tool battery empty

- Tool trigger supervision failure

- Tool cable not supported

- Tool memory failure

- Tool memory corrupt

- Tool service interval expired

- Tool software version mismatch

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | Boolean | 1 | 1
Invert | State | Boolean | 1 | 1

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Tool LED Mirror Green - 98

Signal showing the tool green LED status on an accessory.

The Tool LED Mirror Green signal is set to True, if the tool green LED is ON/flashing.
The Tool LED Mirror Green signal is set to False, if the tool green LED is OFF.

Name in SoftPLC: TOOL_RESULT_LED_GREEN

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Tool LED Mirror Red - 97

Signal showing the tool red LED status on an accessory.

The Tool LED Mirror Red signal is set to True, if the tool red LED is ON/flashing.
The Tool LED Mirror Red signal is set to False, if the tool red LED is OFF.

Name in SoftPLC: TOOL_RESULT_LED_RED

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Tool LED Mirror Yellow - 99

Signal showing the tool yellow LED status on an accessory.

The Tool LED Mirror Yellow signal is set to True, if the tool yellow LED is ON/flashing.
The Tool LED Mirror Yellow signal is set to False, if the tool yellow LED is OFF.

Name in SoftPLC: TOOL_RESULT_LED_YELLOW

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Tool Loosening - 22

Indicates that the tool is loosening.

Name in SoftPLC: TOOL_LOOSENING

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Tool Rotation CCW - 25

Tool rotation direction is counterclockwise for left-handed threaded screws.

Name in SoftPLC: TOOL_ROTATION_CCW

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Tool Rotation CW - 24

Tool rotation direction is clockwise for right-handed threaded screws.

Name in SoftPLC: TOOL_ROTATION_CW

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Tool Running - 23

Indicates that the tool is rotating (clockwise [CW] or counter-clockwise [CCW]).

Name in SoftPLC: TOOL_RUNNING

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Tool Serial Number Numeric - 31021

Integer part of the serial number.

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Integer | 32 | 32

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Tool Tag Identifier - 94

Name in SoftPLC: TOOLTAG_IDENTIFIER

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | String | 8 | 800

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Tool Tightening - 21

Indicates that the tool is tightening.

Name in SoftPLC: TOOL_TIGHTENING

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# ToolsNet Connection Lost - 133

Indicates if enabled connection between ToolsNet and controller got interrupted or is working as expected.

Name in SoftPLC: TOOLSNET_CONNECTION_LOST

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Total Number of Tightenings - 31018

Total number of the tightenings performed by the tool over its entire lifetime.

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Integer | 8 | 32

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Trigger pressed - 11

Indicates that the tool trigger has been pressed.

Name in SoftPLC: TRIGGER_PRESSED

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Virtual Station Name - 105

Provides the virtual station name.

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | String | 8 | 800

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Input/Output Signals

Converter
Signal Type
Value Type
Size Min [bit]
Size Max [bit]
Devices
Search

# Clear Results - 39

Clears status of other signals set to next tightening.

Name in SoftPLC: CLEAR_RESULTS

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Disable Open Protocol Commands - 10060

Disables the possibility to send commands over Open Protocol to the Virtual Station.

Name in SoftPLC: DISABLE_OPEN_PRTCOL_CMDS

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | Boolean | 1 | 1
Invert | State | Boolean | 1 | 1

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# External Identifier - 10045

The string sent in External identifier is included in the result as VIN number. It is possible to provide up to 2 identifiers to be passed from Fieldbus for task selection.

Name in SoftPLC: EXTERNAL_IDENTIFIER

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | String | 8 | 800
IdentifierU32Hnw | State | String | 8 | 800
IdentifierU32 | State | String | 8 | 800

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# External Monitored 1 - 10035

External Monitored 1 is an Input/Output signal that is not attached to any specific feature in the controller and can be used for customer specific needs.

Name in SoftPLC: EXTERNAL_MONITORED_1

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | Boolean | 1 | 1
Invert | State | Boolean | 1 | 1

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# External Monitored 2 - 10036

External Monitored 2 is an Input/Output signal that is not attached to any specific feature in the controller and can be used for customer specific needs.

Name in SoftPLC: EXTERNAL_MONITORED_2

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | Boolean | 1 | 1
Invert | State | Boolean | 1 | 1

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# External Monitored 3 - 10037

External Monitored 3 is an Input/Output signal that is not attached to any specific feature in the controller and can be used for customer specific needs.

Name in SoftPLC: EXTERNAL_MONITORED_3

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | Boolean | 1 | 1
Invert | State | Boolean | 1 | 1

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# External Monitored 4 - 10038

External Monitored 4 is an Input/Output signal that is not attached to any specific feature in the controller and can be used for customer specific needs.

Name in SoftPLC: EXTERNAL_MONITORED_4

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | Boolean | 1 | 1
Invert | State | Boolean | 1 | 1

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# External Monitored 5 - 10039

External Monitored 5 is an Input/Output signal that is not attached to any specific feature in the controller and can be used for customer specific needs.

Name in SoftPLC: EXTERNAL_MONITORED_5

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | Boolean | 1 | 1
Invert | State | Boolean | 1 | 1

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# External Monitored 6 - 10040

External Monitored 6 is an Input/Output signal that is not attached to any specific feature in the controller and can be used for customer specific needs.

Name in SoftPLC: EXTERNAL_MONITORED_6

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | Boolean | 1 | 1
Invert | State | Boolean | 1 | 1

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# External Monitored 7 - 10041

External Monitored 7 is an Input/Output signal that is not attached to any specific feature in the controller and can be used for customer specific needs.

Name in SoftPLC: EXTERNAL_MONITORED_7

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | Boolean | 1 | 1
Invert | State | Boolean | 1 | 1

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# External Monitored 8 - 10042

External Monitored 8 is an Input/Output signal that is not attached to any specific feature in the controller and can be used for customer specific needs.

Name in SoftPLC: EXTERNAL_MONITORED_8

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | Boolean | 1 | 1
Invert | State | Boolean | 1 | 1

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Fieldbus Keep Alive - 30002

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Integer | 1 | 8

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Flash Tool Green LED (external protocol) - 10058

Name in SoftPLC: FLASH_TOOL_GREEN_LED

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Generic I/O 1 - 50

Input/Output 1 used for Open Protocol.

Name in SoftPLC: GENERIC_IO_1

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Integer | 1 | 8

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: TRUE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Generic I/O 2 - 51

Input/Output 2 used for Open Protocol.

Name in SoftPLC: GENERIC_IO_2

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Integer | 1 | 8

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: TRUE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Generic I/O 3 - 52

Input/Output 3 used for Open Protocol.

Name in SoftPLC: GENERIC_IO_3

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Integer | 1 | 8

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: TRUE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Generic I/O 4 - 53

Input/Output 4 used for Open Protocol.

Name in SoftPLC: GENERIC_IO_4

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Integer | 1 | 8

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: TRUE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Generic I/O 5 - 54

Input/Output 5 used for Open Protocol.

Name in SoftPLC: GENERIC_IO_5

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Integer | 1 | 8

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: TRUE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Generic I/O 6 - 55

Input/Output 6 used for Open Protocol.

Name in SoftPLC: GENERIC_IO_6

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Integer | 1 | 8

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: TRUE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Generic I/O 7 - 56

Input/Output 7 used for Open Protocol.

Name in SoftPLC: GENERIC_IO_7

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Integer | 1 | 8

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: TRUE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Generic I/O 8 - 57

Input/Output 8 used for Open Protocol.

Name in SoftPLC: GENERIC_IO_8

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Integer | 1 | 8

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: TRUE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Generic I/O 9 - 58

Input/Output 9 used for Open Protocol.

Name in SoftPLC: GENERIC_IO_9

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Integer | 1 | 8

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: TRUE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Generic I/O 10 - 59

Input/Output 10 used for Open Protocol.

Name in SoftPLC: GENERIC_IO_10

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Integer | 1 | 8

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: TRUE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Generic Rising Edge 1 - 169

Generic Input/Output signal.

Name in SoftPLC: GENERIC_RISING_EDGE_1

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Generic Rising Edge 2 - 170

Generic Input/Output signal.

Name in SoftPLC: GENERIC_RISING_EDGE_2

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Generic Rising Edge 3 - 171

Generic Input/Output signal.

Name in SoftPLC: GENERIC_RISING_EDGE_3

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Generic Rising Edge 4 - 172

Generic Input/Output signal.

Name in SoftPLC: GENERIC_RISING_EDGE_4

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Generic Rising Edge 5 - 173

Generic Input/Output signal.

Name in SoftPLC: GENERIC_RISING_EDGE_5

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Generic Rising Edge 6 - 174

Generic Input/Output signal.

Name in SoftPLC: GENERIC_RISING_EDGE_6

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Generic Rising Edge 7 - 175

Generic Input/Output signal.

Name in SoftPLC: GENERIC_RISING_EDGE_7

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Generic Rising Edge 8 - 176

Generic Input/Output signal.

Name in SoftPLC: GENERIC_RISING_EDGE_8

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Generic Rising Edge 9 - 177

Generic Input/Output signal.

Name in SoftPLC: GENERIC_RISING_EDGE_9

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Generic Rising Edge 10 - 178

Generic Input/Output signal.

Name in SoftPLC: GENERIC_RISING_EDGE_10

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE

# Socket Lifted - 10014

Is generated when a unique socket is lifted on socket selector (integer = socket ID), no socket is lifted (integer = 0) or when more than one is lifted (integer = 0).

Name in SoftPLC: SOCKET_LIFTED

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Integer | 1 | 32

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Socket Lifted Raw - 10043

Added to support backwards compatibility with PF4000 in certain protocols for socket lifted notifications (as opposed to Socket Lifted 10013). Integer is bit pattern for all lifted sockets (regardless of flashing or how many is lifted).

Name in SoftPLC: SOCKET_LIFTED_RAW

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | uint64 | 1 | 32
SocketSelectorTwoDevices | State | uint64 | 1 | 32

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Tool in Production Space - 93

Name in SoftPLC: TOOL_IN_PRODUCT_SPACE

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# Tool in Work Space - 92

Name in SoftPLC: TOOL_IN_WORK_SPACE

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE

# User ID - 10050

Name in SoftPLC: USER_ID

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | String | 8 | 800

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

# Third Party Licenses

# List of Third-Party Licenses

Power Focus controllers incorporate third party components whose licenses require us to publish copies of the licensing language and/or copyright notices. In compliance with those requirements, here are copies of the licenses. Please, click on any of the licenses below to show a copy of the license text.

Software | Version | Licenses
--- | --- | ---
acl | 2.2.52 | GPL v2.0 LGPL v2.1
alsa-lib | 1.1.2 | GPL v2.0 LGPL v2.1
alsa-state | 0.2.0 | MIT
alsa-tools | 1.1.0 | GPL v2.0 LGPL v2.0
alsa-utils | 1.1.2 | GPL v2.0
anybus | 1.1 | Proprietary
atftp | 0.7.1 + gitAUTOINC + be3291a18c | GPL v2.0
attr | 2.4.47 | GPL v2.0 LGPL v2.1
barebox | 2018.06.0 | GPL v2.0
base-files | 3.0.14 | GPL v2.0
base-files-px2-base | 1.0 | MIT
base-passwd | 3.5.29 | GPL v2.0
bash | 4.3.30 | GPL v3.0
bash-completion | 2.4 | GPL v2.0
bluez5 | 5.41 | GPL v2.0 LGPL v2.1
boost | 1.61.0 | MIT BSL v1.0 Python v2.0
busybox-px2base | 1.24.1 | GPL v2.0 bzip v2.0
bzip2 | 1.0.6 | bzip v2.0
ca-certificates | 20160104 | GPL v2.0 MPL v2.0
cppunit | 1.13.1 | LGPL v2.1
cryptodev-linux | 1.8 | GPL v2.0
curl | 7.50.1 | MIT
db | 3.0.35 | AGPL v3.0
dbus | 1.10.10 | GPL v2.0 AFL v2.0
dhcp | 4.3.4 | ISC
dosfstools | 4.0 | GPL v3.0
dt-utils | 2017.03.0 | GPL v2.0
e2fsprogs | 1.43 | GPL v2.0 LGPL v2.0 BSD MIT
ecryptfs-tools | 1.0 | GPL v1.0
elfutils | 0.166 | GPL v3.0 Elfutils-Exception
eudev | 3.2.2 | GPL v2.0 LGPL v2.1
expat | 2.2.0 | MIT
fbset | 2.1 | GPL v2.0
fb-test | 1.1.0 | GPL v2.0
fcgi | 2.4.0 | OML
finit | 3.1 | MIT
firmware-imx | 5.4 | Proprietary
flac | 1.3.1 | GPL v2.0 LGPL v2.1 BSD GFDL v1.2
flatbuffers | 1.9.0 | Apache v2.0
fruit | 3.4.0 + gitAUTOINC + ece0f7218c | Apache v2.0
fuse | 2.9.4 | GPL v2.0 LGPL v2.0
gcc-runtime | 6.2.0 | GPL v3.0 with GCC exception
gdb | 8.0.1 | GPL v2.0 LGPL v2.0 GPL v3.0 LGPL v3.0
gdbm | 1.12 | GPL v3.0
glib-2.0 | 2.48.2 | LGPL v2.0 BSD Public Domain License
glibc | 2.24 | GPL v2.0 LGPL v2.1
gmp | 6.1.1 | GPL v2.0 LGPL v3.0
gnutls | 3.5.3 | GPL v3.0 LGPL v2.1
grep | 2.25 | GPL v3.0
gstreamer1.0 | 1.8.3 | LGPL v2.0
gstreamer1.0-plugins-base | 1.8.3 | GPL v2.0 LGPL v2.0
hostpad | 2.6 | GPL v2.0 BSD
htop | 1.0.3 | GPL v2.0
icu | 57.1 | ICU
init-ifupdown | 1.0 | GPL v2.0
initscripts | 1.0 | GPL v2.0
iproute2 | 4.7.0 | GPL v2.0
iptables | 1.6.0 | GPL v2.0
ipwatchd | 1.2 | GPL v2.0
iw | 4.7 | BSD
json-spirit | 4.08 | MIT
keyutils | 1.5.9 | GPL v2.0
kmod | 23 + gitAUTOINC + 65a885df5f | GPL v2.0 LGPL v2.1
kmsfbwrap-px2base | 12.0 | GPL v2.0
libarchive | 3.2.2 | BSD
libbsd | 0.8.3 | BSD v4 Clause ISC Public Domain License
libcap | 2.25 | GPL v2.0 BSD
libdrm | 2.4.70 | MIT
libestr | 0.1.10 | LGPL v2.1
libevent | 2.0.22 | BSD
libfastjson | 0.99.4 | MIT
libffi | 3.2.1 | MIT
libgcc | 6.2.0 | GPL v3.0 with GCC exception GPL v3.0
libgcrypt | 1.7.3 | GPL v2.0 LGPL v2.1 GPL v3.0
libgpg-error | 1.24 | GPL v2.0 LGPL v2.1
libidn | 1.33 | LGPL v3.0 LGPL v2.1 GPL v3.0
libite | 2.0.2 | BSD ISC MIT
libjpeg-turbo | 1.5.0 | BSD v3 Clause
liblogging | 1.0.5 | BSD
libnet | 1.2-rc3 | BSD
libnfsidmap | 0.25 | BSD
libnl | 3.2.28 | LGPL v2.1
libogg | 1.3.2 | BSD
libpcap | 1.8.1 | BSD
libpcre | 8.39 | BSD
libpng | 1.6.24 | Libpng
librcf | 2.2.0.0 | GPL v2.0
libsamplerate0 | 0.1.8 | GPL v2.0
libsndfile1 | 1.0.27 | LGPL v2.1
libtinyxml | 2.6.2 | Zlib
libtirpc | 1.0.1 | BSD
libuev | 2.2.0 | MIT
libusb1 | 1.0.20 | LGPL v2.1
libvorbis | 1.3.5 | BSD
libxml2 | 2.9.4 | MIT
libxslt | 1.1.29 | MIT
lighttpd | 1.4.51 | BSD
linux-atlas | 4.14 | GPL v2.0
linux-libc-headers | 4.14.13 | GPL v2.0
logrotate | 3.9.1 | GPL v2.0
lua | 5.1.5 | MIT
luabind | git | MIT
lzo | 2.09 | GPL v2.0
lzop | 1.03 | GPL v2.0
memlog | 2.0 | MIT
mesa | 12.0.1 | MIT
mg | 20161005 | Public Domain License
minizip | 1.2.8 | Zlib
mmc-utils | 0.1 | GPL v2.0
mtd-utils | 1.5.2 | GPL v2.0
nano | 2.2.5 | GPL v3.0
ncurses | 6.0 + 20160625 | MIT
netbase | 5.3 | GPL v2.0
netcat-openbsd | 1.105 | BSD v3 Clause
nettle | 3.2 | GPL v2.0 LGPL v3.0
nfs-utils | 2.1.1 | GPL v2.0 BSD MIT
ntp | 4.2.8p8 | NTP
openssh | 7.6p1 | BSD
openssl | 1.0.2n | openSSL
opkg | 0.3.3 | GPL v2.0
opkg-arch-config | 1.0 | MIT
opkg-utils | 0.3.2 + gitAUTOINC + 3ffece9bf1 | GPL v2.0
orc | 0.4.25 | BSD v3 Clause BSD v2 Clause
os-release | 1.0 | MIT
packagegroup-atlas-qt5 | 1.0 | MIT
packagegroup-atlas-sxb | 1.0 | MIT
packagegroup-base | 1.0 | MIT
packagegroup-core-boot | 1.0 | MIT
packagegroup-core-eclipse-debug | 1.0 | MIT
packagegroup-core-nfs | 1.0 | MIT
packagegroup-core-ssh-openssh | 1.0 | MIT
packagegroup-px2it | 1.0 | MIT
parted | 3.2 | GPL v3.0
perl | 5.22.1 | GPL v1.0 Artistic v1.0
pm-utils | 1.4.1 | GPL v2.0
poco | 1.9.0 | BSL v1.0
pointercal | 0.0 | MIT
popt | 1.16 | MIT
procps | 3.3.12 | GPL v2.0 LGPL v2.0
protobuf | 2.6.1 + gitAUTOINC + bba83652e1 | BSD v3 Clause
python | 2.7.12 | Python v2.0
qtbase | 5.7.1 + gitAUTOINC + a55f36211e | BSD GPL v2.0 GPL v3.0 GFDL v1.3 LGPL v3.0 The Qt Company Commercial The Qt Company LGPL Exception v1.0
qtdeclarative | 5.7.1 + gitAUTOINC + 2a992040e2 | BSD GPL v2.0 GPL v3.0 GFDL v1.3 LGPL v3.0 The Qt Company Commercial The Qt Company LGPL Exception v1.0
qtlocation | 5.7.1 + gitAUTOINC + de5be121d8 | BSD GPL v2.0 LGPL v2.1 GFDL v1.3 LGPL v3.0 The Qt Company LGPL Exception v1.1
qtsensors | 5.7.1 + gitAUTOINC + 5a57beaaa5 | BSD GPL v2.0 GPL v3.0 GFDL v1.3 LGPL v3.0 The Qt Company Commercial The Qt Company LGPL Exception v1.0
qtwebkit | 5.7.1 + gitAUTOINC + 76e2732f01 | BSD GPL v2.0 LGPL v2.0
qtwebsockets | 5.7.1 + gitAUTOINC + 60cede232a | GFDL v1.3 LGPL v2.1 LGPL v3.0 The Qt Company LGPL Exception v1.1
qtxmlpatterns | 5.7.1 + gitAUTOINC + 89dbcc4f80 | BSD GPL v2.0 GPL v3.0 GFDL v1.3 LGPL v3.0 The Qt Company Commercial The Qt Company LGPL Exception v1.0
rauc | 0.4 | LGPL v2.1
readline | 6.3 | GPL v3.0
rpcbind | 0.2.3 | BSD
rsync | 3.1.2 | GPL v3.0
rsyslog | 8.22.0 | Apache v2.0 GPL v3.0 LGPL v3.0
run-postinsts | 1.0 | MIT
shadow | 4.2.1 | BSD Artistic v1.0
shadow-security | 4.2.1 | MIT
sqlite3 | 3.14.1 | Public Domain License
squashfs-tools | 5.7.1 + gitrAUTOINC + 9c1db6d13a | Public Domain License GPL v2.0
st-load | 1.0 | Public Domain License
stm32flash | git | GPL v2.0
strace | 4.13 | BSD
sysfsutils | 2.1.0 | GPL v2.0 LGPL v2.1
sysvinit-bootlogd | 2.88dsf | GPL v2.0
tcf-agent | 1.4.0 + gitAUTOINC + 2dddd5f440 | EDL v1.0 EPL v1.0
tcpdump | 4.7.4 | BSD
tcp-wrappers | 7.6 | BSD
tslib | 1.1 | LGPL v2.0
tzdata | 2016i | BSD BSD v3 Clause Public Domain License
u-boot-atlas | 2017.09 | GPL v2.0
u-boot-fw-utils | 2017.09 | GPL v2.0
unzip | 6.0 | BSD v3 Clause
usbutils | 008 | GPL v2.0
util-linux | 2.28.1 | BSD GPL v2.0 LGPL v2.1
wireless-tools | 30.pre9 | BSD GPL v2.0 LGPL v2.1 MPL v1.1
wpa-supplicant | 2.5 | BSD
xerces-c | 2.7.0 | Apache v2.0
xz | 5.2.2 | GPL v2.0 LGPL v2.1 GPL v3.0 with autoconf exception Public Domain License
yaml-cpp | 0.6.2 | MIT
zip | 3.0 | BSD v3 Clause
zlib | 1.2.8 | Zlib