# Pairing mode for STB tool and STwrench

## Placing the STB Tool in Pairing Mode

1. Disconnect the (charged) battery from the tool.

2. Press the tool trigger while re-attaching the battery.

3. When the tool LEDs are off, release the tool trigger.

4. When the tool LEDs are on again, press the tool trigger.

5. When the tool LEDs are off again, release the tool trigger. Both LEDs start to flash (after approximately 10 seconds).

6. The tool is now in pairing mode. The LEDs keep flashing when the tool is in pairing mode.

Do not start the Power Focus pairing procedure before both LEDs on the tool are flashing. Initiate pairing within 30 seconds or the tool might time out.

When the tool is placed in pairing mode, tap the connection type to start the pairing process.

## Placing the STwrench in pairing mode

1. Turn on the STwrench.

2. During the cell and gyroscope adjustment, press the UP, RIGHT and BARCODE buttons on the STwrench keyboard in that order.

3. At the end of the zero adjustment, the wrench is in pairing mode.

When the tool is placed in pairing mode, tap the connection type to start the pairing process.