# Pass-Through Identifier - 104

Output signal for sending a scanned string from a scanner to an external device.

Name in SoftPLC: BARCODE_ID_PASSTHROUGH

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | String | 8 | 800

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE