# Accessing the Controller On Lan

Select the Settings menu, and click on Edit to access the Factory Ethernet port window. There you can alter the Ethernet settings.

Connect the network cable to the Factory Ethernet port and then either manually specify the required information or, if available, use the information provided by the DHCP server. Required information is:

- IP address

- Subnet mask

- Gateway

This information is provided by the local system administrator.

When using the manual option there are optional settings available for the use of DNS servers.