# Configuring Fieldbus Window in a Virtual Station

The Fieldbus entry in the GUI shows the fieldbus mapping assigned to the controller.

To analyze the fieldbus configuration click on perform in the diagnostics field for the fieldbus mapping. Read more about the diagnostics tool in the Virtual station - Accessories section of this chapter.

To configure Fieldbus mappings, ToolsTalk 2 is required.

Virtual station - Fieldbus