# Exporting "Logs from Connected Tools"

The export of tool logs enables a service technician to share the tool log data with Atlas Copco Service personnel to troubleshoot problems with the tool(s).

It is possible to export tool logs from the following tools: STB, SRB and TBP/TBP-S.

To export the tool logs, the tool has to be connected to the controller. It is not necessary for the tool to be assigned to a Virtual Station.

All data included in the tool log export is stored in a file "PFExport_<IAM name>_<datetime>.tar.gz", which includes the following files and directories:

- "atlas_tool_i.zip" – All available results

  For each connected tool an individual files is created. The file format for tool log files is "tool-<tool type>-<tool serial number>.log"

- "ExportInfo.txt" - Text document containing information about the IAM, Controller and connected tools

## How to Export "Logs from Connected Tools"

1. On the Home view, select the Controller Tab. Then, on the left side, select the Export/Import Tab .

2. In the Export window, open the drop-down menu and select Logs from connected tools.

3. In the Export window, select Export.
   At the end of the exporting process, an exporting pop-up window confirms that the export is done.
   A PFExport_<IAM name>_<datetime>.tar.gz file is automatically downloaded.