# Configuration of the Function Button

Use the function button on the tool to control up to six of the available input signals. The button’s three possible condition states are combined with the two possible states of the direction switch.

Function button states | Direction switch states
--- | ---
Single push | CW
Single push | CCW
Double push | CW
Double push | CCW
Pressed | CW
Pressed | CCW

Two configurable parameters controls the push time.

Parameter | Description | Default value
--- | --- | ---
Push detection interval | For single push: the maximum push time (in milliseconds) between the button being pressed and the button being released. | 300 ms
Next push interval | For double push: the maximum time (in milliseconds) between the button being released after the first push, and the buttong being pressed again. | 300 ms