# NOK Results List

Error message | Description | GUI location
--- | --- | ---
Drive error | Internal driver error or driver loss detected. | N/A
Rehit | Attempt to tighten an already tightened bolt. | Tightening parameters (Edit) > Rehit detection
Soft start torque above max | Soft start torque exceeded maximum level. | Tightening parameters (Edit) > (Step 1) Soft Start > Torque max
Selftap torque above max | Selftap torque exceeded maximum level. | Tightening parameters (Edit) > (Step 2) Selftap > Torque max
Selftap torque below min | Selftap torque below minimum limit. | Tightening parameters (Edit) > (Step 2) Selftap > Torque min
Safety torque limit low | Automatically calculated torque value to ensure torque sensor is mounted correctly. | N/A
Rundown torque above max | Rundown torque exceeded maximum level. | Tightening parameters (Edit) > (Step 2) Rundown torque limits > Torque max
Rundown angle above max | Rundown angle exceeded maximum level. | Tightening parameters (Edit) > (Step 2) Rundown angle limits > Angle max
Rundown exceeded max time limit | Rundown time exceeded maximum limit. | Tightening parameters (Edit) > (Step 2) Rundown angle limits > Time max
Rundown below min time limit | Rundown time below minimum limit. | Tightening parameters (Edit) > (Step 2) Rundown angle limits > Time min
Rundown torque below min | Rundown torque below minimum level. | Tightening parameters (Edit) > (Step 2) Rundown torque limits > Torque min
Rundown angle below min | Rundown angle below minimum level. | Tightening parameters (Edit) > (Step 2) Rundown angle limits > Angle min
Final step torque above max | Final step torque exceeded maximum level. | Tightening parameters (Edit) > (Step 3) Final step > Torque limits Manual > Torque max
Final step angle above max | Final step angle exceeded maximum level. | Tightening parameters (Edit) > (Step 3) Final step > Angle max
Final step torque below min | Final step torque below minimum level. | Tightening parameters (Edit) > (Step 3) Final step > Torque limits Manual > Torque min
Final step angle below min | Final step angle below minimum level. | Tightening parameters (Edit) > (Step 3) Final step > Angle max
Tightening timeout | Tightening time limit exceeded. | [Multistep] Tightening parameters (Edit) > Step dependent [Other tightening programs]: fixed parameter set to 30 seconds
Trigger lost | Tool trigger was released before target was reached. | [Multistep]: trigger release before tightening step target has been reached [Other tightening programs]: trigger release before tightening stage has finished
Slip off | Socket has slipped off the nut. | Tightening parameters (Edit) > (Step 3) Tightening parameters > Slipoff detection time
Target reached before final step | Target torque reached before final step in tightening program. | Target torque
Post view torque below min | Post view torque below minimum level. | Tightening parameters (Edit) > (Step 2) Post view torque > Torque min
Post view torque above max | Post view torque exceeded maximum level. | Tightening parameters (Edit) > (Step 2) Post view torque > Torque max
Post view torque interval not reached | Post view torque interval not reached. | Tightening parameters (Edit) > (Step 2) Post view torque > Torque min length
Torque compensation interval not reached | Torque compensation interval angle before rundown end not reached. | Tightening parameters (Edit) > (Step 3) Torque compensation > Torque compensation point
Tool movement exceeded | Tool was moved beyond set angle limits. | Tightening parameters (Edit) > (Step 1) TrueAngle compensation (On); Tool movement limits > Positive/Negative
Current monitoring error | Current monitoring error. | Tightening parameters (Edit) > (Step 1) Current monitoring (On)
Final step exceeded max time limit |  | [TurboTight] Tightening parameters (Edit) > (Step 3) Final step > Time max
Final step below min time limit |  | [TurboTight] Tightening parameters (Edit) > (Step 3) Final step > Time min
TurboTight time limit exceeded | TurboTight time limit exceeded. | [TurboTight] Tightening parameters (Edit) > (Step 3) Final step > Time max
Snug monitor high | Wrench only. Monitor detected snug value exceeded. | Tightening parameters (Edit) > Rundown stage (Step 2) Rundown complete > Rundown complete torque
No residual torque | Wrench only. Residual torque was under threshold. | [TurboTight] + [TensorPulse] Tightening parameters (Edit) > (Step 3) > Tightening parameters > Residual torque correlation factor
Overspeed | Wrench only. Wrench gyro failed to measure angle due to high speed. | N/A