# ST Selector

The ST selector is a tool accessory. It is installed on the tool and connected to the tool accessory bus. It has a small display, two input buttons and output LEDs.

## Display

The display shows one information at a time and has four different pages that can be configured to display different preset items on every page.

Parameter | Description
--- | ---
Page 1 | Select the mesage to be displayed from the list:. Final torque Final angle Batch count Remaining batch Generic IO 1 Generic IO 2 Generic IO 3 Generic IO 4 Generic IO 5 Generic IO 6 Generic IO 7 Generic IO 8 Generic IO 9 Generic IO 10 Selected tightening program Selected batch sequence id Target torque Target/Final torque
Page 2
Page 3
page 4

## Switch time

Parameter | Description
--- | ---
Switch time | Select the time to display one message before the next message is displayed.

## Buttons

The two buttons can be configured to act upon the displayed information and used to step through listed items.

Parameter | Description
--- | ---
Left button | Select one action from the shortcut menu.
Right button | Select one action from the shortcut menu.

## Status LEDs

The status LEDs can be activated or deactivated.

Parameter | Description
--- | ---
Enable result LEDs | Select the desired On or Off radio button.
Enable extra LEDs | Select the desired On or Off radio button.

The result LEDs are red, green and yellow, and show the same information as the main tool LEDs.

The two extra LEDs can show Batch OK and Batch sequence OK. Both these LEDs are turned off at the next tightening.