# STwrench Stop Step Parameters

The parameters shown in the tables are available if one of the STwrench strategies are used. There are several combinations of strategies. Some of the parameters are only available for certain strategies and may not be visible in other strategies.

Parameter rules are automatically checked. If a violation occurs, the error indicator is displayed beside the incorrect parameters. Select the error indicator to display more information about the error.

Switching between strategies can result in the error indicator being shown. This indicates that the chosen combination is invalid, and needs to be corrected.

For more information about the STwrench, see the STwrench User Guide (printed matter number 9836 4134 01).

Parameters in the STwrench loosening step
Parameter name | Condition | Description | Default value
--- | --- | --- | ---
End cycle time |  | It is applied when torque goes below the cycle start and gets to the third percentage value set on the STwrench LEDs. | 100 ms