# Single Controller without Emergency Stop Button

Connector: Phoenix, 6-pin Headers 3.5mm pitch

WARNING

Remote start switch must be set to OFF for this configuration

Use the following PIN configuration:
Pin | Use |
--- | --- | ---
1 | Do not use | Connections with no EM stop
2 | Do not use
3 | Connect a jumper between pin 3 and pin 4
4 | See pin 3
5 | Connect a jumper between pin 5 and pin 6
6 | See pin 5
7 | Connect a jumper between pin 7 and pin 8
8 | See pin 7
9 | Connect a jumper between pin 9 and pin 10
10 | See pin 9