# Configuring Task Window in a Virtual Station

The selected task can either be running a tightening program, running a batch sequence or enabling the task using a source configured in the Sources menu.

The task can be monitored from the controller and the result of the task can be presented together with any events that may have occurred during the operation.

In this Section

- Configuring Manual Mode in a Virtual Station