# Diagnostics Configuration

Diagnostics for a specific accessory or fieldbus is accessible through the Info option in the Virtual Station view for the accessory or fieldbus.

1. Tap Info and on the next screen tap Diagnostics.

2. Activate Monitor mode or Forced mode with the switch.

3. The statuses of input signals and output signals are available under the respective tabs.

It is only possible to access the diagnostics from one single user or function at a time. If the diagnostics is already in use an information message is shown on the screen.