# Entering and Leaving Signals

The parameters for entering and leaving signals are the same.

There are two types of signals: Boolean and integer/string type. For Boolean type signals, an on/off (true/false) switch is used. For integer/string type signals, a text field is used where the (I/O) signal or string can be indicated.

Signal | Type | Default value
--- | --- | ---
Abort sequence | Boolean | Off
Acknowledge events | Boolean | Off
Activate tool scanner | Boolean | Off
Clear results | Boolean | Off
Disable Fieldbus | Boolean | Off
Disable Open Protocol Commands | Boolean | Off
Disable Tool scanner | Boolean | Off
Dynamic batch size | Integer | 0
External identifier | Integer | 0
External monitored [1-8] | Boolean | Off
Flash Tool Green Led (external protocol) | Boolean | Off
Generic IO [1-10] | Integer | 0
Id for dynamic batch size | Integer | 0
Reset batch | Boolean | Off
Reset batch sequence | Boolean | Off
Reset bistable relay | Boolean | Off
Reset Too Many NOK | Boolean | Off
Select input | Integer | 0
Set bistable relay | Boolean | Off
Unlock tool on complete | Boolean | Off
Unlock tool on disable | Boolean | Off