# Configuration of the Buzzer

The buzzer is configured by assigning a sound to a signal selected from a list of available signals.

The sound consists of a set of parameters described in the table. A signal with a sound can be prioritized between 1 and 10 where 1 is highest priority and 10 the lowest. By default a signal and sound has the priority 5. Up to 20 sounds can be assigned to signals.

Parameter | Description
--- | ---
Frequency | Exact frequency in Hz.
Time on | Time (in ms) that the buzzer makes a sound.
Time off | Time (in ms) that the buzzer is quiet.
Repetition | Number of times the buzzer repeats the on/off sequence.
Volume | The buzzer volume, in percentage of max volume.