# Route and install power- and control cables to FlexCarrier

Make sure that the cables are in good condition before connecting them to the system. Check that

- Cables are not damaged

- Connectors are not damaged.

If these conditions are not fulfilled the system must not be connected to mains or switched on.

Systems where damages to connections or cables are found must be disconnected and repaired immediately.

WARNING

It is dangerous to use systems, cables or units that are not in good condition or not connected according to electrical regulations and system requirements, whether manufactured by Atlas Copco or third party.

Procedure

1. Install power cables.

   WARNING

   Use only Atlas Copco tool cables.

   WARNING

   Do not connect or disconnect power cables when the power is on. Always turn off the power to the system with the electrical mains.

   WARNING

   Risk of Injury When Handling Power Cable Latch

   Fingers can be injured.

   - Open and close the latch with care.

2. Install control cables.