# Mounting FlexSystem

For minimal footprint select power cables and mount the FlexSystem according to the specified distances.

The FlexCarrier should be mounted vertically for optimal system functionality. This will allow for best air flow and heat transfer. Mounting FlexCarrier horizontally can affect the lifetime of the system.

The FlexSystem and the main switch box can be mounted in any normal industrial environment without any extra enclosure, if local regulations do not require otherwise.

The FlexSystem should not be exposed to excessive amount of vibrations. The vibration should be less than 10 g (98 m/s2) and between 1000 to 2000 Hz.

Screw: M6, Torque: 9.8 Nm

Distances between FlexSystem parts for minimal footprint (with FlexFan)

Distances between FlexSystem parts for minimal footprint (without FlexFan)

In this Section

- Placement of FlexSystem