# Configuration parameters

Parameter | Atlas Copco FlexSystem
--- | ---
CH1/2: Input Enabled | Disable
CH1/2: Input Channel Mode | Single Channel
CH1/2: Input Type | DIC
CH1/2: Input Reset Type | Manual
CH1/2: Input Test Output Signal | 2400us
CH1/2: Input Debounce Filter Time (400us steps) | 0
CH1/2: Input Consistency Filter Time (400us steps) | 0
CH3/4: Input Enabled | Enable
CH3/4: Input Channel Mode | Single Channel
CH3/4: Input Type | DIC
CH3/4: Input Reset Type | Manual
CH3/4: Input Test Output Signal | 2400us
CH3/4: Input Debounce Filter Time (400us steps) | 125
CH3/4: Input Consistency Filter Time (400us steps) | 625
CH5/6: Input Enabled | Disable
CH5/6: Input Channel Mode | Single Channel
CH5/6: Input Type | DIC
CH5/6: Input Reset Type | Manual
CH5/6: Input Test Output Signal | 2400us
CH5/6: Input Debounce Filter Time (400us steps) | 0
CH5/6: Input Consistency Filter Time (400us steps) | 0
CH1/2: Output Enabled | Enable
CH1/2: Output Channel Mode | Dual Channel
CH1/2: Output Reset Type | Manual
CH1/2: Output Test Offset (extension) | No Offset
iPar CRC | 0x4DC13CF8