# Emergency stop for FlexSystem

The FlexSystem makes it possible to connect emergency stops (e-stops) in different configurations with up to 15 FlexCarriers.

For the e-stop button and reset button there is a protected 24VDC input via the e-stop terminals on the front of the first FlexCarrier in the system.

Test the e-stop function every time the power supply chain is changed, to make sure the e-stop function is still intact.

In this Section

- E-stop rules
- E-stop configuration plug
- E-stop entry plug
- Bypass plug
- ASM plug
- Emergency stop modes
- E-stop source from button connected to first FlexCarrier
- E-stop source safety PLC connected FlexController
- E-stop cable length