# Mount FlexFan

Power must be turned off when mounting a FlexFan.

This step is optional.

For 3 slot FlexCarrier:

1. Remove the fan cover on the FlexCarrier.

2. Plug in the FlexFan cables to the contacts on the FlexCarrier.

3. Fasten the FlexFan with the screws closest to the backside. Use torque 2.2 Nm.

   Screw MRT M4x20 tuflok (or thread-locking adhesive) plus a washer.

4. Fasten the FlexFan with the remaining screws closest to the front. Torque 2.2 Nm.

   Screw MRT M4x70 tuflok (or thread-locking adhesive).

For 6-slot FlexCarrier, repeat for second FlexFan.