# Recommended cables for general positioning

FlexCarriers can be positioned freely, with more spacing or with FlexCarriers not placed in the same plane.

Power cables

The selection is based on the routed length between cable ends from A to B. Select a FlexPower cable with the closest longer length to the measurement.

The minimum bending radius (0.12 m) must be followed.

Length (L) | Name | Article number | Remark
--- | --- | --- | ---
1 m | Power Cable | 4222 1948 01 | DaisyCh Power Cable SE 1m
2 m | Power Cable | 4222 1948 02 | DaisyCh Power Cable SE 2m
3 m | Power Cable | 4222 1948 03 | DaisyCh Power Cable SE 3m
5 m | Power Cable | 4222 1948 05 | DaisyCh Power Cable SE 5m
10 m | Power Cable | 4222 1948 10 | DaisyCh Power Cable SE 10m

Control cables

The selection is based on the routed length between cable ends from A to B. Select a FlexControl cable with the closest longer length to the measurement.

The minimum bending radius (0.1 m) must be followed.

Length (L) | Name | Article number | Remark
--- | --- | --- | ---
1 m | Control Cable | 4222 2062 11 | Flex Daisy Control Cable 1m
2 m | Control Cable | 4222 2062 12 | Flex Daisy Control Cable 2m
3 m | Control Cable | 4222 2062 13 | Flex Daisy Control Cable 3m
5 m | Control Cable | 4222 2062 15 | Flex Daisy Control Cable 5m
10 m | Control Cable | 4222 2062 20 | Flex Daisy Control Cable 10m