# Connecting to web GUI through the service ethernet port

Table Title
A | ToolsTalk server
B | Service ethernet port.

When the ToolsTalk server is connected to the service ethernet port, perform the following steps to connect to the web GUI:

1. Select IP address to the IPC, for example 169.254.1.100

2. Open a web browser on the IPC.

3. In the address field, type 169.254.1.1 .

   The web GUI opens.