# FlexCarrier

The FlexCarrier is available in two versions: 3 slot and 6 slot. The FlexController and the FlexDrives connects into device slots in the FlexCarrier. The FlexCarrier distributes power, interconnection, emergency stop (e-stop) and cooling. It also connects to accessories.

It is possible to connect one FlexCarrier to other FlexCarriers in a daisy chain.

The FlexCarrier module has the following functions:

- AC-power, with fuse and distribution

- DC 24V power generation, monitoring/control

- Emergency stop functions

- Supervision and fan control.

Flexible mounting

It is possible to mount the FlexCarrier on a:

- Station

- Power head frame

- Robot arm

- Manual station post

- Suspended tool stations

- Floor stations.