# Setting up connection to ToolsTalk 2 server

Table Title
A | Factory network
B | ToolsTalk server
C | Factory ethernet port.

To set the IP address for the factory ethernet port and point out the ToolsTalk server, perform the following steps:

1. Open the web GUI.

2. Click on the Settings icon.

3. Open the Network part.

4. Insert the settings for the factory ethernet port, manually or via DHCP.

5. Open the Server connections part.

6. Set the Server port and Server host obtained by ToolsTalk 2.

Relevant Information

- Connecting to web GUI via service ethernet port when ToolsTalk server is connected to factory ethernet port