# Protective earth connection for FlexSystem

The FlexSystem is connected to protective earth through the power cables (the power cable and the tool cable). The power cables must be connected even if they are not powered.

Never connect two FlexCarriers without the power cable. Always use both control cable and power cable.

The FlexSystem is still connected to protective earth if the mains switch board is switched off or a fuse is blown.