# Power cable for FlexSystem

The 400/480 VAC between FlexCarriers in a daisy chain goes through the power cables.

Power cables are designed for cable carriers.

Cable to third party mains switch must be an Atlas Copco open end power cable.

Power cable connection

The power cable is available in the following versions:

- Straight Entry (SE)

- Right Entry (RE)

- Left Entry (LE)

- Open End (OE)

- Straight to Right Entry (SRE)

- Right Entry to Straight (RES)

In this Section

- Power cable for FlexSystem product data
- Power cable, straight entry (SE)
- Power cable, right entry (RE)
- Power cable, left entry (LE)
- Power cable, straight to right entry (SRE)
- Power cable, right entry to straight (RES)
- Power cable, open end (OE)