# Recommended cables for minimum footprint

For information of dimensions for minimal footprint installation, see Mounting FlexSystem.

Power cables

To connect a FlexCarrier to mains switch board, use the power cable:

| Name | Article number
--- | --- | ---
A | DaisyCh Power Cable SE 1m | 4222 1948 01

To connect a FlexCarrier to a 3 slot FlexCarrier, use these power cables:

To connect a FlexCarrier to a 6 slot FlexCarrier, use these power cables:

| Name | Article number
--- | --- | ---
A | DaisyCh Power Cable LE 0.365m | 4222 2082 12
B | DaisyCh Power Cable LE 0.22m | 4222 2082 11
C | DaisyCh Power Cable RES 0.65m | 4222 2084 11
D | DaisyCh Power Cable SRE 0.65m | 4222 2083 11
E | DaisyCh Power Cable RE 0.22m | 4222 1946 11
F | DaisyCh Power Cable RE 0.365m | 4222 1946 12

Control cables

Use these control cables:

System orientation | Name | Article number
--- | --- | ---
Horizontal 3 slot | Daisy Control Cable 0.44m | 4222 2062 01
Horizontal 6 slot | Flex Daisy Control Cable 0.61m | 4222 2062 04
Vertical system | Flex Daisy Control Cable 0.84m | 4222 2062 03