# Test loss of FlexCarrier e-stop plug

1. Trigger a stop condition and verify that:

   - An alarm stating that the FlexSystem is stopped is triggered.

2. Disconnect one or more FlexCarrier’s e-stop plug and verify that:

   - A reset action is not possible, that is, the FlexSystem remains stopped regardless of reset activity.

3. 3. Reconnect the e-stop plug and verify that:

   - The FlexSystem remains stopped until reset is activated.