# Configuring Task Window in a Virtual Station

The Task menu enables users to change task and do test tightening. The test tightening is used for easier fault finding and testing of the system.

Enable test tightening from the web GUI

1. Open Virtual Station menu.

2. In the Task window, select Test Tightening.

3. In the Enable test tightening pane, switch from Off to On.

   Activating test bolt will abort current task.

Test modes

1. Select number of iterations.

2. Click Add to add up to four modes. The modes are configured in ToolsTalk2 > Sync mode.

Test single channels

1. Select number of iterations.

2. Click Add to add up to four channels.

3. Select channel.

4. Set multistep index, The multistep index is shown in the list in ToolsTalk2 > Tightening and Multstep program.

Start test tightening

1. Click Execute to start the test tightening.

Stop test tightening

1. Click Stop to stop the test tightening.