# Installation of upgrade

To update the software perform the following steps:

1. Open the web GUI.

2. Click on the FlexSystem icon.

3. Select Software.

4. In the Software update field click on the Browse button.

5. Locate the new software.

6. Click Continue.

7. Follow the instructions on the screen.

8. When the system have restarted, restart the system again using the mains switch. This is to ensure that all system configurations have been updated. Wait 30 seconds before switching the main switch to ON again.

If the software is upgraded from version 1.2.X and the tightening program has errors in conversion after restart, do the following for all the programs in the Tightening Program list:

1. Double click on the tightening program, the tightening program page shows.

2. In the Properties of the tightening program, add a dot (.) in the Description field at the end of the string (if the field is empty, add a dot anyway).

3. Push the changes.