# Placement of FlexSystem

The FlexCarrier should be mounted vertically for optimal system functionality. This will allow for best air flow and heat transfer.

The FlexSystem and the mains switch box can be mounted in any normal industrial environment without any extra enclosure, if local regulations do not require otherwise.

The FlexSystem should not be exposed to excessive amount of vibrations. The vibration should be less than 10 g (98 m/s2) and between 1000 to 2000 Hz.

In this Section

- Distances between FlexSystem parts
- Placement of fastening holes
- Distance from thermal insulating wall
- Daisy chain