# Relays

Relays Relay out

There are 8 relayoutputs. Normally open or normally closed depending on the connection.

Connector

24-pin detachable screw terminal. Mating connector Phoenix MCVR 1.5/12-ST.3.81 or compatible.

Function

Two way dry contact relays. Isolated outputs. Logical function is set in the configuration of the PowerFocus or DS-drive.

Electrical data

Max 50VDC/AC. Switching load: min 1mA, max 500 mA resistive load.

Pos. No. | Function
--- | ---
1 | Relay 5 normally open
2 | Relay 5 common
3 | Relay 5 normally closed
4 | Relay 6 normally open
5 | Relay 6 common
6 | Relay 6 normally closed
7 | Relay 7 normally open
8 | Relay 7 common
9 | Relay 7 normally closed
10 | Relay 8 normally open
11 | Relay 8 common
12 | Relay 8 normally closed
13 | 24V external output
14 | 24V external output
25 | Relay 5 normally open
26 | Relay 5 common
27 | Relay 5 normally closed
28 | Relay 5 normally open
29 | Relay 5 common
30 | Relay 5 normally closed
31 | Relay 5 normally open
32 | Relay 5 common
33 | Relay 5 normally closed
34 | Relay 5 normally open
35 | Relay 5 common
36 | Relay 5 normally closed
37 | 24V external ground
38 | 24V external ground

Screw terminal

External output