# Install FlexController

1. Insert the FlexIAM.

2. Plug in the FlexController in the first slot on the FlexCarrier.

3. Fasten the FlexController to the FlexCarrier. Wait to tighten it until all modules are fastened to the FlexCarrier.

4. Route the cables to the FlexController.

5. Prepare the gasket for cable routing.

6. Install the cables.

   Make sure that the cable will fit under the cover.

   Max length from connection panel surface to inside of cover (L). | max 45.7 mm
   Max cable bend (R) | 25 mm

7. Route the installed cables down through the cable routing gasket.

   To prevent dust or water to get inside the FlexController make sure it is a tight fit between the cable and gasket.

8. Fasten the cover. Make sure the cover fits tight.