# Connecting to web GUI via service ethernet port when ToolsTalk server is connected to factory ethernet port

Make sure the DHCP settings are enabled on the computer.

When the ToolsTalk server is connected to the factory ethernet port, perform the following steps to connect to the web GUI:

1. Connect to the service ethernet port.

2. Open a web browser.

3. In the address field, type 169.254.1.1 .

   The web GUI opens.