# Specifying area distances for all ILT devices

You can set minimum and maximum distances to specific values for all ILT devices in all areas for the currently active configuration at a time. It is possible to leave either of the distance fields blank in case the corresponding distance is not specified.

ILT devices that are either offline or otherwise unreachable will not receive settings update.

- Go to the Smart AMS Manager address in your web browser by using the Open Smart AMS Manager shortcut on the Desktop or on the Windows Start menu.
  Sample address: http://localhost:6394. Port number is selected when you install Smart AMS. The default is 6394. Make sure to replace localhost with the actual IP address of the computer that Smart AMS Manager is running on.

- To switch to the Configuration section, click in the Navigation Panel on the left of the page. On mobile devices with a smaller screen, click your username in the upper right corner of the page, and then select Configuration.

- Click ILT, and then click the Set area distances on all ILT devices button.

Password field: Enter the password, which is supposed to be the same for all ILT devices in the configuration.

Minimum Distance field: Specify the minimum distance between the tools and their base stations. The unit of measure for distance is specified in ILT.

Maximum Distance field: Specify the maximum distance between the tools and their base stations. The unit of measure for distance is specified in ILT.