# Logging on to Smart AMS Config

- Go to the Smart AMS Config address in your web browser by using the Open Smart AMS Config UI shortcut on the Desktop or on the Windows Start menu.
  Sample address: http://localhost:6395. Make sure to replace localhost with the actual IP address of the computer Smart AMS Config is running on.

A dialog box will appear in the web browser prompting you to enter your username and password.

The first time you use Smart AMS Config, you are prompted to specify administrator login and password. You will then need to enter these login credentials to log on to Smart AMS Config as an administrator.

- Select the desired language from the drop-down list and enter your credentials to log on.

The data you enter in the Username and Password fields must match those provided when installing Smart AMS Config. You can get this information from the person responsible for installing Smart AMS.

After you log on, your username will be displayed in the upper right corner of the page. You can then start using Smart AMS Config.