# Logging on to Smart AMS Manager

- Go to the Smart AMS Manager address in your web browser by using the Open Smart AMS Manager shortcut on the Desktop or on the Windows Start menu.
  Sample address: http://localhost:6394. Port number is selected when you install Smart AMS. The default is 6394. Make sure to replace localhost with the actual IP address of the computer Smart AMS Manager is running on.

A dialog box will appear in the web browser prompting you to select a display language and enter your username and password.

- Select the desired language from the drop-down list and enter your credentials to log on.

The data you enter in the Username and Password fields must match those provided when installing Smart AMS Manager. You can get this information from the person responsible for installing Smart AMS.

After you log on, your username will be displayed in the upper right corner of the page. You can then start using Smart AMS Manager.